{"text_format":"2","workbook":"xls","n_sheets":14,"sheets":["说明","S3100&3100V2 SI","S3100&3100V2 EI","S3600&3600V2 SI","S3600&3600V2 EI&3610&5510","S5100EI","S5600","S5120SI&E500&5120EI&5120HI","S5500SI","S5500EI&5500HI","S5800","5830","Sheet1","5820V2&5830V2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":183,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"说明","index":0,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":false,"merged":[[2,0,21,7]],"flags":["formulas_cached_only"]}
[]
[]
["设备说明：E系列设备为教育网包装，不再单独说明。\nE328=H3C S3600-28TP-SI\nE352=H3C S3600-52P-SI\nE152=H3C S3152p\nE126=H3C S3100-26C-SI\nE126A=H3C S3100-26TP-EI\nE008-FE=S2008EI\nE017-FE=S2016EI\nE026-FE=S2403H-EI\nE026-SI=S3026C-SI\nE026T=S3026T\nE026=S3026C\nE050=S3050C\nH3C S2126-EI=H3C S3100-26TP-SI\n规格说明： \n“-”表示不支持， Y表示有正式版本或者测试版本支持   FUTURE表示将来支持\n其中，L2的设备不宣传路由和SECOND IP的概念，都不支持。\n低端设备不宣传背板带宽，因为盒子设备没有背板，实际数据无法计算，只宣传端口容量。"]

{"sheet":"S3100&3100V2 SI","index":1,"n_rows":302,"n_cols":20,"rows_kept":302,"cut":false,"hidden":false,"merged":[[245,0,279,0],[175,0,178,0],[179,0,180,0],[181,0,187,0],[280,0,285,0],[286,0,301,0],[188,0,189,0],[190,0,203,0],[204,0,217,0],[218,0,232,0],[233,0,244,0],[124,0,144,0],[145,0,147,0],[154,0,164,0],[165,0,170,0],[171,0,172,0],[173,0,174,0],[148,0,152,0],[6,0,35,0],[36,0,88,0],[2,0,5,0],[89,0,110,0],[111,0,115,0],[116,0,123,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S3100V2-8TP-SI","S3100V2-16TP-SI","S3100V2-26TP-SI","H3C S3100-8C-SI\n","H3C S3100-16C-SI\n","H3C S3100-26C-SI\n","H3C S3100-8T-SI\n","H3C S3100-16T-SI\n","H3C S3100-26T-SI\n","H3C S3100-8TP-SI","H3C S3100-16TP-SI","H3C S3100-26TP-SI","H3C S3100-52TP-SI"," H3C S2126-EI","E126","H3C S3100-26TP-SI(UM)","H3C S3100-52TP-SI(UM)"]
[null,"CPL","CPL","A3100-8 v2 SI \nJG221A","A3100-16 v2 SI \nJG222A","A3100-24 v2 SI \nJG223A","-","-","-","-","-","-","A3100-8 SI \nJD305A","A3100-16 SI \nJD306A","A3100-24 SI \nJD307A","-","-","-","-","-"]
["端口\nport","固定配置","Fixed configration","8*10/100TX+1* 1000M(COMB","16*10/100TX+2* 1000M(COMB","24*10/100TX+2* 1000M(COMB","8 *10/100TX","16 *10/100TX","24 *10/100TX","8*10/100TX+1*GE","16*10/100TX+1*GE","24*10/100TX+2*GE","8*10/100TX+1* 1000M(COMB)","16*10/100TX+2 *1000M(COMB)","24*10/100TX+2* 1000M(COMB)","48*10/100 BASE-T + 2*1000M SFP+2*1000BASE-T","24*10/100TX+2* 100M(COMB)","24 *10/100TX","24*10/100TX+2* 1000M(COMB)","48*10/100 BASE-T + 2*1000M SFP+2*1000BASE-T"]
[null,"配置口","config interface","console","console","console","console ","console ","console","console ","console ","console","console ","console ","console","console ","console ","console","console","console"]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","1*(10/100/1000BASE-T[100m] /  100BASE-SX[2km] / 100BASE-LX15km] / 100BASE-LH40[40km] / 1000BASE-SX[0.5km] / 1000BASE-LX[10km] /  1000BASE-LH40[40km] / 100BASE-TX PD interface model/Epon/BIDI)","2*(10/100/1000BASE-T[100m] /  100BASE-SX[2km] / 100BASE-LX15km] / 100BASE-LH40[40km] / 1000BASE-SX[0.5km] / 1000BASE-LX[10km] /  1000BASE-LH40[40km] / 100BASE-TX PD interface model /  1000BASE-STACK/Epon/BIDI)","2*(10/100/1000BASE-T[100m] /  100BASE-SX[2km] / 100BASE-LX15km] / 100BASE-LH40[40km] / 1000BASE-SX[0.5km] / 1000BASE-LX[10km] /  1000BASE-LH40[40km] /Epon/BIDI)","-","-","-","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2*100MSFP(2km,15km)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)"]
[null,"100FX SFP支持","100FX SFP support","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","3.6G","7.2G","8.8G","3.6G","7.2G","8.8G","3.6G","5.2G","8.8G","3.6G","7.2G","8.8G","17.6G","5.2G","8.8G","8.8G","17.6G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","2.68M","5.36M","6.55M","2.68M","5.36M","6.55M","2.68M","3.87M","6.55M","2.68M","5.36M","6.55M","13.1M","3.87M","6.55M","6.55M","13.1M"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5",null,null,"FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5"]
[null,"三层路由转发机制","L3 route forwarding mode","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"静态MAC个数","Static mac table","1k","1k","1k","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","8k","8k","8k","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K"]
[null,"路由接口数","Max VLAN interface",1,1,1,"-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IP V4路由条数","IP V4 routing num",16,16,16,"-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"整机支持L2组播数","Multicast L2  entries",512,512,512,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
[null,"整机支持L3组播数","Multicast L3  entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"跨VLAN组播复制能力","Multicast entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VLAN数","Vlan table","4k","4k","4k","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
[null,"ACL流分类数","ACL Num","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",512,512]
[null,"ACL机制说明","ACL policy description","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","global acl","global acl"]
[null,"ACL 方向","ACL direction","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","ingress","ingress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",512,512]
[null,"VACL","ACL BASED VLAN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）"]
[null,"流量整形","traffic shaping","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"Flash大小","Flash","16M","16M","16M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M"]
[null,"SDRAM大小","SDRAM","128M","128M","128M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","384KBytes","384KBytes","384KBytes","256KBytes","256KBytes","256KBytes","256KBytes","256KBytes","256KBytes","256KBytes","256KBytes","256KBytes","512KBytes","256KBytes","256KBytes","384KBytes","512KBytes"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,2048,1536,1536,2048,2048]
[null,"Jumbo frame Support","Jumbo frame Support","2k","2k","2k","-","-","-","-","-","-","-","-","-",2048,"-","-",2048,2048]
[null,"堆叠方式","Stack mode","IRF-Lite","IRF-Lite","IRF-Lite","-","HGMP V2 STACK","HGMP V2 STACK","-","-","HGMP V2 STACK","-","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","-","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK"]
[null,"堆叠带宽","Stack bandwidth","2G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","-","4G(Bidirection and loop network)","4G(Bidirection and loop network)","-","-","4G(Bidirection and loop network)","-","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","-","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)"]
[null,"堆叠台数","MAX Stack num",16,16,16,"-",16,16,"-","-",16,"-",16,16,16,"-",16,16,16]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num",16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16]
[null,"动态ARP数目","Dynamic ARP num",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"PVST+","PVST+","Y(16)","Y(16)","Y(16)","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"TC snooping","TC snooping","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"Smart Link","Smart Link","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"Smart Link multi-instances","Smart Link multi-instances","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VLAN MAPPING ","VLAN MAPPING ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM snooping","PIM snooping","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"组播VLAN","MVR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN+","MVR+","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP multi-instances","RRPP multi-instances","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"EAD","support users by 5 rules","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,"support users by 10 rules","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,"support users by 20 rules","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",128,128]
[null,"IP+PORT绑定个数","IP+PORT Binding","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",128,128]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",128,128]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",128,128]
[null,"可聚合端口数目","MAX num in one link group",8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,"端口聚合组数","Link group num",4,9,13,2,3,3,2,2,3,2,2,3,6,3,3,6,6]
[null,"restore port default config","restore port default config","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"单链路检测","DLDP","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1"]
[null,"流镜像","Traffic Mirroring","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","N:1","N:1"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","flow constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y","Y","Y","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y(1% bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"IPSource Guard","IPSource Guard","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"基于协议类型VLAN","Protocal based vlan","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Voice Vlan","Voice Vlan","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"SuperVLAN","SuperVLAN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RIPV1/2","RIPV1/2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V2","OSPF V2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS","IS-IS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","N","N","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"静态路由","Static routing","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"支持second ip数目","MAX num of second ip ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP Relay","DHCP Relay","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"VRRP","VRRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRPE","VRRPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BFD","BFD","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Routed ports","Routed ports","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ECMP(等值路由)","ECMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"策略路由","Policy based routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-"]
["MPLS","MPLS label number","MPLS label number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS label depth","MPLS label depth","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS interface number","MPLS interface number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"static LSP number","static LSP number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"等价LSP","等价LSP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP local peer number","LDP local peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP remote peer number","LDP remote peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls TE","mpls TE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp ping","mpls lsp ping","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VPN number","VPN number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"CE number per VPN","CE number per VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L3VPN","VRF number","VRF number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"interface number per VRF","interface number per VRF","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["VPLS","VSI number","VSI number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPFIX","IPFIX","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3","IGMP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SM","PIM-SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SSM","PIM-SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-DM","PIM-DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"双向PIM","BI-PIM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MSDP","MSDP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["OAM","802.1AG","802.1AG","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3AH","802.3AH","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y","Y","Y","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ISSU","ISSU","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"端口自动节能","port auto power down","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"triple authentication","triple authentication","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total",1024,1024,1024,"1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"PORTAL认证用户数","portal  USERS",512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512]
["QOS","SP","Strict priority","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WRR","WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WRR","SP+WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SDWRR","SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WDRR","WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ACL logging","ACL logging","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num",16,16,16,"-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 ND数目","IPV6 ND NUM",1024,1024,1024,"-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND proxy","ND proxy","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND detection","ND detection","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SAVI","SAVI","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","Y","-","-"]
[null,"PMTU","PMTU","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","RIPng","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V3","OSPF V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS V6","IS-IS V6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 relay","DHCP V6 relay","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 server","DHCP V6 server","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 端口绑定","IPv6 source guard","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BFD v6","BFD v6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"6VPE","6VPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"是否支持中功率POE","POE(30W PER PORT)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"总功率","Total Power","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"单端口最大功率","Power Per Port","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3af","802.3af","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["物理特性\nphysical feature","电源","Power Supply","AC","AC","AC","AC/DC","AC/DC","AC/DC","AC","AC","AC","AC","AC","AC","AC","AC","AC/DC","AC","AC"]
[null,"功耗(W)","Power Consummtion(w)",9,12,13,10,12,20,10,12,20,10,14,16,24,16,20,17,24]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",30.709282050000002,40.9457094,44.35785185,34.1214245,40.9457094,68.242849,34.1214245,40.9457094,68.242849,34.1214245,47.7699943,54.5942792,81.8914188,54.5942792,68.242849,58.00642165,81.8914188]
[null,"湿度","Humidity","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%"]
[null,"温度","Temperature","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","< 3.0kg","< 3.0kg","< 3.0kg","<2kg","≤3kg","≤3kg","<2kg","≤3kg","≤3kg","<2kg","≤3kg","≤3kg","≤3kg","≤3kg","≤3kg","≤3kg","≤3kg"]
[null,"风扇","Fan NUM",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise(low speed/high speed)","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise"]
[null,"MTBF(年)","MTBF","54.2(AC)","50.1(AC)","49.1(AC)","52.14/58.65(AC/DC)","45.00/49.77(AC/DC)","38.19/41.24(AC/DC)",71.66,61.9,46.18,65,59.2,45.37,39.5,38.19,"38.19/41.24(AC/DC)",49.1,39.5]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[null,"RPS电源","RPS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"热插拔","Hot-Swap","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","Y( ony for DC by 100BASE-TX PD interface model)","Y( ony for DC by 100BASE-TX PD interface model)","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","230（W）*160（D）*43.6(H)","360（W）*160（D）*43.6(H)","440（W）*160（D）*43.6(H)","326×42×200","436×42×200","436×42×240","326×42×200","436×42×200","436×42×240","230×160×43.6","360×160×43.6","440×160×43.6","440×230×43.6","440×160×43.6","436×42×240","440×160×43.6","440×230×43.6"]

{"sheet":"S3100&3100V2 EI","index":2,"n_rows":306,"n_cols":23,"rows_kept":306,"cut":false,"hidden":false,"merged":[[245,0,279,0],[175,0,178,0],[179,0,180,0],[181,0,187,0],[280,0,285,0],[286,0,305,0],[188,0,189,0],[190,0,203,0],[204,0,217,0],[218,0,232,0],[233,0,244,0],[124,0,144,0],[145,0,147,0],[154,0,164,0],[165,0,170,0],[171,0,172,0],[173,0,174,0],[148,0,152,0],[2,0,5,0],[6,0,35,0],[36,0,88,0],[89,0,110,0],[111,0,115,0],[116,0,123,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S3100V2-8TP-EI","S3100V2-16TP-EI","S3100V2-26TP-EI","S3100V2-8TP-PWR-EI","S3100V2-16TP-PWR-EI","S3100V2-26TP-PWR-EI","E126B","H3C S3100-8TP-EI","H3C S3100-16TP-EI","H3C S3100-26TP-EI","H3C S3100-8TP-PWR-EI","H3C S3100-16TP-PWR-EI","H3C S3100-26TP-PWR-EI ","E126A","H3C S3100-8TP-EI-W(only for japan)","H3C S3100-16TP-EI-W(only for japan)","H3C S3100-26TP-EI-W(only for japan)","H3C S3100-8C-EPON-EI","H3C S3100-16C-EPON-EI","S3100-26C-EPON-EI"]
[null,"CPL","CPL","A3100-8 v2 EI \nJD318B","A3100-16 v2 EI \nJD319B","A3100-24 v2 EI \nJD320B","A3100-8-PoE v2 EI \nJD311B","A3100-16-PoE v2 EI \nJD312B","A3100-24-PoE v2 EI \n JD313B","-","A3100-8 EI \nJD318A","A3100-16EI \nJD319A","A3100-24 EI \nJD320A","HP A3100-8-PoE EI\nJD311A","HP A3100-16-PoE EI\nJD312A","HP A3100-24-PoE EI\nJD313A","-","-","-","-","-","-","-"]
["端口\nport","固定配置","Fixed configration","8*10/100TX+1* 1000M(COMB","16*10/100TX+2* 1000M(COMB","24*10/100TX+2* 1000M(COMB","8*10/100TX+1* 1000M(COMB","16*10/100TX+2* 1000M(COMB","24*10/100TX+2* 1000M(COMB","24*10/100TX+2* 1000M(COMB","8 *10/100TX+1*10/100/1000TX(COMB)","16 *10/100TX+2*10/100/1000TX(COMB)","24 *10/100TX+2*10/100/1000TX(COMB)","8*10/100TX+1*10/100/1000TX(COMB)","16 *10/100TX+2*10/100/1000TX(COMB)","24 *10/100TX+2*10/100/1000TX(COMB)","24 *10/100TX+2*1000M(COMB)","8 *10/100TX+1*10/100/1000TX(COMB)","16 *10/100TX+2*10/100/1000TX(COMB)","24 *10/100TX+2*10/100/1000TX(COMB)","8 *10/100TX+1*ONU","16 *10/100TX+1*ONU","24 *10/100TX+1*ONU"]
[null,"配置口","config interface","console","console","console","console","console","console","console","console ","console ","console","console ","console ","console","console ","console ","console","console ","console ","console","console "]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","1* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","1* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","1* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","-","-","-"]
[null,"100FX SFP支持","100FX SFP support","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","3.6G","7.2G","8.8G","3.6G","7.2G","8.8G","8.8G","3.6G","7.2G","8.8G","3.6G","7.2G","8.8G","8.8G","3.6G","7.2G","8.8G","3.6G","7.2G","8.8G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","2.68M","5.36M","6.55M","2.68M","5.36M","6.55M","6.55M","2.68M","5.36M","6.55M","2.68M","5.36M","6.55M","6.55M","2.68M","5.36M","6.55M","2.68M","5.36M","6.55M"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5"]
[null,"三层路由转发机制","L3 route forwarding mode","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"静态MAC个数","Static mac table","1k","1k","1k","1k","1k","1k","1k","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","8k","8k","8k","8k","8k","8k","8k","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K"]
[null,"路由接口数","Max VLAN interface",1,1,1,1,1,1,1,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IP V4路由条数","IP V4 routing num",16,16,16,16,16,16,16,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"整机支持L2组播数","Multicast L2  entries",512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512]
[null,"整机支持L3组播数","Multicast L3  entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"跨VLAN组播复制能力","Multicast entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VLAN数","Vlan table","4k","4k","4k","4k","4k","4k","4k","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4,4]
[null,"ACL流分类数","ACL Num",256,512,1000,256,512,1000,1000,256,512,1000,256,512,1000,1000,256,512,1000,256,512,1000]
[null,"ACL机制说明","ACL policy description","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl"]
[null,"ACL 方向","ACL direction","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress","ingress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM",256,512,1000,256,512,1000,1000,256,512,1000,256,512,1000,1000,256,512,1000,256,512,1000]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）"]
[null,"流量整形","traffic shaping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）"]
[null,"Flash大小","Flash","16M","16M","16M","16M","16M","16M","16M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M","8M"]
[null,"SDRAM大小","SDRAM","128M","128M","128M","128M","128M","128M","128M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k","2k"]
[null,"堆叠方式","Stack mode","IRF-Lite","IRF-Lite","IRF-Lite","IRF-Lite","IRF-Lite","IRF-Lite","IRF-Lite","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK"]
[null,"堆叠带宽","Stack bandwidth","2G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection )","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection )","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection )","4G(Bidirection and loop network)","4G(Bidirection and loop network)"]
[null,"堆叠台数","MAX Stack num",16,16,16,16,16,16,16,2,16,16,16,16,16,16,2,16,16,2,16,16]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num",16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16,16]
[null,"动态ARP数目","Dynamic ARP num",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"PVST+","PVST+","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"TC snooping","TC snooping","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link","Smart Link","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link multi-instances","Smart Link multi-instances",24,24,24,24,24,24,24,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM snooping","PIM snooping","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"组播VLAN","MVR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN+","MVR+","-","-","-","-","-","-","-",null,null,"Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP multi-instances","RRPP multi-instances","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"EAD","support users by 5 rules","Y","Y","Y","Y","Y","Y","Y","all:48\nper port max:48","all:96\nper port max:96","all:192\nper port max:192","all:48\nper port max:48","all:96\nper port max:96","all:192\nper port max:192","all:192\nper port max:192","all:48\nper port max:48","all:96\nper port max:96","all:192\nper port max:192","all:48\nper port max:48","all:96\nper port max:96","all:192\nper port max:192"]
[null,null,"support users by 10 rules","Y","Y","Y","Y","Y","Y","Y","all:24\nper port max:24","all:48\nper port max:48","all:96\nper port max:96","all:24\nper port max:24","all:48\nper port max:48","all:96\nper port max:96","all:96\nper port max:96","all:24\nper port max:24","all:48\nper port max:48","all:96\nper port max:96","all:24\nper port max:24","all:48\nper port max:48","all:96\nper port max:96"]
[null,null,"support users by 20 rules","Y","Y","Y","Y","Y","Y","Y","all:12\nper port max:12","all:24\nper port max:24","all:48\nper port max:48","all:12\nper port max:12","all:24\nper port max:24","all:48\nper port max:48","all:48\nper port max:48","all:12\nper port max:12","all:24\nper port max:24","all:48\nper port max:48","all:12\nper port max:12","all:24\nper port max:24","all:48\nper port max:48"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","Y","Y","Y","Y","Y","Y","Y","20s","20s","20s","20s","20s","20s","20s","20s","20s","20s","20s","20s","20s"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","Y","Y","Y","Y","Y","Y","Y","40s","60s","80s","40s","60s","80s","80s","40s","60s","80s","40s","60s","80s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","Y","Y","Y","Y","Y","Y","Y","30s","40s","40s","30s","40s","40s","40s","30s","40s","40s","30s","40s","40s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","Y","Y","Y","Y",null,null,"-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding",128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128]
[null,"IP+PORT绑定个数","IP+PORT Binding",128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128]
[null,"MAC+PORT绑定个数","MAC+PORT Binding",128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding",128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128,128]
[null,"可聚合端口数目","MAX num in one link group",8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,"端口聚合组数","Link group num",4,9,13,4,9,13,13,4,9,13,4,9,13,13,4,9,13,4,9,13]
[null,"restore port default config","restore port default config","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","flow constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y","Y","Y","Y","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y","Y","Y","Y","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)","Y(bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y","Y","Y","Y","Y","Y","Y","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1% bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"基于协议类型VLAN","Protocal based vlan","Y","Y","Y","Y","Y","Y","Y","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y( all: 16)"]
[null,"Voice Vlan","Voice Vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SuperVLAN","SuperVLAN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RIPV1/2","RIPV1/2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V2","OSPF V2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS","IS-IS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"静态路由","Static routing","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"支持second ip数目","MAX num of second ip ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP Relay","DHCP Relay","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP","VRRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRPE","VRRPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BFD","BFD","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Routed ports","Routed ports","-","-","-","-","-","-","-"]
[null,"ECMP(等值路由)","ECMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"策略路由","Policy based routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS","MPLS label number","MPLS label number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS label depth","MPLS label depth","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS interface number","MPLS interface number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"static LSP number","static LSP number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"等价LSP","等价LSP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP local peer number","LDP local peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP remote peer number","LDP remote peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls TE","mpls TE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp ping","mpls lsp ping","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VPN number","VPN number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"CE number per VPN","CE number per VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L3VPN","VRF number","VRF number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"interface number per VRF","interface number per VRF","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["VPLS","VSI number","VSI number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPFIX","IPFIX","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3","IGMP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SM","PIM-SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SSM","PIM-SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-DM","PIM-DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"双向PIM","BI-PIM","-","-","-","-","-","-","-",null,null,"-","-","-","-","-","-","-","-","-","-","-"]
[null,"MSDP","MSDP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["OAM","802.1AG","802.1AG","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3AH","802.3AH","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y","Y","Y","Y","Y","Y","Y","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ISSU","ISSU","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"端口自动节能","port auto power down","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"triple authentication","triple authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","Y","Y","Y","Y",null,null,"-","-","-","-","-","-","-","-","-","-","-"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total",1024,1024,1024,1024,1024,1024,1024,"1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"PORTAL认证用户数","portal  USERS",512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512,512]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WRR","SP+WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SDWRR","SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WDRR","WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ACL logging","ACL logging","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num",16,16,16,16,16,16,16,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM",256,512,1000,256,512,1000,1000,256,512,1000,256,512,1000,1000,256,512,1000,256,512,1000]
[null,"IPV6 ND数目","IPV6 ND NUM",1024,1024,1024,1024,1024,1024,1024,"-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND proxy","ND proxy","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SAVI","SAVI","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PMTU","PMTU","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","RIPng","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V3","OSPF V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS V6","IS-IS V6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 relay","DHCP V6 relay","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 server","DHCP V6 server","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD v6","BFD v6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"6VPE","6VPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","-","Y","Y","Y","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-"]
[null,"是否支持中功率POE","POE(30W PER PORT)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"总功率","Total Power","-","-","-","125W","250W","370W","-","-","-","-","AC:\nALL:95W POE:65W\n","AC:\nALL:160W POE:125W","AC:\nALL:465W POE:370W\nDC:\nALL:400W POE:370W","-","-","-","-","-","-","-"]
[null,"单端口最大功率","Power Per Port","-","-","-","15.4W","15.4W","15.4W","-","-","-","-","15.4W","15.4W","15.4W","-","-","-","-","-","-","-"]
[null,"802.3af","802.3af","-","-","-","Y","Y","Y","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-","-","Data wire mode","Data wire mode","Data wire mode","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","-","-","-","-","-","-","-"]
["物理特性\nphysical feature","电源","Power Supply","AC","AC","AC","AC","AC/DC","AC/DC","AC","AC/DC","AC/DC","AC/DC","AC","AC","AC&DC(RPS)","AC","AC","AC","AC","AC","AC","AC"]
[null,"功耗(W)","Power Consummtion(w)",9,12,13,155,"AC:300\nDC:273","AC:465\nDC:400",13,12,15,17,"AC:\nALL:95W POE:65W\n","AC:\nALL:160W POE:125W","AC:\nALL:465W POE:370W\nDC:\nALL:400W POE:370W",17,14,17,22,11,13,20]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",30.70928205,40.9457094,44.35785185,532.2942222,"AC:1023.642735\nDC:931.51488885","AC:1586.64623925\nDC:1364.85698",44.35785185,40.9457094,51.182136750000005,58.00642165,324.15353275,545.942792,"AC:\n1586.64623925\nDC:\n1364.85698",58.00642165,47.7699943,58.00642165,75.0671339,37.53356695,44.35785185,68.242849]
[null,"电源模块","Power Supply module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"电源功率","power rating\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"电源负载均衡","power load-sharing\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PDU电缆","PDU cable\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"湿度","Humidity","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%"]
[null,"温度","Temperature","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","< 3.0kg","< 3.0kg","< 3.0kg","< 3.0kg","< 6.5kg","< 6.5kg","< 3.0kg","<2kg","≤3kg","≤3kg","<2kg","≤3kg","≤3kg","≤3kg","<2kg","≤3kg","≤3kg","<2kg","≤3kg","≤3kg"]
[null,"风扇","Fan NUM",0,0,0,2,3,4,0,0,0,0,2,2,4,0,0,0,0,0,0,1]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise(low speed/high speed)","No fan,no noise","No fan,no noise","No fan,no noise","37.6(low speed)\n44.7(high speed)","40.2(low speed)49.4(high speed)","42.2(low speed)51.5(high speed)","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","37.6(low speed)\n44.7(high speed)","40.2(low speed)49.4(high speed)","42.2(low speed)51.5(high speed)","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","-"]
[null,"MTBF(年)","MTBF","54.2(AC)","50.1(AC)","49.1(AC)","52.8(AC)","45.7(AC)","40.7(AC)","49.1(AC)","54.2/60.5(AC/DC)","50.1/55.4(AC/DC)","49.1/54.3(AC/DC)",52.8,45.7,40.7,"49.1/54.3(AC/DC)",72.7,70.2,65.9,52.14,45,38.19]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[null,"RPS电源","RPS","-","-","-","-","RPS1000-A3","RPS1000-A3","-","-","-","-","-","-","RPS1000-A3","-","-","-","-","-","-","-"]
[null,"热插拔","Hot-Swap","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","230（W）*160（D）*43.6(H)","360（W）*160（D）*43.6(H)","440（W）*160（D）*43.6(H)","300（W）*220（D）*43.6(H)","440（W）*420（D）*43.6(H)","440（W）*420（D）*43.6(H)","440（W）*160（D）*43.6(H)","230×160×43.6","360×160×43.6","440×160×43.6","300×220×43.6","300×260×43.6","440×420×43.6","440×160×43.6","230×200×43.6","300×220×43.6","440×260×43.6","326×200×42","436×200×42","436×240×42"]

{"sheet":"S3600&3600V2 SI","index":3,"n_rows":312,"n_cols":13,"rows_kept":312,"cut":false,"hidden":false,"merged":[[280,0,285,0],[286,0,311,0],[188,0,189,0],[190,0,203,0],[204,0,217,0],[218,0,232,0],[233,0,244,0],[245,0,279,0],[165,0,170,0],[171,0,172,0],[173,0,174,0],[175,0,178,0],[179,0,180,0],[181,0,187,0],[2,0,5,0],[145,0,147,0],[154,0,164,0],[6,0,35,0],[36,0,88,0],[89,0,110,0],[111,0,115,0],[116,0,123,0],[124,0,144,0],[148,0,152,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S3600V2-28TP-SI\n(E328B)","S3600V2-52TP-SI\n(E352B)","S3600V2-28TP-PWR-SI\n","S3600V2-52TP-PWR-SI\n","S3100V2-52TP\n","H3C S3600-28P-SI\n","H3C S3600-28TP-SI\n","H3C S3600-52P-SI\n","H3C S3600-28P-PWR-SI\n","H3C S3600-52P-PWR-SI\n"]
[null,"CPL","CPL","A3600-24 v2 SI\nJG304A","A3600-48 v2 SI\nJG305A","A3600-24-PoE+ v2 SI\nJG306A","A3600-48-PoE+ v2 SI\nJG307A","A3100-48 v2 \nJG315A","A3600-24 SI\nJD330A","A3600-24TP SI\nJD329A"," A3600-48 SI \nJD332A","A3600-24-PoE SI\nJD325A"," A3600-48-PoE SI \nJD327A"]
["端口\nport","固定配置","Fixed configration","24 *10/100TX+2 1000TX（combo）+4*1000SFP","48 *10/100TX+2 1000TX（combo）+4*1000SFP","24 *10/100TX（PoE+）+2 1000TX（combo）+4*1000SFP","48 *10/100TX（PoE+）+2 1000TX（combo）+4*1000SFP","48 *10/100TX+2 1000TX（combo）+4*1000SFP","24 * 10/100TX","24 * 10/100TX+2*10/100/1000TX","48 * 10/100TX","24 * 10/100TX","48 * 10/100TX"]
[null,"配置口","config interface","console","console","console","console","console","console ","console ","console","console ","console "]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","-","-","-","-","-","4* 1000MSFP(550m,10km,40km,70km,RJ45)","2* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)"]
[null,"100FX SFP支持","100FX SFP support","-","-","-","-","-","-","-","-","-","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","12.8Gbps","17.6Gbps","12.8Gbps","17.6Gbps","17.6Gbps","12.8G","12.8G","17.6G","12.8G","17.6G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","9.53M","13.1M","9.53M","13.1M","13.1M","9.53M","9.53M","11.78M","9.53M","11.78M"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K"]
[null,"路由接口数","Max VLAN interface","1K","1K","1K","1K",8,64,64,64,64,64]
[null,"IP V4路由条数","IP V4 routing num","up to 2K","up to 2K","up to 2K","up to 2K",32,"up to 1088","up to 1088","up to 1088","up to 1088","up to 1088"]
[null,"整机支持L2组播数","Multicast L2  entries","IPv4：up to 1K\nIPv6：up to 512","IPv4：up to 1K\nIPv6：up to 512","IPv4：up to 1K\nIPv6：up to 512","IPv4：up to 1K\nIPv6：up to 512","IPv4：up to 1K\nIPv6：up to 512",255,255,255,255,255]
[null,"整机支持L3组播数","Multicast L3  entries","-","-","-","-","-","-","-","-","-","-"]
[null,"跨VLAN组播复制能力","Multicast entries","-","-","-","-","-","-","-","-","-","-"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","Y","Y","Y","Y","Y","NO","NO","NO","NO","NO"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8,8,8,8,8,8,8,8,8]
[null,"ACL流分类数","ACL Num","Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Ingress:1k*2\nEgress:512*2","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM","TCAM","TCAM","TCAM","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask."]
[null,"ACL 方向","ACL direction","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Ingress:1k*2\nEgress:512*2","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100"]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"端口限速粒度","port line-rate granularity","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)"]
[null,"流量整形","traffic shaping","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps"]
[null,"Flash大小","Flash","128M （NAND）","128M （NAND）","128M （NAND）","128M （NAND）","128M （NAND）","8M","8M","8M","8M","8M"]
[null,"SDRAM大小","SDRAM","256M","256M","256M","256M","256M","64M","64M","64M","64M","64M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","2M","4M","2M","4M","4M","32M","32M","32M","32M","32M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support",10000,10000,10000,10000,10000,"9k","9k","9k","9k","9k"]
[null,"堆叠方式","Stack mode","IRF2","IRF2","IRF2","IRF2","IRF2 and IRF lite","IRF(only DDM DLA)","IRF(only DDM DLA)","IRF(only DDM DLA)","IRF(only DDM DLA)","IRF(only DDM DLA)"]
[null,"堆叠带宽","Stack bandwidth","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)"]
[null,"堆叠台数","MAX Stack num",9,9,9,9,"9（IRF）/16（IRF-Lite）",8,8,8,8,8]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K","1K","1K",256,"1K","1K","1K","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up to 2K","up to 2K","up to 2K","up to 2K","up to 256","2K","2K","2K","2K","2K"]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"PVST+","PVST+","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","-","-","-","-","-"]
[null,"TC snooping","TC snooping","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link","Smart Link","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y","Y","Y","Y","Y"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","-","-","-","-","-"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM SNOOPING","PIM SNOOPING","-","-","-","-","-","-","-","-","-","-"]
[null,"组播VLAN","MVR","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y"]
[null,"组播VLAN+","MVR+","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"RRPP multi-instances","RRPP multi-instances","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","-","-","-","-","-"]
[null,"EAD","support users by 5 rules","per port :102\nall:102","per port :102\nall:204","per port :102\nall:102","per port :102\nall:204","per port :102\nall:204","all:96\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32"]
[null,null,"support users by 10 rules","per port :51\nall:51","per port :51\nall:102","per port :51\nall:51","per port :51\nall:102","per port :51\nall:102","all:48\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16"]
[null,null,"support users by 20 rules","per port :25\nall:25","per port :25\nall:50","per port :25\nall:25","per port :25\nall:50","per port :25\nall:50","all:24\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","单芯片：4S","双芯片：4S","单芯片：4S","双芯片：4S","双芯片：4S","17s","17s","17s","17s","17s"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","单芯片：9S","双芯片：10S","单芯片：9S","双芯片：10S","双芯片：10S","58s","58s","100s","58s","100s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","单芯片：9S","双芯片：10S","单芯片：9S","双芯片：10S","双芯片：10S","28s","28s","42s","28s","42s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-","-","-","-","Y","Y","Y","Y","Y"]
[null,"IP+PORT绑定个数","IP+PORT Binding","all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","all 256，per port 256","Y","Y","Y","Y","Y"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","all 256，per port 256","Y","Y","Y","Y","Y"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","all 256，per port 256","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800"]
[null,"可聚合端口数目","MAX num in one link group","8FE/8GE","8FE/8GE","8FE/8GE","8FE/8GE","8FE/8GE",8,8,8,8,8]
[null,"端口聚合组数","Link group num","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )"]
[null,"restore port default config","restore port default config","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:4","N:4","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:4","N:4","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","N","N","N","N","N"]
[null,"storm constrain","flow constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","-","-","-","-","-"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","-","-","-","-","-"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)"]
[null,"Voice Vlan","Voice Vlan","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y","Y","Y","Y","Y"]
[null,"SuperVLAN","SuperVLAN","Y","Y","Y","Y","-","-","-","-","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","Y","Y","Y","Y","Y","-","-","-","-","-"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"RIPV1/2","RIPV1/2","Y","Y","Y","Y","-","Y","Y","Y","Y","Y"]
[null,"OSPF V2","OSPF V2","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS","IS-IS","-","-","-","-","-","-","-","-","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","-","-","-","-","-","-","-","-","-","-"]
[null,"静态路由","Static routing","Y(2k)","Y(2k)","Y(2k)","Y(2k)",32,64,64,64,64,64]
[null,"支持second ip数目","MAX num of second ip ",48,48,48,48,4,4,4,4,4,4]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"VRRP","VRRP","Y(255)","Y(255)","Y(255)","Y(255)","-","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)"]
[null,"VRRPE","VRRPE","Y","Y","Y","Y","-","-","-","-","-","-"]
[null,"BFD","BFD","Y(VRRP/STATIC ROUTING)","Y(VRRP/STATIC ROUTING)","Y(VRRP/STATIC ROUTING)","Y(VRRP/STATIC ROUTING)","Y(STATIC ROUTING)","-","-","-","-","-"]
[null,"Routed ports","Routed ports","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"ECMP(等值路由)","ECMP","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","-"]
[null,"策略路由","Policy based routing","Y","Y","Y","Y","-","-","-","-","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","Y(63 instances)","Y(63 instances)","Y(63 instances)","Y(63 instances)","-","-","-","-","-","-"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","Y","Y","Y","Y","-","-","-","-","-","-"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","Y","Y","Y","Y","-","-","-","-","-","-"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-","-","-"]
["MPLS","MPLS label number","MPLS label number","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS label depth","MPLS label depth","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS interface number","MPLS interface number","-","-","-","-","-","-","-","-","-","-"]
[null,"static LSP number","static LSP number","-","-","-","-","-","-","-","-","-","-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-","-","-","-","-","-","-","-","-"]
[null,"等价LSP","等价LSP","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP local peer number","LDP local peer number","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP remote peer number","LDP remote peer number","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls TE","mpls TE","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp ping","mpls lsp ping","-","-","-","-","-","-","-","-","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-","-","-","-","-","-","-","-","-"]
[null,"VPN number","VPN number","-","-","-","-","-","-","-","-","-","-"]
[null,"CE number per VPN","CE number per VPN","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-","-","-","-","-","-","-","-","-"]
["MPLS L3VPN","VRF number","VRF number","-","-","-","-","-","-","-","-","-","-"]
[null,"interface number per VRF","interface number per VRF","-","-","-","-","-","-","-","-","-","-"]
["VPLS","VSI number","VSI number","-","-","-","-","-","-","-","-","-","-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-","-","-","-","-","-","-","-","-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-","-","-","-","-","-","-","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-","-","-","-","-","-","-","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-","-","-","-","-","-","-","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-","-","-","-","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"IPFIX","IPFIX","-","-","-","-","-","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3","IGMP V3","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SM","PIM-SM","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SSM","PIM-SSM","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-DM","PIM-DM","-","-","-","-","-","-","-","-","-","-"]
[null,"双向PIM","BI-PIM","-","-","-","-","-","-","-","-","-","-"]
[null,"MSDP","MSDP","-","-","-","-","-","-","-","-","-","-"]
["OAM","802.1AG","802.1AG","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"802.3AH","802.3AH","Y","Y","Y","Y","Y","-","-","-","-","-"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"ISSU","ISSU","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","-","-","-","-","-"]
[null,"端口自动节能","port auto power down","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"triple authentication","triple authentication","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","Y","Y","Y","Y","Y"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ","2K","2K","2K","2K","2K",256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","2K","2K","2K","2K","2K","1K","1K","1K","1K","1K"]
[null,"PORTAL认证用户数","portal  USERS","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512"]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+WRR","SP+WRR","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"SP+SDWRR","SP+SDWRR","-","-","-","-","-","-","-","-","-","-"]
[null,"SDWRR","SDWRR","-","-","-","-","-","-","-","-","-","-"]
[null,"WDRR","WDRR","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-","-","-","-","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"ACL logging","ACL logging","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 1K","up to 1K","up to 1K","up to 1K","up to 32","-","-","-","-","-"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","Ingress:512\nEgress:256","Ingress:512*2\nEgress:256*2","Ingress:512\nEgress:256","Ingress:512*2\nEgress:256*2","Ingress:512*2\nEgress:256*2","-","-","-","-","-"]
[null,"IPV6 ND数目","IPV6 ND NUM","up to 1K","up to 1K","up to 1K","up to 1K","up to 256","-","-","-","-","-"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND proxy","ND proxy","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SAVI","SAVI","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"PMTU","PMTU","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"RIPng","RIPng","Y","Y","Y","Y","-","-","-","-","-","-"]
[null,"OSPF V3","OSPF V3","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS V6","IS-IS V6","-","-","-","-","-","-","-","-","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","Y","Y","Y","Y","-","-","-","-","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","Y","Y","Y","Y","-","-","-","-","-","-"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"DHCP V6 relay","DHCP V6 relay","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"DHCP V6 server","DHCP V6 server","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD v6","BFD v6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"IPV6 TUNNEL","GRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","Y","Y","Y","Y","Y","-","-","-","-","-"]
[null,"6VPE","6VPE","-","-","-","-","-","-","-","-","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","Y(15.4W)","Y(15.4W)","-","-","-","-","Y","Y"]
[null,"是否支持中功率POE","POE(30W PER PORT)","-","-","Y(30W)","Y(30W)","-"]
[null,"总功率","Total Power","-","-","无PoE负载：42W\n满PoE负载：\nDC：795W(720W for poe)\nAC：465W(370W for poe)","无PoE负载：58W\n满PoE负载：\nDC：820W(720W for poe)\nAC：440W(320W for poe)","-","-","-","-","DC:370W\nAC:300","DC:740W\nAC:300"]
[null,"单端口最大功率","Power Per Port","-","-","30W","30W","-","-","-","-",15.4,15.4]
[null,"802.3af","802.3af","-","-","Y","Y","-","-","-","-","Y","Y"]
[null,"供电模式","Mode of  Voltage Supply","-","-","Data wire mode","Data wire mode","-","-","-","-","Data wire mode","Data wire mode"]
["物理特性\nphysical feature","电源","Power Supply","AC","AC","AC&RPS(52V)","AC&RPS(52V)","AC","AC","AC","AC","AC&DC","AC&DC"]
[null,"功耗(W)","Power Consummtion(w)","26W","41W","无PoE负载：42W\n满PoE负载：\nDC：795W(720W for poe)\nAC：465W(370W for poe)","无PoE负载：58W\n满PoE负载：\nDC：820W(720W for poe)\nAC：440W(320W for poe)","41W",40,40,50,"DC:430W;AC:450W","DC:820w;AC:465W"]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",88.7157037,139.8978405,"无PoE负载：143.3099829\n满PoE负载：\nDC：2712.653248(2456.742564 for poe)\nAC：1586.646239(1262.492707 for poe)","无PoE负载：197.9042621\n满PoE负载：\nDC：2797.956809(2456.742564 for poe)\nAC：1501.342678(1091.885584 for poe)",139.8978405,136.485698,136.485698,170.6071225,"DC:1467.2212535\nAC:1535.4641025","DC:2797.956809\nAC:1586.64623925"]
[null,"电源模块","Power Supply module","-","-","-","-","-","-","-","-","-","-"]
[null,"电源功率","power rating\n","-","-","-","-","-","-","-","-","-","-"]
[null,"电源负载均衡","power load-sharing\n","-","-","-","-","-","-","-","-","-","-"]
[null,"PDU电缆","PDU cable\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"湿度","Humidity","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%"]
[null,"温度","Temperature","0℃～50℃","0℃～50℃","0℃～50℃","0℃～50℃","0℃～50℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","< 5kg","< 5kg","< 10kg","< 10kg","< 5kg","《3.5kg.","《3.5kg.","《4kg","《5.8kg","《6.2kg"]
[null,"风扇","Fan NUM",1,1,6,6,1,1,1,1,2,2]
[null,"风向\n","Airflow direction\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back"]
[null,"风向反转","Ariflow reverse\n","-","-","-","-","-","-","-","-","-","-"]
[null,"风向控制","Airflow detection\n","-","-","-","-","-","-","-","-","-","-"]
[null,"缺省风向","Default Airflow\n","-","-","-","-","-","-","-","-","-","-"]
[null,"风扇速率可调","Fan Speed adjustment\n","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","-","-","-","-","-"]
[null,"安装方式","Installation\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise(low speed/high speed)","39.5/48.4","43.2/50.0","44.7/53.8","43.5/55.0","43.2/50.0",40.1,41.4,46.5,47.3,46.3]
[null,"MTBF(年)","MTBF",82.99,67.38,37.94,28.97,67.38,57.1,84.5,51.8,29.5,26.9]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,2,2]
[null,"RPS电源","RPS","-","-","Y","Y","-","-","-","-","Y(RPS1000-A3)","Y(RPS1000-A3)"]
[null,"热插拔","Hot-Swap","-","-","-","-","-","-","-","-","-","-"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*420（D）","440（W）*43.6(H)*420（D）","440（W）*43.6(H)*260（D）","440mm×43.6mm×260mm","440mm×43.6mm×260mm","440mm×43.6mm×260mm","440×43.6×420 mm","440×43.6×420 mm"]

{"sheet":"S3600&3600V2 EI&3610&5510","index":4,"n_rows":312,"n_cols":24,"rows_kept":312,"cut":false,"hidden":false,"merged":[[245,0,279,0],[280,0,285,0],[286,0,311,0],[181,0,187,0],[188,0,189,0],[190,0,203,0],[204,0,217,0],[218,0,232,0],[233,0,244,0],[154,0,164,0],[165,0,170,0],[171,0,172,0],[173,0,174,0],[175,0,178,0],[179,0,180,0],[148,0,152,0],[124,0,144,0],[145,0,147,0],[2,0,5,0],[6,0,35,0],[36,0,88,0],[89,0,110,0],[111,0,115,0],[116,0,123,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S3600V2-28TP-EI\n","S3600V2-52TP-EI\n","S3600V2-28TP-PWR-EI \n","S3600V2-52TP-PWR-EI \n","S3600V2-28F-EI\n","H3C S3600-28P-EI\n","H3C S3600-52P-EI\n","H3C S3600-28P-PWR-EI\n","H3C S3600-52P-PWR-EI\n","H3C S3600-28F-EI\n","E152","E328","E352","H3C-3100-52P","H3C S3610-28P","H3C S3610-52P","H3C S3610-28TP","H3C S3610-28F","S3610-52M","H3C S5510-24P","H3C S5510-24F"]
[null,"CPL","CPL","A3600-24 v2 EI\nJG299A","A3600-48 v2 EI\nJG300A","A3600-24-PoE+ v2 EI\nJG301A","A3600-24-PoE+ v2 EI\nJG301A","A3600-24-PoE+ v2 EI\nJG301A","A3600-24 EI \nJD331A","A3600-48 EI \nJD333A","A3600-24-PoE EI \nJD326A","A3600-48-PoE EI \nJD328A","A3600-24-SFP EI\nJD334A\n","-","-","-","A3100-48\nJD317A"," A3610-24 with 4 SPF Ports\nJD336A"," A3610-48\nJD335A","A3610-24 with 2 GigT and 2 SPF Ports\nJD337A","A3610-24-SFP\nJD338A","-","-","-"]
["端口\nport","固定配置","Fixed configration","24 *10/100TX+2 1000TX（combo）+4*1000SFP","48 *10/100TX+2 1000TX（combo）+4*1000SFP","24 *10/100TX（PoE+）+2 1000TX（combo）+4*1000SFP","48 *10/100TX（PoE+）+2 1000TX（combo）+4*1000SFP","24 *100FX+2 1000TX（combo）+4*1000SFP","24 * 10/100TX","48 * 10/100TX","24 * 10/100TX","48 * 10/100TX","2*10/100/1000TX","48 * 10/100TX","24 * 10/100TX","48 * 10/100TX","48 * 10/100TX","24 *10/100TX+4*1000SFP","48 *10/100TX+4*1000SFP","24 *10/100TX+2*1000SFP+2*10/100/1000T","24 100M SFP+2*1000SFP+2*10/100/1000T","4* 1000 M SFP(comb)","24 *10/100/1000TX( 4 comb)","24 * 1000SFP( 4 comb)"]
[null,"配置口","config interface","console","console","console","console","console","console","console ","console ","console","console ","console ","console","console ","console","console ","console ","console","console ","console ","console ","console "]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","-","-","-","-","-","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","24*100MSFP(2KM,15KM,40KM,80KM)/2* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/4*100MSFP","4* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/4*100MSFP","2* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/2*100MSFP","2* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/2*100MSFP/24*100MSFP(2km,15km,40km,80km)","6*8(10/100TX / 100FX-MM / 100FX-SM/100M SFP)","4* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/4*100MSFP","4* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/4*100MSFP"]
[null,"100FX SFP支持","100FX SFP support","-","-","-","-","百兆光口支持","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","12.8Gbps","17.6Gbps","12.8Gbps","17.6Gbps","12.8Gbps","12.8G","17.6G","12.8G","17.6G","12.8G","17.6G","12.8G","17.6G","17.6G","12.8G","17.6G","12.8G","12.8G","17.6G","48G","48G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","9.53M","13.1M","9.53M","13.1M","9.53M","9.53M","11.78M","9.53M","11.78M","9.53M","11.78M","9.53M","11.78M","11.78M","9.53M","13.1M","9.53M","9.53M","13.1M","35.71M","35.71M"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","\nGE:<5","\nGE:<5"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","-","LPM","LPM","-","LPM","LPM","LPM","LPM","LPM","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K",256,"1K","1K",256,"1K","1K","1K","1K","1K","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 8K","up to 16K","up to 16K","up to 8K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K"]
[null,"路由接口数","Max VLAN interface","1K","1K","1K","1K","1K",64,64,64,64,64,"-",64,64,"-",256,256,256,256,256,256,256]
[null,"IP V4路由条数","IP V4 routing num","up to 12K","up to 12K","up to 12K","up to 12K","up to 12K","up to 8448","up to 8448","up to 8448","up to 8448","up to 8448","-","up to 1088","up to 1088","-","up to 11K","up to 11K","up to 11K","up to 11K","up to 11K","up to 11K","up to 11K"]
[null,"整机支持L2组播数","Multicast L2  entries","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000",255,255,255,255,255,255,255,255,255,"ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n"]
[null,"整机支持L3组播数","Multicast L3  entries","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000",{"$nulls":9},"ipv4：512\nipv6：200","ipv4：512\nipv6：200","ipv4：512\nipv6：200","ipv4：512\nipv6：200","ipv4：512\nipv6：200","ipv4：512\nipv6：200","ipv4：512\nipv6：200"]
[null,"跨VLAN组播复制能力","Multicast entries","Y","Y","Y","Y","Y",{"$nulls":9},"Y","Y","Y","Y","Y","Y","Y"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","Y","Y","Y","Y","Y","NO","NO","NO","NO","NO","-","NO","NO","-","NO","NO","NO","NO","NO","NO","NO"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,"ACL流分类数","ACL Num","Ingress:1k\nEgress:512","Ingress:2k\nEgress:1k","Ingress:1k\nEgress:512","Ingress:2k\nEgress:1k","Ingress:1k\nEgress:512","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100",1824,1824,1824,1824,1824,"per 12 GE: 1824\nTotal:3648","per 12 GE: 1824\nTotal:3648"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM","TCAM","TCAM","TCAM","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","only IPv4 ACL apply on phisical port can support 2K. IPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K;\n IPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K;\n IPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K;\nIPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K;\nIPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K per 12 GE; \nIPv6 ACL, MAC ACL,user-defined ACL  can support 1K per 12 GE; \nVLAN ACL can support 1K totally.","only IPv4 ACL apply on phisical port can support 2K per 12 GE; \nIPv6 ACL, MAC ACL,user-defined ACL  can support 1K per 12 GE; \nVLAN ACL can support 1K totally."]
[null,"ACL 方向","ACL direction","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","Ingress:1k\nEgress:512","Ingress:1k\nEgress:512","Ingress:1k\nEgress:512","Ingress:1k\nEgress:512","Ingress:1k\nEgress:512","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100",1824,1824,1824,1824,1824,"per 12 GE: 1824\nTotal:3648","per 12 GE: 1824\nTotal:3648"]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","650Kbps(outbound)","650Kbps(outbound)","650Kbps(outbound)","650Kbps(outbound)","650Kbps(outbound)","650Kbps(outbound)","650Kbps(outbound)"]
[null,"流量整形","traffic shaping","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)"]
[null,"Flash大小","Flash","128M （NAND）","128M （NAND）","128M （NAND）","128M （NAND）","128M （NAND）","16M","16M","16M","16M","16M","8M","8M","8M","8M","32M","32M","32M","32M","32M","32M","32M"]
[null,"SDRAM大小","SDRAM","256M","256M","256M","256M","256M","64M","64M","64M","64M","64M","64M","64M","64M","64M","128M","128M","128M","128M","128M","128M","128M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","2M","4M","2M","4M","2M","32M","32M","32M","32M","32M","32M","32M","32M","32M","32M","32M","32M","32M","32M","32M","32M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1522,1522,1522,1522,1522,1522,1522]
[null,"Jumbo frame Support","Jumbo frame Support",10000,10000,10000,10000,10000,"9k","9k","9k","9k","9k","9k","9k","9k","9k","GE:10K\nFE:1552","GE:10K\nFE:1552","GE:10K\nFE:1552","GE:10K\nFE:1552","GE:10K\nFE:1552","GE:10K","GE:10K"]
[null,"堆叠方式","Stack mode","IRF2","IRF2","IRF2","IRF2","IRF2","IRF","IRF","IRF","IRF","IRF","HGMP STACK","IRF(only DDM DLA)","IRF(only DDM DLA)","HGMP STACK","IRF LITE","IRF LITE","IRF LITE","IRF LITE","IRF LITE","IRF LITE","IRF LITE"]
[null,"堆叠带宽","Stack bandwidth","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","stackable port number:1/2\nstack bandwidth: first 2 prots/1Gbps（双向2Gbps）, last 2 ports with SFP/1Gbps（双向2Gbps）,last 2 ports with Stack Cable/2.5Gbps（双向5Gbps）.\n堆叠口支持聚合","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G","4G","4G","4G","4G","4G","4G"]
[null,"堆叠台数","MAX Stack num",9,9,9,9,9,8,8,8,8,8,16,8,8,16,16,16,16,16,16,16,16]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K",16,"1K","1K","1K","1K","1K","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","4K","4K","4K","4K","4K",256,"2K","2K",256,"2.5K","2.5K","2.5K","2.5K","2.5K","2.5K","2.5K"]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"PVST+","PVST+","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"TC snooping","TC snooping","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-"]
[null,"Smart Link","Smart Link","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM SNOOPING","PIM SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-"]
[null,"组播VLAN","MVR","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(MVR+)","Y(MVR+)","Y(MVR+)","Y(MVR+)","Y(MVR+)","Y(MVR+)","Y(MVR+)"]
[null,"组播VLAN+","MVR+","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"RRPP multi-instances","RRPP multi-instances","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","-","-","-","-","-","-","-","-","-","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)"]
[null,"EAD","support users by 5 rules","per port :102\nall:102/204(双芯片)","per port :102\nall:102/204(双芯片)","per port :102\nall:102/204(双芯片)","per port :102\nall:102/204(双芯片)","per port :102\nall:102/204(双芯片)","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all: 360\nper fe:50\nper ge:100","all: 360\nper fe:50\nper ge:100","all: 360\nper fe:50\nper ge:100","all: 360\nper fe:50\nper ge:100","all: 360\nper fe:50\nper ge:100","all: 720\nper ge:100","all: 720\nper ge:100"]
[null,null,"support users by 10 rules","per port :51\nall:51/102(双芯片)","per port :51\nall:51/102(双芯片)","per port :51\nall:51/102(双芯片)","per port :51\nall:51/102(双芯片)","per port :51\nall:51/102(双芯片)","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all: 180\nper fe:25\nper ge:50","all: 180\nper fe:25\nper ge:50","all: 180\nper fe:25\nper ge:50","all: 180\nper fe:25\nper ge:50","all: 180\nper fe:25\nper ge:50","all: 360\nper ge:50","all: 360\nper ge:50"]
[null,null,"support users by 20 rules","per port :25\nall:25/50(双芯片)","per port :25\nall:25/50(双芯片)","per port :25\nall:25/50(双芯片)","per port :25\nall:25/50(双芯片)","per port :25\nall:25/50(双芯片)","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all: 90\nper fe:12\nper ge:24","all: 90\nper fe:12\nper ge:24","all: 90\nper fe:12\nper ge:24","all: 90\nper fe:12\nper ge:24","all: 90\nper fe:12\nper ge:24","all: 180\nper ge:25","all: 180\nper ge:25"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","单芯片：4S\n双芯片：4S","单芯片：4S\n双芯片：4S","单芯片：4S\n双芯片：4S","单芯片：4S\n双芯片：4S","单芯片：4S\n双芯片：4S","17s","17s","17s","17s","17s","17s","17s","17s","17s","15s","15s","15s","15s","15s","15s","15s"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","58s","100s","58s","100s","58s","100s","58s","100s","100s","35s","60s","35s","35s","60s","35s","60s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","单芯片：9S\n双芯片：10S","28s","42s","28s","42s","28s","42s","28s","42s","42s","50s","100s","50s","50s","100s","50s","100s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-"]
[null,"IP+PORT绑定个数","IP+PORT Binding","all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","all 512，per port 256","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","all 512，per port 256","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","all 512，per port 256","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","GE:50   8FE:100\nTotal:500","100 per port\nTotal: 500","100 per port\nTotal: 500","100 per port\nTotal: 500","100 per port\nTotal: 500","100 per port\nTotal: 500","100 per port\nTotal: 500","100 per port\nTotal: 500"]
[null,"可聚合端口数目","MAX num in one link group","8FE/8GE","8FE/8GE","8FE/8GE","8FE/8GE","8FE/8GE",8,8,8,8,8,8,8,8,8,"8FE/4GE","8FE/4GE","8FE/4GE","8FE/4GE","8FE/4GE","8GE","8GE"]
[null,"端口聚合组数","Link group num","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )",26,"8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )",26,14,26,14,14,26,12,12]
[null,"restore port default config","restore port default config","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","Y","Y","Y","Y","Y",{"$nulls":9},"Y","Y","Y","Y","Y","Y","Y"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:4","N:4","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","8:1","8:1","8:1","8:1","8:1","8:1","8:1"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:4","N:4","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","N","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","flow constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y（1%，pps）","Y（1%，pps）","Y（1%，pps）","Y(1% or pps)","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）"]
[null,"多播风暴抑制","Multicast  Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y（1%，pps）","Y（1%，pps）","Y（1%，pps）","Y(1% or pps)","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y（1%，pps）","Y（1%，pps）","Y（1%，pps）","Y(1% or pps)","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y（%1）"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","-","-","-","-","-","-","-","-","-","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )"]
[null,"Voice Vlan","Voice Vlan","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SuperVLAN","SuperVLAN","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RIPV1/2","RIPV1/2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V2","OSPF V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"IS-IS","IS-IS","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"静态路由","Static routing","Y(2k)","Y(2k)","Y(2k)","Y(2k)","Y(2k)",256,256,256,256,256,"-",64,64,"-","1K","1K","1K","1K","1K","1K","1K"]
[null,"支持second ip数目","MAX num of second ip ",48,48,48,48,48,4,4,4,4,4,"-",4,4,"-",9,9,9,9,9,9,9]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP","VRRP","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16 instance)","Y(16 instance)","Y(16 instance)","Y(16 instance)","Y(16 instance)","Y(16 instance)","Y(16 instance)"]
[null,"VRRPE","VRRPE","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BFD","BFD","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","-","-","-","-","-","-","-","-","-","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)"]
[null,"Routed ports","Routed ports","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"ECMP(等值路由)","ECMP","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*3)","Y(256*3)","Y(256*3)","Y(256*3)","Y(256*3)","-","-","-","-","Y(600*4)","Y(600*4)","Y(600*4)","Y(600*4)","Y(600*4)","Y(600*4)","Y(600*4)"]
[null,"策略路由","Policy based routing","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","Y(63 instances)","Y(63 instances)","Y(63 instances)","Y(63 instances)","Y(63 instances)","-","-","-","-","-","-","-","-","-","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS","MPLS label number","MPLS label number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS label depth","MPLS label depth","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS interface number","MPLS interface number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"static LSP number","static LSP number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"等价LSP","等价LSP","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP local peer number","LDP local peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP remote peer number","LDP remote peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls TE","mpls TE","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp ping","mpls lsp ping","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VPN number","VPN number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"CE number per VPN","CE number per VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L3VPN","VRF number","VRF number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"interface number per VRF","interface number per VRF","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["VPLS","VSI number","VSI number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPFIX","IPFIX","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP V3","IGMP V3","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-SM","PIM-SM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-SSM","PIM-SSM","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-DM","PIM-DM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"双向PIM","BI-PIM","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MSDP","MSDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
["OAM","802.1AG","802.1AG","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3AH","802.3AH","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ISSU","ISSU","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","-","-","-","-","-","-","-","-","-"]
[null,"端口自动节能","port auto power down","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-"]
[null,"triple authentication","triple authentication","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","Y","Y",null,null,"-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ","2K","2K","2K","2K","2K",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","2K","2K","2K","2K","2K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"PORTAL认证用户数","portal  USERS","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","-","-","-","-","-","-","-","-"]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-"]
[null,"SP+WRR","SP+WRR","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SDWRR","SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WDRR","WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ACL logging","ACL logging","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 6K","up to 6K","up to 6K","up to 6K","up to 6K","-","-","-","-","-","-","-","-","-","1K","1K","1K","1K","1K","1K","1K"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","Ingress:512\nEgress:256","Ingress:512\nEgress:256","Ingress:512\nEgress:256","Ingress:512\nEgress:256","Ingress:512\nEgress:256","-","-","-","-","-","-","-","-","-","1K","1K","1K","1K","1K","per 12 GE: 1K\nTotal:2K","per 12 GE: 1K\nTotal:2K"]
[null,"IPV6 ND数目","IPV6 ND NUM","up to 4K","up to 4K","up to 4K","up to 4K","up to 4K","-","-","-","-","-","-","-","-","-","2.5K","2.5K","2.5K","2.5K","2.5K","2.5K","2.5K"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND","ND","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND proxy","ND proxy","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SAVI","SAVI","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PMTU","PMTU","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","RIPng","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V3","OSPF V3","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"IS-IS V6","IS-IS V6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPV6 策略路由","IPV6 policied routing","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"MLD SNOOPING","MLD SNOOPING","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","-","-","-","-","-","-","-","-","-","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)"]
[null,"IPv6 PIM DM","IPv6 PIM DM","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 relay","DHCP V6 relay","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 server","DHCP V6 server","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BFD v6v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv7 STATIC ROUTING)","BFD v6v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv7 STATIC ROUTING)","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP"]
[null,"6VPE","6VPE","N","N","N","N","N","-","-","-","-","-","-","-","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","Y(15.4W)","Y(15.4W)","-","-","-","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"是否支持中功率POE","POE(30W PER PORT)","-","-","Y(30W)","Y(30W)","-",{"$nulls":9},"-","-","-","-","-","-","-"]
[null,"总功率","Total Power","-","-","无PoE负载：42W\n满PoE负载：\nDC：795W(720W for poe)\nAC：465W(370W for poe)","无PoE负载：58W\n满PoE负载：\nDC：820W(720W for poe)\nAC：440W(320W for poe)","-","-","-","DC:370W\nAC:300","DC:740W\nAC:300","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"单端口最大功率","Power Per Port","-","-","30W","30W","-","-","-",15.4,15.4,"-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3af","802.3af","-","-","Y","Y","-","-","-","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-","Data wire mode","Data wire mode","-","-","-","Data wire mode","Data wire mode","-","-","-","-","-","-","-","-","-","-","-","-"]
["物理特性\nphysical feature","电源","Power Supply","AC&RPS(48V)","AC&RPS(48V)","AC&RPS(52V)","AC&RPS(52V)","AC&RPS(48V)","AC&DC","AC&DC","AC&DC","AC&DC","AC&DC","AC","AC","AC","AC","AC&DC","AC&DC","AC&DC","AC&DC","AC/DC","dual power suppoy:\nAC/DC","dual power suppoy:\nAC/DC"]
[null,"功耗(W)","Power Consummtion(w)","31W","43W","无PoE负载：42W\n满PoE负载：\nDC：795W(720W for poe)\nAC：465W(370W for poe)","无PoE负载：58W\n满PoE负载：\nDC：820W(720W for poe)\nAC：440W(320W for poe)","60W",40,50,"DC:430W;AC:450W","DC:820w;AC:465W",65,50,40,50,50,35,45,40,60,110,80,75]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",105.776416,146.7221254,"无PoE负载：143.3099829\n满PoE负载：\nDC：2712.653248(2456.742564 for poe)\nAC：1586.646239(1262.492707 for poe)","无PoE负载：197.9042621\n满PoE负载：\nDC：2797.956809(2456.742564 for poe)\nAC：1501.342678(1091.885584 for poe)",204.728547,136.485698,170.6071225,"DC:1467.2212535\nAC:1535.4641025","DC:2797.956809\nAC:1586.64623925",221.78925925000001,170.6071225,136.485698,170.6071225,170.6071225,119.42498575,153.54641025,136.485698,204.72854700000002,375.3356695,272.971396,255.91068375]
[null,"电源模块","Power Supply module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"电源功率","power rating\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"电源负载均衡","power load-sharing\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PDU电缆","PDU cable\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"湿度","Humidity","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%"]
[null,"温度","Temperature","0℃～50℃","0℃～50℃","0℃～50℃","0℃～50℃","0℃～50℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃","0~45","0~45","0~45","0~45","0~45","0~45","0~45"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","< 5kg","< 5kg","< 10kg","< 10kg","< 5kg","《3.5kg.","《4kg","《3.5kg.","《4kg","《3.5kg.","《4kg","《3.5kg.","《4kg","《4kg","<4KG","<4KG","<4KG","<4KG","<8.5KG","<5KG","<5KG"]
[null,"风扇","Fan NUM",1,1,6,6,2,1,1,2,2,5,1,1,1,1,1,1,1,2,2,2,3]
[null,"风向\n","Airflow direction\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back"]
[null,"风向反转","Ariflow reverse\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"风向控制","Airflow detection\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"缺省风向","Default Airflow\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"风扇速率可调","Fan Speed adjustment\n","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","-","-","-","-","-","-","-","-","-"]
[null,"安装方式","Installation\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","-","-","-","-","-","-","-","-","-"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise(low speed/high speed)","42.8/49.9","43.2/50.0","44.7/53.8","43.5/55.0","43.5/50.1",40.1,46.5,47.3,46.3,51.3,46.5,40.1,46.5,46.5,41.7,47.8,41.6,48.8,51.6,44.8,47.6]
[null,"MTBF(年)","MTBF",82.68,67.36,37.94,28.97,74.43,45.91,42.4,29.5,26.9,51.9,51.8,57.1,51.84,51.8,32.2,30.3,31.4,26.9,31.24,21.5,27]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2]
[null,"RPS电源","RPS","Y","Y","Y","Y","Y","Y（RPS800-A3/RPS1000-A3）","Y（RPS800-A / RPS1000-A3）","Y(RPS1000-A3)","Y(RPS1000-A3)","Y（RPS800-A /RPS1000-A3）","-","-","-","-","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A ）","Y（RPS800-A）(only for DC)","Y（RPS800-A）(only for DC)"]
[null,"热插拔","Hot-Swap","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*420（D）","440（W）*43.6(H)*420（D）","440（W）*43.6(H)*260（D）","440mm×43.6mm×260mm","440mm×43.6mm×260mm","440×43.6×420 mm","440×43.6×420 mm","440mm×43.6mm×260mm","440×43.6×260","440×43.6×260","440×43.6×260","440×43.6×260","440×43.6×260","440×43.6×260","440×43.6×260","440×43.6×260","436×86×390","440×43.6×360 ","440×43.6×360 "]

{"sheet":"S5100EI","index":5,"n_rows":250,"n_cols":13,"rows_kept":250,"cut":false,"hidden":false,"merged":[[1,0,4,0],[5,0,33,0],[190,0,197,0],[82,0,102,0],[103,0,107,0],[108,0,115,0],[116,0,134,0],[140,0,141,0],[145,0,151,0],[154,0,167,0],[229,0,233,0],[234,0,249,0],[34,0,81,0],[198,0,228,0],[176,0,189,0],[152,0,153,0],[142,0,144,0],[168,0,175,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","H3C S5100-24P-EI\n","H3C S5100-48P-EI\n","H3C S5100-26C-EI\n","H3C S5100-50C-EI\n","H3C S5100-8P-EI\n","H3C S5100-16P-EI\n","H3C S5100-8P-PWR-EI\n","H3C S5100-16P-PWR-EI\n","H3C S5100-26C-PWR-EI\n","H3C S5100-50C-PWR-EI\n"]
["端口\nport","固定配置","Fixed configration","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","8 *10/100/1000TX, 2*1000MSFP","16 *10/100/1000TX( 4 comb)","8 *10/100/1000TX, 2*1000MSFP","16 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)"]
[null,"配置口","config interface","console ","console ","console","console ","console ","console ","console","console ","console ","console "]
[null,"可选配置（插槽数*端口个数）","optional configration(slot× interface board)","4*1000MSFP(274m,550m,10km,40km,70km,RJ45)/4*100MSFP","4*1000MSFP(274m,550m,10km,40km,70km,RJ45);4*100MSFP","4*1000MSFP(274m,550m,10km,40km,70km,RJ45)/4*100MSFP /  2*10GBase-SX-XFP（300m）/ 2*10GBase-LX-XFP（10km）/ 2* 10GBase-LH40-XFP（40km） / 2*10GBASE-SX-XENPAK（300m）/ 2*10GBASE-LX-XENPAK（10km）/ 2*10GBASE-LH40-XENPAK（40km）/ 2*10GBASE Stack","4*1000MSFP(274m,550m,10km,40km,70km,RJ45) /4*100MSFP/  2*10GBase-SX-XFP（300m）/ 2*10GBase-LX-XFP（10km）/ 2* 10GBase-LH40-XFP（40km） / 2*10GBASE-SX-XENPAK（300m）/ 2*10GBASE-LX-XENPAK（10km）/ 2*10GBASE-LH40-XENPAK（40km）/ 2*10GBASE Stack","2*1000MSFP(274m,550m,10km,40km,70km,RJ45)/2*100MSFP","4*1000MSFP(274m,550m,10km,40km,70km,RJ45)/4*100MSFP","2*1000MSFP(274m,550m,10km,40km,70km,RJ45)/2*100MSFP","4*1000MSFP(274m,550m,10km,40km,70km,RJ45)/4*100MSFP","4*1000MSFP(274m,550m,10km,40km,70km,RJ45) /4*100MSFP/  2*10GBase-SX-XFP（300m）/ 2*10GBase-LX-XFP（10km）/ 2* 10GBase-LH40-XFP（40km） / 2*10GBASE-SX-XENPAK（300m）/ 2*10GBASE-LX-XENPAK（10km）/ 2*10GBASE-LH40-XENPAK（40km）/ 2*10GBASE Stack","4*1000MSFP(274m,550m,10km,40km,70km,RJ45) /4*100MSFP/  2*10GBase-SX-XFP（300m）/ 2*10GBase-LX-XFP（10km）/ 2* 10GBase-LH40-XFP（40km） / 2*10GBASE-SX-XENPAK（300m）/ 2*10GBASE-LX-XENPAK（10km）/ 2*10GBASE-LH40-XENPAK（40km）/ 2*10GBASE Stack"]
[null,"100FX SFP支持","100FX SFP","-","-","-","-","-","-","-","-","-","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","48G","96G","88G","136G","20G","32G","20G","32G","88G","136G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","35.7Mpps","71.4Mpps","65.47Mpps","101.2Mpps","14.88Mpps","23.8Mpps","14.88Mpps","23.8Mpps","65.47Mpps","101.2Mpps"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","GE:<5\n","GE:<5\n","GE:<5\n","GE:<5\n","GE:<5\n","GE:<5\n","GE:<5\n","GE:<5\n","GE:<5\n","GE:<5\n"]
[null,"三层路由转发机制","L3 route forwarding mode","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL"]
[null,"静态MAC个数","Static mac table","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 16K","up to 16K","up to 16K","up to 16K","up to 8K","up to 16K","up to 8K","up to 16K","up to 16K","up to 16K"]
[null,"路由接口数","Max VLAN interface",8,8,8,8,8,8,8,8,8,8]
[null,"IP单播路由表深度","IP unicast routing table",32,32,32,32,32,32,32,32,32,32]
[null,"IP V4路由条数","IP V4 routing num",32,32,32,32,32,32,32,32,32,32]
[null,"整机支持组播数","Multicast entries","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","-","-","-","-","-","-","-","-","-","-"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8,8,8,8,8,8,8,8,8]
[null,"ACL流分类数","ACL Num","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:1920\nextended:960(per port max : standard:200\nextended:100)","standard:960\nextended:480(per port max : standard:200\nextended:100)","standard:1920\nextended:960\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:1920\nextended:960\n(per port max : standard:200\nextended:200)"]
[null,"ACL机制说明","ACL policy description","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl","global acl"]
[null,"ACL 方向","ACL direction"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:1920\nextended:960(per port max : standard:200\nextended:100)","standard:960\nextended:480(per port max : standard:200\nextended:200)","standard:1920\nextended:960\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:960\nextended:480\n(per port max : standard:200\nextended:200)","standard:1920\nextended:960\n(per port max : standard:200\nextended:200)"]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","\noutbound: shaping\nGE <=80M 20K\nGE 80M～1G 260K\n\n","\noutbound: shaping\nGE <=80M 20K\nGE 80M～1G 260K\n\n","\noutbound: shaping\nGE <=80M 20K\nGE 80M～1G 260K\n10GE 2.5M\n","\noutbound: shaping\nGE <=80M 20K\nGE 80M～1G 260K\n10GE 2.5M\n","\noutbound: \nGE <=80M 20K\nGE 80M～1G 260K","\noutbound:\nGE <=80M 20K\nGE 80M～1G 260K","\noutbound: \nGE <=80M 20K\nGE 80M～1G 260K","\noutbound:\nGE <=80M 20K\nGE 80M～1G 260K","\noutbound: shaping\nGE <=80M 20K\nGE 80M～1G 260K\n10GE 2.5M\n","\noutbound: shaping\nGE <=80M 20K\nGE 80M～1G 260K\n10GE 2.5M\n"]
[null,"流量整形","traffic shaping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n1～10G 10M","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n1～10G 10M","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n1～10G 10M","inbound:\n0～1M 1K\n1～10M 10K\n10～100M 100K\n100M～1G 1M\n1～10G 10M"]
[null,"Flash大小","Flash","16M","16M","16M","16M","16M","16M","16M","16M","16M","16M"]
[null,"SDRAM大小","SDRAM","64M","64M","64M","64M","64M","64M","64M","64M","64M","64M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","0.75M ","1.5M","0.75M ","1.5M","0.125M ","0.75M ","0.125M ","0.75M ","0.75M ","1.5M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","9k","9k","9k","9k","9k","9k","9k","9k","9k","9k"]
[null,"堆叠方式","Stack mode","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK"]
[null,"堆叠带宽","Stack bandwidth","4G(Bidirection and loop network)","4G(Bidirection and loop network)","40G(Bidirection and loop network)","40G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","40G(Bidirection and loop network)","40G(Bidirection and loop network)"]
[null,"堆叠台数","MAX Stack num",16,16,16,16,16,16,16,16,16,16]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num",16,16,16,16,16,16,16,16,16,16]
[null,"动态ARP数目","Dynamic ARP num",256,256,256,256,256,256,256,256,256,256]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","-","-","-","-","-","-","-","-","-","-"]
[null,"LACP短超时","LACP short-time","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1p","802.1p","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x","802.1x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link","Smart Link","Y(24 group)","Y(24 group)","Y(24 group)","Y(24 group)","Y(24 group)","Y(24 group)","Y(24 group)","Y(24 group)","Y(24 group)","Y(24 group)"]
[null,"Smart Link multi-instances","Smart Link multi-instances","-","-","-","-","-","-","-","-","-","-"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN","MVR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN+","MVR+","-","-","-","-","-","-","-","-","-","-"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP multi-instances","RRPP multi-instances","-","-","-","-","-","-","-","-","-","-"]
[null,"EAD","support users by 5 rules","all:96\nper port max:40","all:192\nper port max:40","all:96\nper port max:40","all:192\nper port max:40","all:96\nper port max:40","all:96\nper port max:40","all:96\nper port max:40","all:96\nper port max:40","all:96\nper port max:40","all:192\nper port max:40"]
[null,null,"support users by 10 rules","all:48\nper port max:20","all:96\nper port max:20","all:48\nper port max:20","all:96\nper port max:20","all:48\nper port max:20","all:48\nper port max:20","all:48\nper port max:20","all:48\nper port max:20","all:48\nper port max:20","all:96\nper port max:20"]
[null,null,"support users by 20 rules","all:24\nper port max:10","all:48\nper port max:10","all:24\nper port max:10","all:48\nper port max:10","all:24\nper port max:10","all:24\nper port max:10","all:24\nper port max:10","all:24\nper port max:10","all:24\nper port max:10","all:48\nper port max:10"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","21s","21s","21s","21s","21s","21s","21s","21s","21s","21s"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","61s","92s","61s","92s","67s","67s","67s","67s","61s","92s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","33s","63s","33s","63s","41s","41s","41s","41s","33s","63s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","-","-","-","-","-","-","-","-","-","-"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IP+PORT绑定个数","IP+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding",128,128,128,128,128,128,128,128,128,128]
[null,"可聚合端口数目","MAX num in one link group","8GE","8GE","8GE/2*10GE","8GE/2*10GE","8GE","8GE","8GE","8GE","8GE/2*10GE","8GE/2*10GE"]
[null,"端口聚合组数","Link group num",12,24,13,25,5,8,5,8,13,25]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","-","-","-","-","-","-","-","-","-","-"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","storm constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","-","-","-","-","-","-","-","-","-","-"]
[null,"多播风暴抑制","Multicast  Suppression","-","-","-","-","-","-","-","-","-","-"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1%, pps)","Y(1%, pps)","Y(1% ,pps)","Y(1% ,pps)","Y(1%, pps)","Y(1% ,pps)","Y(1%, pps)","Y(1%, pps)","Y(1%, pps)","Y(1%, pps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于IP子网VLAN","IP subnet based vlan","-","-","-","-","-","-","-","-","-","-"]
[null,"基于协议类型VLAN","Protocal based vlan","Y（8）","Y（8）","Y（8）","Y（8）","Y（8）","Y（8）","Y（8）","Y（8）","Y（8）","Y（8）"]
[null,"Voice Vlan","Voice Vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SuperVLAN","SuperVLAN","-","-","-","-","-","-","-","-","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","-","-","-","-","-","-","-","-","-","-"]
["IP路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","-","-","-","-","-","-","-","-","-","-"]
[null,"RIPV1/2","RIPV1/2","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V2","OSPF V2","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS","IS-IS","-","-","-","-","-","-","-","-","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","-","-","-","-","-","-","-","-","-","-"]
[null,"静态路由","Static routing",32,32,32,32,32,32,32,32,32,32]
[null,"支持second ip数目","MAX num of second ip ","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRP","VRRP","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRPE","VRRPE","-","-","-","-","-","-","-","-","-","-"]
[null,"BFD","BFD","-","-","-","-","-","-","-","-","-","-"]
[null,"ECMP(等值路由)","ECMP","-","-","-","-","-","-","-","-","-","-"]
[null,"策略路由","Policy based routing","-","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","-","-","-","-","-","-","-","-","-","-"]
["MCE组播","MCE MULTICAST","MCE MULTICAST","-","-","-","-","-","-","-","-","-","-"]
["MPLS","MPLS","MPLS","-","-","-","-","-","-","-","-","-","-"]
["组播VPN","multicast vpn","multicast vpn","-","-","-","-","-","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","-","-","-","-","-","-","-","-","-","-"]
[null,"NetStream/NetFlow/IPFIX","NetStream/NetFlow","-","-","-","-","-","-","-","-","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3","IGMP V3","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SM","PIM-SM","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SSM","PIM-SSM","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-DM","PIM-DM","-","-","-","-","-","-","-","-","-","-"]
[null,"双向PIM","BI-PIM","-","-","-","-","-","-","-","-","-","-"]
[null,"MSDP","MSDP","-","-","-","-","-","-","-","-","-","-"]
["OAM","802.1AG","802.1AG","-","-","-","-","-","-","-","-","-","-"]
[null,"802.3AH","802.3AH","-","-","-","-","-","-","-","-","-","-"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","-","-","-","-","-","-","-","-","-","-"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2","Y(256)","Y(256)","Y(256)","Y(256)","Y(256)","Y(256)","Y(256)","Y(256)","Y(256)","Y(256)"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","-","-","-","-","-","-","-","-","-","-"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","-","-","-","-","-","-","-","-","-","-"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","-","-","-","-","-","-","-","-","-","-"]
[null,"ISSU","ISSU","-","-","-","-","-","-","-","-","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"triple authentication","triple authentication","-","-","-","-","-","-","-","-","-","-"]
[null,"HWTACACS","TACACS+","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server",{"$nulls":5},"-","-","-","-","-"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","-","-","-","-","-","-","-","-","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-","-","-","-","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ",256,256,256,256,256,256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SDWRR","SDWRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+SDWRR","SP+SDWRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"设备buffer可配置特性","BUFFER configurable","-","-","-","-","-","-","-","-","-","-"]
[null,"ACL logging","ACL logging","-","-","-","-","-","-","-","-","-","-"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","-","-","-","-","-","-","-","-","-","-"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:1920\nextended:960(per port max : standard:200\nextended:100)","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:1920\nextended:960(per port max : standard:200\nextended:100)","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:960\nextended:480\n\n(per port max : standard:200\nextended:100)","standard:1920\nextended:960(per port max : standard:200\nextended:100)"]
[null,"IPV6 ND数目","IPV6 ND NUM","-","-","-","-","-","-","-","-","-","-"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND proxy","ND proxy","-","-","-","-","-","-","-","-","-","-"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PMTU","PMTU","-","-","-","-","-","-","-","-","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","RIPng","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V3","OSPF V3","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS V6","IS-IS V6","-","-","-","-","-","-","-","-","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","-","-","-","-","-","-","-","-","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 双向PIM","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 relay","DHCP V6 relay","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 server","DHCP V6 server","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD v6","BFD v6","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 TUNNEL","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","-","-","-","-","-","-","-","-","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","-","-","-","-","Y","Y","Y","Y"]
[null,"总功率","Total Power","-","-","-","-","-","-","65W","125W","AC:370W\nDC:370W","AC:370W\nDC:740W"]
[null,"单端口最大功率","Power Per Port","-","-","-","-","-","-","15.4W","15.4W","15.4W","15.4W"]
[null,"802.3af","802.3af","-","-","-","-","-","-","Y","Y","Y","Y"]
[null,"供电模式","Mode of  Voltage Supply","-","-","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","Data wire mode"]
["物理特性\nphysical feature","电源","Power Supply","AC&DC","AC&DC","AC&DC","AC&DC","AC","AC","AC","AC","AC&DC","AC&DC"]
[null,"功耗(W)","Power Consummtion",46,97,68,116,18,26,100,170,"AC:500W(370W fow poe)\nDC:435W(370W for poe)","AC:540W(370W for poe)\nDC:840W(740W for poe)"]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",156.9585527,330.97781765,232.0256866,395.8085242,61.418564100000005,88.7157037,341.214245,580.0642165,"AC:1706.071225\nDC:1484.28196575","AC:1842.556923\nDC:2866.199658"]
[null,"湿度","Humidity","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%"]
[null,"温度","Temperature","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","<4 kg","<.4.5kg","<4 kg","< 5kg","<1.6kg","<2.3kg","<1.6kg","<2.3kg","<4 kg","< 5kg"]
[null,"风扇","Fan NUM",1,2,2,3,1,1,2,3,2,3]
[null,"噪音（LPA，DB）\n（ISO7779标准bystander声压级噪声测试）","Noise",46.7,50.2,50.1,51.5,"35.2（low speed）\n40(high speed)","35.1（low speed）\n44.1(high speed)","35.3（low speed）\n43.5(high speed)","36.2（low speed）\n46(high speed)","48.3（low speed）\n51.8(high speed)","47.9（low speed）\n52(high speed)"]
[null,"MTBF(年)","MTBF",22,13.3,"21.1/18.9/17.4(STACK/XFP/XENPAK)","12.1/11.3/10.8(STACK/XFP/XENPAK)",44.2,33.9,34.3,30.4,"20.6/18.4/17.1(STACK/XFP/XENPAK)","16.2/14.8/13.9(STACK/XFP/XENPAK)"]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,2,2]
[null,"RPS电源","RPS","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","N","N","N","N","Y（RPS1000-A3）","Y（RPS1000-A3）"]
[null,"热插拔","Hot-Swap","N","N","N","N","N","N","N","N","N","N"]
[null,"是否支持POE受电","Power Supply by POE","N","N","N","N","N","N","N","N","N","N"]
[null,"外形尺寸（宽x高x深）","Size (WxHxd)","440×43.6×260 （mm3）","440×43.6×260 （mm3）","440×43.6×300（mm3）","440×43.6×300（mm3）","230×43.6×200 （mm3）","300×43.6×220 （mm3）","300×43.6×220 （mm3）","300×43.6×260 （mm3）","440×43.6×420（mm3）","440×43.6×420（mm3）"]

{"sheet":"S5600","index":6,"n_rows":250,"n_cols":16,"rows_kept":250,"cut":false,"hidden":false,"merged":[[1,0,4,0],[198,0,228,0],[229,0,233,0],[234,0,249,0],[34,0,81,0],[176,0,189,0],[140,0,141,0],[152,0,153,0],[142,0,144,0],[5,0,33,0],[190,0,197,0],[82,0,102,0],[103,0,107,0],[108,0,115,0],[116,0,134,0],[145,0,151,0],[154,0,167,0],[168,0,175,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","H3C S5600-26C\n","H3C S5600-26C-PWR\n","H3C S5600-50C\n","H3C S5600-50C-PWR\n","H3C S5600-26F\n"]
["端口\nport","固定配置","Fixed configration","24 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 * 1000SFP(4 comb)"]
[null,"配置口","config interface","console ","console ","console","console ","console "]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","1*8SFP(550m,10km,30km，40km,70km,RJ45) /  1*2 10GBase-LR-XFP（10km）/ 1*2 10GBase-ER-XFP（40km） / 1*10GBASE-LR-XENPAK（10km）/ 1*10GBASE-ER-XENPAK（40km）","1*8SFP(550m,10km,30km，40km,70km,RJ45) /  1*2 10GBase-LR-XFP（10km）/ 1*2 10GBase-ER-XFP（40km） / 1*10GBASE-LR-XENPAK（10km）/ 1*10GBASE-ER-XENPAK（40km）","1*8SFP(550m,10km,30km，40km,70km,RJ45) /  1*2 10GBase-LR-XFP（10km）/ 1*2 10GBase-ER-XFP（40km） / 1*10GBASE-LR-XENPAK（10km）/ 1*10GBASE-ER-XENPAK（40km）","1*8SFP(550m,10km,30km，40km,70km,RJ45) /  1*2 10GBase-LR-XFP（10km）/ 1*2 10GBase-ER-XFP（40km） / 1*10GBASE-LR-XENPAK（10km）/ 1*10GBASE-ER-XENPAK（40km）","1*8SFP(550m,10km,30km，40km,70km,RJ45) /  1*2 10GBase-LR-XFP（10km）/ 1*2 10GBase-ER-XFP（40km） / 1*10GBASE-LR-XENPAK（10km）/ 1*10GBASE-ER-XENPAK（40km）"]
[null,"100FX SFP支持","100FX SFP支持","-","-","-","-","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","88G","88G","136G","136G","88G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","65.47M","65.47M","101.19M","101.19M","65.47M"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM","LPM","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1K","1K","1K","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K"]
[null,"路由接口数","Max VLAN interface",128,128,128,128,128]
[null,"IP单播路由表深度(HASH算法)","IP unicast routing table","up  to 16K","up  to 16K","up  to 16K","up  to 16K","up  to 16K"]
[null,"IP V4路由条数\n(HASH算法)","IP V4 routing num","up  to 16K","up  to 16K","up  to 16K","up  to 16K","up  to 16K"]
[null,"整机支持组播数","Multicast entries","1K","1K","1K","1K","1K"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","NO","NO","NO","NO","NO"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8,8,8,8]
[null,"ACL流分类数","ACL Num","100/port","100/port","100/port","100/port","100/port"]
[null,"ACL机制说明","ACL policy description","Each block  one GE.\nIncluding rule and mask.","Each block  one GE.\nIncluding rule and mask.","Each block  one GE.\nIncluding rule and mask.","Each block  one GE.\nIncluding rule and mask.","Each block  one GE.\nIncluding rule and mask."]
[null,"ACL 方向","ACL direction"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","100/port","100/port","100/port","100/port","100/port"]
[null,"VACL","ACL BASED VLAN","-","-","-","-","-"]
[null,"端口限速粒度","port line-rate granularity","GE:64K\n10GE:1M\n(outbound)","GE:64K\n10GE:1M\n(outbound)","GE:64K\n10GE:1M\n(outbound)","GE:64K\n10GE:1M\n(outbound)","GE:64K\n10GE:1M\n(outbound)"]
[null,"流量整形","traffic shaping","-","-","-","-","-"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","GE:64K\n10GE:1M\n(inbound)","GE:64K\n10GE:1M\n(inbound)","GE:64K\n10GE:1M\n(inbound)","GE:64K\n10GE:1M\n(inbound)","GE:64K\n10GE:1M\n(inbound)"]
[null,"Flash大小","Flash","16M","16M","16M","16M","16M"]
[null,"SDRAM大小","SDRAM","128M","128M","128M","128M","128M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","3M","3M","3M","3M","3M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","9K","9K","9K","9K","9K"]
[null,"堆叠方式","Stack mode","IRF","IRF","IRF","IRF","IRF"]
[null,"堆叠带宽","Stack bandwidth","96G(Bidirection and loop network)","96G(Bidirection and loop network)","96G(Bidirection and loop network)","96G(Bidirection and loop network)","96G(Bidirection and loop network)"]
[null,"堆叠台数","MAX Stack num",8,8,8,8,8]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1k","1k","1k","1k","1k"]
[null,"动态ARP数目","Dynamic ARP num","8K","8K","8K","8K","8K"]
[null,"RARP","RARP","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y","Y","Y","Y"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","-","-","-","-","-"]
[null,"LACP短超时","LACP short-time","-","-","-","-","-"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y"]
[null,"Smart Link","Smart Link","Y","Y","Y","Y","Y"]
[null,"Smart Link multi-instances","Smart Link multi-instances","-","-","-","-","-",{"$nulls":7},"-"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","Y","Y","Y","Y","Y"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y"]
[null,"组播VLAN","MVR","Y","Y","Y","Y","Y"]
[null,"组播VLAN+","MVR+","-","-","-","-","-"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-"]
[null,"RRPP","RRPP","-","-","-","-","-"]
[null,"RRPP multi-instances","RRPP multi-instances","-","-","-","-","-"]
[null,"EAD","support users by 5 rules","all:480\nper GE max:20","all:480\nper GE max:20","all:960\nper GE max:20","all:960\nper GE max:20","all:480\nper GE max:20"]
[null,null,"support users by 10 rules","all:240\nper GE max:10","all:240\nper GE max:10","all:480\nper GE max:10","all:480\nper GE max:10","all:240\nper GE max:10"]
[null,null,"support users by 20 rules","all:120\nper GE max:5","all:120\nper GE max:5","all:240\nper GE max:5","all:240\nper GE max:5","all:120\nper GE max:5"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","12s","12s","12s","12s","12s"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","270s","270s","520s","520s","270s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","100s","100s",190,190,"100s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y","Y","Y","Y"]
[null,"NTP","NTP","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","-","-","-","-","-"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-","-","-","-"]
[null,"IP+PORT绑定个数","IP+PORT Binding","-","-","-","-","-"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","-","-","-","-","-"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","50  per GE\n","50  per GE\n","50  per GE\n","50  per GE\n","50 per GE\n"]
[null,"可聚合端口数目","MAX num in one link group","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE"]
[null,"端口聚合组数","Link group num",32,32,32,32,32]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","-","-","-","-","-"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:1","N:1","N:1","N:1","N:1"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:1","N:1","N:1","N:1","N:1"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y"]
[null,"storm constrain","storm constrain","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)","Y (1% or pps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","-","-","-","-","-"]
[null,"基于IP子网VLAN","IP subnet based vlan","-","-","-","-","-"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)"]
[null,"Voice Vlan","Voice Vlan","Y","Y","Y","Y","Y"]
[null,"SuperVLAN","SuperVLAN","-","-","-","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","-","-","-","-","-"]
["IP路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","-","-","-","-","-"]
[null,"RIPV1/2","RIPV1/2","Y","Y","Y","Y","Y"]
[null,"OSPF V2","OSPF V2","Y","Y","Y","Y","Y"]
[null,"IS-IS","IS-IS","-","-","-","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","Y","Y","Y","Y","Y"]
[null,"静态路由","Static routing",256,256,256,256,256]
[null,"支持second ip数目","MAX num of second ip ","6 second ip per inteface vlan ,\n128 totally","6 second ip per inteface vlan ,\n128 totally","6 second ip per inteface vlan ,\n128 totally","6 second ip per inteface vlan ,\n128 totally","6 second ip per inteface vlan ,\n128 totally"]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y","Y","Y","Y"]
[null,"VRRP","VRRP","Y(32 instance)","Y(32 instance)","Y(32 instance)","Y(32 instance)","Y(32 instance)"]
[null,"VRRPE","VRRPE","-","-","-","-","-"]
[null,"BFD","BFD","-","-","-","-","-"]
[null,"ECMP(等值路由)","ECMP","Y(512*4)","Y(512*4)","Y(512*4)","Y(512*4)","Y(512*4)"]
[null,"策略路由","Policy based routing","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","-","-","-","-","-"]
["MCE组播","MCE MULTICAST","MCE MULTICAST","-","-","-","-","-"]
["MPLS","MPLS","MPLS","-","-","-","-","-"]
["组播VPN","multicast vpn","multicast vpn","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","-","-","-","-","-"]
[null,"NetStream/NetFlow/IPFIX","NetStream/NetFlow","-","-","-","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","Y","Y","Y","Y","Y"]
[null,"IGMP V3","IGMP V3","-","-","-","-","-"]
[null,"PIM-SM","PIM-SM","Y","Y","Y","Y","Y"]
[null,"PIM-SSM","PIM-SSM","-","-","-","-","-"]
[null,"PIM-DM","PIM-DM","Y","Y","Y","Y","Y"]
[null,"双向PIM","BI-PIM","-","-","-","-","-"]
[null,"MSDP","MSDP","Y","Y","Y","Y","Y"]
["OAM","802.1AG","802.1AG","-","-","-","-","-"]
[null,"802.3AH","802.3AH","-","-","-","-","-"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","-","-","-","-","-"]
[null,"SMON","SMON","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）"]
[null,"IMC","IMC","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","Y","Y","Y","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","-","-","-","-","-"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","-","-","-","-","-"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","-","-","-","-","-"]
[null,"ISSU","ISSU","-","-","-","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","-","-","-","-","-"]
[null,"triple authentication","triple authentication","-","-","-","-","-"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","-","-","-","-","-"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","-","-","-","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","-","-","-","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ",256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","1K","1K","1K","1K","1K"]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","-","-","-","-","-"]
[null,"HQ+WRR","HQ+WRR","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","-","-","-","-","-"]
[null,"ACL logging","ACL logging","-","-","-","-","-"]
[null,"RED","RED","-","-","-","-","-"]
[null,"WRED","WRED","-","-","-","-","-"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","-","-","-","-","-"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","-","-","-","-","-"]
[null,"IPV6 ND数目","IPV6 ND NUM","-","-","-","-","-"]
[null,"ICMPV6","ICMPV6","-","-","-","-","-"]
[null,"TRACEROUTE V6","TRACEROUTE V6","-","-","-","-","-"]
[null,"TELNET V6","TELNET V6","-","-","-","-","-"]
[null,"ND","ND","-","-","-","-","-"]
[null,"ND snooping","ND snooping","-","-","-","-","-"]
[null,"ND proxy","ND proxy","-","-","-","-","-"]
[null,"ND detection","ND detection","-","-","-","-","-"]
[null,"PMTU","PMTU","-","-","-","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","-","-","-","-","-"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","-","-","-","-","-"]
[null,"RIPng","RIPng","-","-","-","-","-"]
[null,"OSPF V3","OSPF V3","-","-","-","-","-"]
[null,"IS-IS V6","IS-IS V6","-","-","-","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-","-","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","-","-","-","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","-","-","-","-","-"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 双向PIM","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","-","-","-","-","-"]
[null,"DHCP V6 snooping","DHCP V6 snooping","-","-","-","-","-"]
[null,"DHCP V6 client","DHCP V6 client","-","-","-","-","-"]
[null,"DHCP V6 relay","DHCP V6 relay","-","-","-","-","-"]
[null,"DHCP V6 server","DHCP V6 server","-","-","-","-","-"]
[null,"IPv6 端口绑定","IPv6 source guard","-","-","-","-","-"]
[null,"BFD v6","BFD v6","-","-","-","-","-"]
[null,"IPV6 TUNNEL","IPV6 TUNNEL","-","-","-","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","Y","-","Y","-"]
[null,"总功率","Total Power","-","DC:370W\nAC:300W","-","DC: 740W\nAC: 300W","-"]
[null,"单端口最大功率","Power Per Port","-","15.4W","-","15.4W","-"]
[null,"802.3af","802.3af","-","Y","-","Y","-"]
[null,"供电模式","Mode of  Voltage Supply","-","data wire mode","-","data wire mode","-"]
["物理特性\nphysical feature","电源","Power Supply","AC&DC","AC&DC","AC&DC","AC&DC","AC&DC"]
[null,"功耗(W)","Power Consummtion",170,"DC:540\nAC:560",230,"DC:970\nAC:640",170]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",580.0642165,"DC:1842.556923\nAC:1910.799772",784.7927635000001,"DC:3309.7781765\nAC:2183.771168",580.0642165]
[null,"湿度","Humidity","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%"]
[null,"温度","Temperature","0~45","0~45","0~45","0~45","0~45"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","<7.5kg","<7.5kg","<8kg","<8kg","<7.5kg"]
[null,"风扇","Fan NUM",2,2,4,3,3]
[null,"噪音（LPA，DB）\n（GR-63-CORE(issue 2)）","Noise","50.8(low speed)\n52.6(high speed)\n","51.8(low speed)\n54.1(high speed)\n","51.4(low speed)\n54.5(high speed)\n","52.2(low speed)\n53(high speed)\n","54.6(low speed)\n57.4(high speed)\n"]
[null,"MTBF(年)","MTBF",24.21,24.21,21.3,21.3,23.89]
[null,"MTTR(小时)","MTTR",2,2,2,2,2]
[null,"RPS电源","RPS","Y（RPS800-A /RPS1000-A3）","Y（RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS1000-A3）","Y（RPS800-A/RPS1000-A3）"]
[null,"热插拔","Hot-Swap","extend board support","extend board support","extend board support","extend board support","extend board support"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-"]
[null,"外形尺寸（宽x高x深）","Size (WxHxd)","440×43.6×420mm","440×43.6×420mm","440×43.6×420mm","440×43.6×420mm","440×43.6×420mm"]

{"sheet":"S5120SI&E500&5120EI&5120HI","index":7,"n_rows":312,"n_cols":24,"rows_kept":312,"cut":false,"hidden":false,"merged":[[286,0,311,0],[36,0,88,0],[188,0,189,0],[124,0,144,0],[218,0,232,0],[154,0,164,0],[165,0,170,0],[89,0,110,0],[111,0,115,0],[116,0,123,0],[233,0,244,0],[280,0,285,0],[171,0,172,0],[173,0,174,0],[175,0,178,0],[204,0,217,0],[245,0,279,0],[2,0,5,0],[181,0,187,0],[190,0,203,0],[145,0,147,0],[6,0,35,0],[179,0,180,0],[148,0,152,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]"," S5120-9P-SI"," S5120-20P-SI"," S5120-28P-SI"," S5120-52P-SI"," S5120-9P-PWR-SI","S5120-28P-PWR-SI"," S5120-9P-HPWR-SI","S5120-28P-HPWR-SI","E528"," E552"," S5120-28P-LI"," S5120-52P-LI","S5120-24P-EI","S5120-48P-EI","S5120-28C-EI","S5120-52C-EI","S5120-28C-PWR-EI","S5120-28C-PWR-EI(POE+)","S5120-52C-PWR-EI","S5120-52C-PWR-EI(POE+)","S5120-52SC-HI\n"]
[null,"CPL","CPL","A5120-8G SI \nJG308A","A5120-16G SI \nJE073A","A5120-24G SI \nJE074A ","A5120-48G SI \nJE072A ","A5120-8G-PPoE+ SI \nJG310A ","A5120-24G-PPoE+ SI \nJG092A","A5120-8G-PoE+ SI \nJG309A","A5120-24G-PoE+ SI \nJG091A","-","-","-","-","A5120-24G EI \nJE066A","A5120-48G EI\nJE067A"," A5120-24G EI Switch with 2 Interface Slots\nJE068A","A5120-48G EI Switch with 2 Interface Slots\nJE069A","-","A5120-24G-PoE+ EI Switch with 2 Interface Slots\nJG236A","-","A5120-48G-PoE+ EI Switch with 2 Interface Slots\nJG237A","A5120AF-48G HI Switch w 1 intf Slot\nJG319A"]
["端口\nport","固定配置","Fixed configration","8*10/100/1000TX+1*SFP","16*10/100/1000TX+4*SFP","24*10/100/1000TX+4*SFP","48*10/100/1000TX+4*SFP","8*10/100/1000TX+1*SFP","24*10/100/1000TX+4*SFP","8*10/100/1000TX+1*SFP","24*10/100/1000TX+4*SFP","24*10/100/1000TX+4*SFP","48*10/100/1000TX+4*SFP","24*10/100/1000TX+4*SFP","48*10/100/1000TX+4*SFP","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","48*10/100/1000TX（2combo）+ 2*  1G/10G BASE-X SFP PLUS"]
[null,"配置口","config interface","console ","console ","console ","console","console ","console ","console ","console ","console ","console","console ","console","console ","console ","console","console ","console ","console ","console ","console ","console , outband mangement interface"]
[null,"可选配置（插槽数*端口个数）","optional configration(slot× interface board)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","1*1XFP(SR/LR/ER)\n1*2XFP(SR/LR/ER)\n1*2SFP+\n1*2SFP\n1*2CX4;  \n"]
[null,"100FX SFP支持","100FX SFP支持","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","18G","40G","56G","104G","18G","56G","18G","56G","56G","104G","56G","104G","48G","96G","128G","176G","128G","128G","176G","176G","176Gbps"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","13.4Mpps","29.8Mpps","41.7Mpps","77.4Mpps","13.4Mpps","41.7Mpps","13.4Mpps","41.7Mpps","41.7Mpps","77.4Mpps","41.7Mpps","77.4Mpps","35.7Mpps","71.4Mpps","95.23M","130.94M","95.23M","95.23M","130.94M","130.94M","130.95Mpps"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3"]
[null,"三层路由转发机制","L3 route forwarding mode","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1k"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","32k"]
[null,"路由接口数","Max VLAN interface",8,8,8,8,8,8,8,8,8,8,1,1,8,8,8,8,8,8,8,8,32]
[null,"IP V4路由条数","IP V4 routing num",32,32,32,32,32,32,32,32,32,32,32,32,32,32,32,32,32,32,32,32,128]
[null,"整机支持L2组播数","Multicast L2  entries","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","1000\n","1000\n","1000\n","1000\n","1000\n","1000\n","1000\n","1000\n","IPV4：1000\nIPV6：1000\n"]
[null,"整机支持L3组播数","Multicast L3  entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"跨VLAN组播复制能力","Multicast entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",4,4,4,4,4,4,4,4,4,4,4,4,8,8,8,8,8,8,8,8,8]
[null,"ACL流分类数","ACL Num",960,960,960,960,960,960,960,960,960,1920,8,8,"1k","2k","1k","2k","1k","1k","2k","2k",3072]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM"]
[null,"ACL 方向","ACL direction"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress","Ingress:3072  Egress:1024"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM",960,960,960,960,960,960,960,960,960,1920,8,8,"1k","2k","1k","2k","1k","1k","2k","2k","Ingress:3072  Egress:1024"]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","8kbps(outbound)"]
[null,"流量整形","traffic shaping","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate","-","-","-","-","-","-","-","-","-","-","-","-","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","8kbps（inbound）"]
[null,"Flash大小","Flash","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","16M","16M","16M","16M","32M","32M","32M","32M","128M"]
[null,"SDRAM大小","SDRAM","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","256M","256M","256M","256M","512M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","0.5M","0.5M","0.5M","1M","0.5M","0.5M","0.5M","0.5M","0.5M","1M","0.5M","1M","2M","4M","2M","4M","2M","2M","4M","4M","4M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","10k","10k","10k","10k","10k","10k","10k","10k","10k","10k","10k","10k","9K","9K","9K","9K","9K","9K","9K","9K","9k"]
[null,"堆叠方式","Stack mode","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF-lite","IRF-lite","-","-","IRF ","IRF ","IRF ","IRF ","IRF ","IRF ","IRF"]
[null,"堆叠带宽","Stack bandwidth","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","40G","40G","-","-","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 to 4\nStack bandwidth:\n80G(96G)"]
[null,"堆叠台数","MAX Stack num",4,4,4,4,4,4,4,4,4,4,4,4,"-","-",4,4,4,4,4,4,9]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num",64,64,64,64,64,64,64,64,64,64,64,64,512,512,512,512,512,512,512,512,512]
[null,"动态ARP数目","Dynamic ARP num",256,256,256,256,256,256,256,256,256,256,256,256,"1k","1k","1k","1k","1k","1k","1k","1k","1k"]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1p","802.1p","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x","802.1x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(1  instances)","Y(1  instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"PVST+","PVST+","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)"]
[null,"TC snooping","TC snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link","Smart Link","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","-","-","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","-","-","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM snooping","PIM snooping","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN","MVR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN+","MVR+","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RRPP multi-instances","RRPP multi-instances","-","-","-","-","-","-","-","-","-","-","-","-","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )"]
[null,"EAD","support users by 5 rules","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y",140,280,140,280,140,140,280,280,"Per port :128\nall:256(双芯片)/128(单芯片)\n"]
[null,null,"support users by 10 rules","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y",70,140,70,140,70,70,140,140,"Per port:64\nall:128(双芯片)/64(单芯片)\n"]
[null,null,"support users by 20 rules","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y",35,70,35,70,35,35,70,70,"Per port:32\nall:64(双芯片)/32(单芯片)\n"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n\n\n","10s\n\n","10s\n\n","10s\n\n\n","10s\n\n\n","5s\n"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","30s\n\n\n","60s\n\n\n","30s\n\n","60s\n\n\n","30s\n\n","30s\n\n","60s\n\n\n","60s\n\n\n","18s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","20s\n\n\n","33s\n\n\n","20s\n\n","33s\n\n\n","20s\n\n","20s\n\n","33s\n\n\n","33s\n\n\n","17s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-"]
[null,"IP+PORT绑定个数","IP+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","Y acl规格限制","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","Y(500)"]
[null,"可聚合端口数目","MAX num in one link group","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/8*10GE"]
[null,"端口聚合组数","Link group num",4,10,14,26,4,14,4,14,14,26,14,26,12,24,"single device:14\nirf:128","single device:26\nirf:128","single device:14\nirf:128","single device:14\nirf:128","single device:26\nirf:128","single device:26\nirf:128",128]
[null,"restore port default config","restore port default config","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单链路检测","DLDP","-","-","-","-","-","-","-","-","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"流镜像","Traffic Mirroring","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","-","-","-","-","-","-","-","-","-","-","-","-","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","storm constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)"]
[null,"基于IP子网VLAN","IP subnet based vlan","-","-","-","-","-","-","-","-","-","-","-","-","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)"]
[null,"基于协议类型VLAN","Protocal based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)"]
[null,"Voice Vlan","Voice Vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SuperVLAN","SuperVLAN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["IP路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPV1/2","RIPV1/2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V2","OSPF V2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS","IS-IS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"静态路由","Static routing","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y",32,32,32,32,32,32,32,32,128]
[null,"支持second ip数目","MAX num of second ip ","-","-","-","-","-","-","-","-","-","-","-","-",4,4,4,4,4,4,4,4,4]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP","VRRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRPE","VRRPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BFD","BFD","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Routed ports","Routed ports","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-"]
[null,"ECMP(等值路由)","ECMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"策略路由","Policy based routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS","MPLS label number","MPLS label number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS label depth","MPLS label depth","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MPLS interface number","MPLS interface number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"static LSP number","static LSP number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"等价LSP","等价LSP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP local peer number","LDP local peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"LDP remote peer number","LDP remote peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls TE","mpls TE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp ping","mpls lsp ping","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VPN number","VPN number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"CE number per VPN","CE number per VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["MPLS L3VPN","VRF number","VRF number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"interface number per VRF","interface number per VRF","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["VPLS","VSI number","VSI number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NetStream/NetFlow/IPFIX","NetStream/NetFlow","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3","IGMP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SM","PIM-SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SSM","PIM-SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"PIM-DM","PIM-DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"双向PIM","BI-PIM",null,null,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MSDP","MSDP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["OAM","802.1AG","802.1AG","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3AH","802.3AH","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","shutdown-interval"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","-","-","-","-","-","-","-","-","Y"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ISSU","ISSU","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自动节能","port auto power down","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-"]
[null,"triple authentication","triple authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HWTACACS","TACACS+","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"PORTAL认证用户数","portal  USERS",512,512,512,512,512,512,512,512,512,512,512,512,"-","-","-","-","-","-","-","-",1000]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+WRR","SP+WRR","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SDWRR","SDWRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WDRR","WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL logging","ACL logging","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 64"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM",480,480,480,480,480,480,480,480,480,480,8,8,"1k","2k","1k","2k","1k","1k","2k","2k","Ingress:3072  Egress:1024"]
[null,"IPV6 ND数目","IPV6 ND NUM",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,500]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND proxy","ND proxy","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SAVI","SAVI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PMTU","PMTU","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","RIPng","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"OSPF V3","OSPF V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS V6","IS-IS V6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 relay","DHCP V6 relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 server","DHCP V6 server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD v6","BFD v6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"6VPE","6VPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-"]
[null,"是否支持中功率POE","POE+","-","-","-","-","-","-","Y","Y","-","-","-","-","-","-","-","-","-","Y","-","Y","-"]
[null,"总功率","Total Power","-","-","-","-","MIN:\nAC：10W\nMAX:\nAC：95W(65W for poe)","MIN:\nAC：25W\nMAX:\nAC：255W(170W for poe)","MIN:\nAC：19W\nMAX:\nAC：230W(180W for poe)","MIN:\nDC：27.5W\nAC：45.6W\nMAX:\nDC：832W(740W for poe)\nAC：528W(370W for poe)","-","-","-","-","-","-","-","-","MIN:55W\nMAX:580W(210W for system，370W for poe)","MIN:65W\nMAX:585W(215W for system，370W for poe)","MIN:78W\nMAX:\nAC:646W(276W for system，370W for poe)\nRPS:916W(176W for system，740W for poe)","MIN:90W\nMAX:\nAC:550W(281W for system，370W for poe)\nRPS:920W(181W for system，740W for poe)","-"]
[null,"单端口最大功率","Power Per Port","-","-","-","-","15.4W","15.4W","30W","30W","-","-","-","-","-","-","-","-","15.4W","30W","15.4W","30W","-"]
[null,"802.3af","802.3af","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","Data wire mode","-","-","-","-","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","Data wire mode","-"]
["物理特性\nphysical feature","电源","Power Supply","AC","AC","AC","AC","AC","AC","AC","AC/RPS","AC","AC","AC","AC",{"$nulls":8},"AC/DC(48V)BAK 1+1 Dual-hot-pluggable"]
[null,"功耗(W)","Power Consummtion",14.4,22.4,31.5,59.8,"MIN:\nAC：10W\nMAX:\nAC：95W(65W for poe)","MIN:\nAC：25W\nMAX:\nAC：255W(170W for poe)","MIN:\nAC：19W\nMAX:\nAC：230W(180W for poe)","MIN:\nDC：27.5W\nAC：45.6W\nMAX:\nDC：832W(740W for poe)\nAC：528W(370W for poe)",31.5,59.8,31.5,59.8,"MIN:35W\nMAX:62W","MIN:54W\nMAX:110W","MIN:36W\nMAX:103W","MIN:55W\nMAX:145W","MIN:55W\nMAX:\nAC:580W(210W for system，370W for poe)\nDC:486W(116W for system，370W for poe)","MIN:65W\nMAX:\nAC:585W(215W for system，370W for poe)\nDC:491W(121W for system，370W for poe)","MIN:78W\nMAX:\nAC:646W(276W for system，370W for poe)\nRPS:916W(176W for system，740W for poe)","MIN:90W\nMAX:\nAC:651W(281W for system，370W for poe)\nRPS:921W(181W for system，740W for poe)\nRPS供电：740W（其中编号为1～24的以太网口的PoE供电总功率为370W；编号为25～48的以太网口的PoE供电总功率为370W）",145]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",49.13485128000001,76.43199088,107.482487175,204.04611851,"MIN:34.1214245\n\nMAX:324.15353275","MIN:85.30356125\n\nMAX:870.09632475","MIN:64.83070655\n\nMAX:784.7927635","MIN:\nDC：93.833917375\nAC：155.59369572\nMAX:\nDC：2838.9025184\nAC：1801.6112136",107.482487175,204.04611851,107.482487175,204.04611851,"MIN:119.42498575\nMAX:211.5528319","MIN:184.2556923\nMAX:375.3356695","MIN:122.8371282\nMAX:351.45067235","MIN:187.66783475\nMAX:494.76065525","MIN:187.6678348\nMAX:\nAC:1979.042621\nRPS:1658.301231","MIN:221.7892593\nMAX:\nAC:1996.103333\nRPS:1675.361943","MIN:266.1471111\nMAX:\nAC:3238.123185\nRPS:3125.522484","MIN:307.0928205\nMAX:\nAC:2221.304735\nRPS:3142.583196",494.76065525]
[null,"电源模块","Power Supply module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","150W AC, 150W DC\n"]
[null,"电源功率","power rating\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","AC: min：68W；max：145W\nDC: min：57.6W；max：126W\n"]
[null,"电源负载均衡","power load-sharing\n","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","No, hot-standby\n"]
[null,"PDU电缆","PDU cable\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"湿度","Humidity","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－95%"]
[null,"温度","Temperature","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45"," -5~50℃"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","≤3kg","≤3kg","≤3kg","≤5kg","≤3kg","≤7kg","≤3kg","≤7kg","≤3kg","≤5kg","≤3kg","≤5kg","<4.5kg","<5kg","<4.5kg","<5kg","<7kg","<7kg","<7.5kg","<7.5kg","<8.2kg "]
[null,"风扇","Fan NUM",0,1,1,1,0,1,0,1,1,1,1,1,4,4,4,4,4,4,4,4,"Dual-hot-pluggable one Fan tray with two fans\n"]
[null,"风向\n","Airflow direction\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back",{"$nulls":8},"Front-to-Back: power->port\nBack-to-Front port->power\n"]
[null,"风向反转","Ariflow reverse\n","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":8},"Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. \n"]
[null,"风向控制","Airflow detection\n","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":8},"detect airflow direction via software\n"]
[null,"缺省风向","Default Airflow\n","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":8},"front-to-back power->port\n"]
[null,"风扇速率可调","Fan Speed adjustment\n","-","-","-","2 level adjustment\n","-","2 level adjustment\n","-","2 level adjustment\n","-","2 level adjustment\n","-","2 level adjustment\n",{"$nulls":8},"8 level adjustment\n"]
[null,"安装方式","Installation\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n",{"$nulls":8},"rack mount\n"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise","-","43.8dB(high speed)","44.4dB(high speed)","42.2dB(low speed)/50.0dB(high speed)","-","44.4dB(high speed)","39.4B/48.6B","44.4dB(high speed)","44.4dB(high speed)","42.2dB(low speed)/50.0dB(high speed)","44.4dB(high speed)","42.2dB(low speed)/50.0dB(high speed)","42.6(low speed)\n49.7(high speed)","41.3(low speed)\n50.1(high speed)","42.6(low speed)\n49.7(high speed)","41.3(low speed)\n50.1(high speed)","48.1(low speed)\n51.1(high speed)","48.1(low speed)\n51.1(high speed)","49.5(low speed)\n54.1(high speed)","49.5(low speed)\n54.1(high speed)","51.6/66.2"]
[null,"MTBF(年)","MTBF",77,77,73.6,54.5,70.8,50.5,58.4,48.6,73.6,54.5,73.6,54.5,"54.42","44.82","46.62","39.43","42.50","42.50","33.56","33.56",53.65]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,2,2,2,2,1,1,1,1,1,1,1,1,1]
[null,"RPS电源","RPS","-","-","-","-","-","-","-","RPS 1000","-","-","-","-","Y（RP8500-A）","Y（RP8500-A）","Y（RP8500-A）","Y（RP8500-A）","Y（RPS1000-A3）","Y（RPS1000-A3）","Y（RPS1000-A3）","Y（RPS1000-A3）","-"]
[null,"热插拔","Hot-Swap","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","210×43.6×210 （mm3）","440×43.6×160 （mm3）","440×43.6×160 （mm3）","440×43.6×260 （mm3）","300×260×43.6（mm3）","440×43.6×420 （mm3）","300×260×43.6（mm3）","440×43.6×420 （mm3）","440×43.6×160 （mm3）","440×43.6×260 （mm3）","440×43.6×160 （mm3）","440×43.6×260 （mm3）","440×300×43.6 mm","440×300×43.6 mm","440×300×43.6 mm","440×300×43.6 mm","440×420×43.6 mm","440×420×43.6 mm","440×420×43.6 mm","440×420×43.6 mm","440×420 ×43.6"]

{"sheet":"S5500SI","index":8,"n_rows":312,"n_cols":256,"rows_kept":312,"cut":false,"hidden":false,"merged":[[2,0,5,0],[6,0,35,0],[233,0,244,0],[89,0,110,0],[111,0,115,0],[116,0,123,0],[181,0,187,0],[204,0,217,0],[165,0,170,0],[171,0,172,0],[245,0,279,0],[280,0,285,0],[173,0,174,0],[175,0,178,0],[286,0,311,0],[36,0,88,0],[179,0,180,0],[188,0,189,0],[218,0,232,0],[124,0,144,0],[154,0,164,0],[148,0,152,0],[190,0,203,0],[145,0,147,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","H3C S5500-28C-SI","H3C S5500-52C-SI","H3C S5500-28C-PWR-SI","H3C S5500-28C-PWR-SI(POE+)","H3C S5500-52C-PWR-SI","H3C S5500-52C-PWR-SI(POE+)","H3C S5500-20TP-SI","H3C 5500-24P-SI","H3C 5500-48P-SI"]
[null,"CPL","CPL","A5500-24G SI Switch with 2 Interface Slots\nJD369A","A5500-48G SI Switch with 2 Interface Slots\nJD370A","-","A5500-24G-PoE+ SI Switch with 2 Interface Slots\nJG238A","-","A5500-48G-PoE+ SI Switch with 2 Interface Slots\nJG239A","-","-","-"]
["端口\nport","固定配置","Fixed configration","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","12*10/100/1000TX+8* SFP","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)"]
[null,"配置口","config interface","console ","console ","console","console","console ","console ","console ","console ","console "]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","-","-","-"]
[null,"100FX SFP支持","100FX SFP","-","-","-","-","-","-","-","-","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","128G","176G","128G","128G","176G","176G","40G","48G","96G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","95.23M","130.94M","95.23M","95.23M","130.94M","130.94M","29.76M","35.71M",71.42]
[null,"转发时延(64byte/us)","Latency(64byte/us)","GE:<5\n10GE:<3","GE:<5\n","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n","GE:<5\n","GE:<5\n"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1k","1k","1k","1k","1k","1k","1k","1k","1k"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K"]
[null,"路由接口数","Max VLAN interface",64,64,64,64,64,64,64,64,64]
[null,"IP V4路由条数","IP V4 routing num","up to 512","up to 512","up to 512","up to 512","up to 512","up to 512","up to 512","up to 512","up to 512"]
[null,"整机支持L2组播数","Multicast L2  entries","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n"]
[null,"整机支持L3组播数","Multicast L3  entries","-","-","-","-","-","-","-","-","-"]
[null,"跨VLAN组播复制能力","Multicast entries","-","-","-","-","-","-","-","-","-"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8,8,8,8,8,8,8,8]
[null,"ACL流分类数","ACL Num","1k","2k","1k","1k","2k","2k","1k","1k","2k"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM"]
[null,"ACL 方向","ACL direction"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","1k","2k","1k","1k","2k","2k","1k","1k","2k"]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)"]
[null,"流量整形","traffic shaping","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）"]
[null,"Flash大小","Flash","16M","16M","16M","16M","16M","16M","32M","16M","16M"]
[null,"SDRAM大小","SDRAM","128M","128M","128M","128M","128M","128M","256M","128M","128M"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","2M","4M","2M","2M","4M","4M","2M","2M","4M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","9K","9K","9K","9K","9K","9K","9K","9K","9K"]
[null,"堆叠方式","Stack mode","IRF","IRF","IRF","IRF","IRF","IRF","IRF lite","IRF lite","IRF lite"]
[null,"堆叠带宽","Stack bandwidth","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","40G","40G","40G"]
[null,"堆叠台数","MAX Stack num",4,4,4,4,4,4,16,16,16]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up to 2k","up to 2k","up to 2k","up to 2k","up to 2k","up to 2k","up to 2k","up to 2k","up to 2k"]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"PVST+","PVST+","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)"]
[null,"TC snooping","TC snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"Smart Link","Smart Link","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","-","-","-","-","-","-","-","-","-"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM snooping","PIM snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN","MVR","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN+","MVR+","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RRPP multi-instances","RRPP multi-instances","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )"]
[null,"EAD","support users by 5 rules",140,280,140,140,280,280,140,140,280]
[null,null,"support users by 10 rules",70,140,70,70,140,140,70,70,140]
[null,null,"support users by 20 rules",35,70,35,35,70,70,35,35,70]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n\n","10s\n\n\n","10s\n\n\n","10s\n\n\n","10s\n\n\n","10s\n\n\n"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","30s\n\n\n","60s\n\n\n","30s\n\n","30s\n\n","60s\n\n\n","60s\n\n\n","10s\n\n\n","30s\n\n\n","60s\n\n\n"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","20s\n\n\n","33s\n\n\n","20s\n\n","20s\n\n","33s\n\n\n","33s\n\n\n","20s\n\n\n","20s\n\n\n","33s\n\n\n"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","Y","-","-","-","-","-","-","-","-"]
[null,"IP+PORT绑定个数","IP+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500"]
[null,"可聚合端口数目","MAX num in one link group","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE","8GE","8GE"]
[null,"端口聚合组数","Link group num","14\nirf:128","26\nirf:128","14\nirf:128","14\nirf:128","26\nirf:128","26\nirf:128",10,12,24]
[null,"restore port default config","restore port default config","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","storm constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)"]
[null,"Voice Vlan","Voice Vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SuperVLAN","SuperVLAN","-","-","-","-","-","-","-","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPV1/2","RIPV1/2","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V2","OSPF V2","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS","IS-IS","-","-","-","-","-","-","-","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","-","-","-","-","-","-","-","-","-"]
[null,"静态路由","Static routing",64,64,64,64,64,64,64,64,64]
[null,"支持second ip数目","MAX num of second ip ",4,4,4,4,4,4,4,4,4]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP","VRRP","-","-","-","-","-","-","-","-","-"]
[null,"VRRPE","VRRPE","-","-","-","-","-","-","-","-","-"]
[null,"BFD","BFD","-","-","-","-","-","-","-","-","-"]
[null,"Routed ports","Routed ports","-","-","-","-","-","-","-","-","-"]
[null,"ECMP(等值路由)","ECMP","-","-","-","-","-","-","-","-","-"]
[null,"策略路由","Policy based routing","-","-","-","-","-","-","-","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","-","-","-","-","-","-","-","-","-"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-","-","-","-",null,"-","-"]
["MPLS","MPLS label number","MPLS label number","-","-","-","-","-","-","-","-","-"]
[null,"MPLS label depth","MPLS label depth","-","-","-","-","-","-","-","-","-"]
[null,"MPLS interface number","MPLS interface number","-","-","-","-","-","-","-","-","-"]
[null,"static LSP number","static LSP number","-","-","-","-","-","-","-","-","-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-","-","-","-","-","-","-","-"]
[null,"等价LSP","等价LSP","-","-","-","-","-","-","-","-","-"]
[null,"LDP local peer number","LDP local peer number","-","-","-","-","-","-","-","-","-"]
[null,"LDP remote peer number","LDP remote peer number","-","-","-","-","-","-","-","-","-"]
[null,"mpls TE","mpls TE","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-","-","-","-","-","-","-","-"]
[null,"mpls lsp ping","mpls lsp ping","-","-","-","-","-","-","-","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-","-","-","-","-","-","-","-"]
[null,"VPN number","VPN number","-","-","-","-","-","-","-","-","-"]
[null,"CE number per VPN","CE number per VPN","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-","-","-","-","-","-","-","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-","-","-","-","-","-","-","-"]
["MPLS L3VPN","VRF number","VRF number","-","-","-","-","-","-","-","-","-"]
[null,"interface number per VRF","interface number per VRF","-","-","-","-","-","-","-","-","-"]
["VPLS","VSI number","VSI number","-","-","-","-","-","-","-","-","-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-","-","-","-","-","-","-","-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-","-","-","-","-","-","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-","-","-","-","-","-","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-","-","-","-","-","-","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-","-","-","-","-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NetStream/NetFlow/IPFIX","NetStream/NetFlow","-","-","-","-","-","-","-","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","-","-","-","-","-","-","-","-","-"]
[null,"IGMP V3","IGMP V3","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SM","PIM-SM","-","-","-","-","-","-","-","-","-"]
[null,"PIM-SSM","PIM-SSM","-","-","-","-","-","-","-","-","-"]
[null,"PIM-DM","PIM-DM","-","-","-","-","-","-","-","-","-"]
[null,"双向PIM","BI-PIM","-","-","-","-","-","-","-","-","-"]
[null,"MSDP","MSDP","-","-","-","-","-","-","-","-","-"]
["OAM","802.1AG","802.1AG","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3AH","802.3AH","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","-","-","-","-","-","-","-","-","-"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","-","-","-","-","-","-","-","-","-"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ISSU","ISSU","-","-","-","-","-","-","-","-","-"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自动节能","port auto power down","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"triple authentication","triple authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-","-","-","-","-","-","-","-"]
[null,"portal双机热备","portal hotbackup","-","-","-","-","-","-","-","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ",256,256,256,256,256,256,256,256,256]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"PORTAL认证用户数","portal  USERS","-","-","-","-","-","-","-","-","-"]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","-","-","-","-","-","-","-","-","-"]
[null,"SP+WRR","SP+WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-","-","-","-","-","-","-","-"]
[null,"SDWRR","SDWRR","-","-","-","-","-","-","-","-","-"]
[null,"WDRR","WDRR","-","-","-","-","-","-","-","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-","-","-","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL logging","ACL logging","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","-","-","-","-","-","-","-","-","-"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 256","up to 256","up to 256","up to 256","up to 256","up to 256","up to 256","up to 256","up to 256"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","1k","2k","1k","1k","2k","2k","1k","1k","2k"]
[null,"IPV6 ND数目","IPV6 ND NUM","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","Y","Y","Y","Y","Y","Y",{"$nulls":159},"SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6","SSH2 V6"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","Y","Y","Y","Y","Y","Y",{"$nulls":159},"SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6","SFTP V6"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND proxy","ND proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SAVI","SAVI","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PMTU","PMTU","-","-","-","-","-","-","-","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","RIPng","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V3","OSPF V3","-","-","-","-","-","-","-","-","-"]
[null,"IS-IS V6","IS-IS V6","-","-","-","-","-","-","-","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","-","-","-","-","-","-","-","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","-","-","-","-","-","-","-","-","-"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","-","-","-","-","-","-","-","-"]
[null,"VRRP V3","VRRP V3","-","-","-","-","-","-","-","-","-"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 relay","DHCP V6 relay","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 server","DHCP V6 server","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD v6","BFD v6","-","-","-","-","-","-","-","-","-"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","-","-","-","-","-","-","-","-","-"]
[null,"6VPE","6VPE","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","Y","Y","Y","Y","-","-","-"]
[null,"是否支持中功率POE","POE+","-","-","-","Y","-","Y","-","-","-"]
[null,"总功率","Total Power","-","-","AC:\n580W (370W for poe)\nDC(RPS):\n486W (370W for poe)","AC:\n585W (370W for poe)\nDC(RPS):\n491W (370W for poe)","AC:\n646W (370W for poe)\nDC(RPS):\n916W (740W fow poe)","AC:\n651W (370W for poe)\nDC(RPS):\n921W (740W fow poe)\nRPS供电：740W（其中编号为1～24的以太网口的PoE供电总功率为370W；编号为25～48的以太网口的PoE供电总功率为370W）","-","-","-"]
[null,"单端口最大功率","Power Per Port","-","-","15.4W","30W","15.4W","30W","-","-","-"]
[null,"802.3af","802.3af","-","-","Y","Y","Y","Y","-","-","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-","Data wire mode","Data wire mode","Data wire mode","Data wire mode","-","-","-"]
["物理特性\nphysical feature","电源","Power Supply","AC/DC","AC/DC","AC/DC","AC/DC","AC/DC","AC/DC","AC+AC bakup","AC","AC"]
[null,"功耗(W)","Power Consummtion",80,120,"AC:\n580W (370W for poe)\nDC(RPS):\n486W (370W for poe)","AC:\n585W (370W for poe)\nDC(RPS):\n491W (370W for poe)","AC:\n646W (370W for poe)\nDC(RPS):\n916W (740W fow poe)","AC:\n651W (370W for poe)\nDC(RPS):\n921W (740W fow poe)",65,80,120]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",272.971396,409.45709400000004,"AC: \n1552.52481475\nDC(RPS):\n1552.52481475","AC: \n1996.103333\nDC(RPS):\n1675.361943","AC: \n1706.071225\nDC(RPS)：\n2968.5639315\n","AC: \n2221.304735\nDC(RPS)：\n3139.171054\n",221.78925925000001,272.971396,409.45709400000004]
[null,"电源模块","Power Supply module","-","-","-","-","-","-","-","-","-"]
[null,"电源功率","power rating\n","-","-","-","-","-","-","-","-","-"]
[null,"电源负载均衡","power load-sharing\n","-","-","-","-","-","-","-","-","-"]
[null,"PDU电缆","PDU cable\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"湿度","Humidity","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%"]
[null,"温度","Temperature","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","<4.5kg","<5kg","<7kg","<7kg","<7.5kg","<7.5kg","<6kg","<4.5kg","<5kg"]
[null,"风扇","Fan NUM",4,4,4,4,4,4,4,4,4]
[null,"风向\n","Airflow direction\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back"]
[null,"风向反转","Ariflow reverse\n","-","-","-","-","-","-","-","-","-"]
[null,"风向控制","Airflow detection\n","-","-","-","-","-","-","-","-","-"]
[null,"缺省风向","Default Airflow\n","-","-","-","-","-","-","-","-","-"]
[null,"风扇速率可调","Fan Speed adjustment\n","2 level","2 level","2 level","2 level","2 level","2 level","2 level","2 level","2 level"]
[null,"安装方式","Installation\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise","42.6(low speed)\n49.7(high speed)","41.3(low speed)\n50.1(high speed)","48.1(low speed)\n51.1(high speed)","48.1(low speed)\n51.1(high speed)","49.5(low speed)\n54.1(high speed)","49.5(low speed)\n54.1(high speed)","45.3(low speed)\n50.4(high speed)","42.6(low speed)\n49.7(high speed)","41.3(low speed)\n50.1(high speed)"]
[null,"MTBF(年)","MTBF","20.1/23.0(XFP/CX4)","13.6/14.9(XFP/CX4)","19.8/21.9(XFP/CX4)","19.8/21.9(XFP/CX4)","13.4/14.1(XFP/CX4)","13.4/14.1(XFP/CX4)","33.9(XFP/CX4)","20.1/23.0(XFP/CX4)","13.6/14.9(XFP/CX4)"]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,2]
[null,"RPS电源","RPS","Y（RPS800-A）","Y（RPS800-A）","Y（RPS1000-A3）","Y（RPS1000-A3）","Y（RPS1000-A3）","Y（RPS1000-A3）","-","-","-"]
[null,"热插拔","Hot-Swap","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440×43.6×300","440×43.6×420","440×43.6×300","440×43.6×300","440×43.6×420","440×43.6×420","440×43.6×360","440×43.6×300","440×43.6×420"]

{"sheet":"S5500EI&5500HI","index":9,"n_rows":312,"n_cols":13,"rows_kept":312,"cut":false,"hidden":false,"merged":[[280,0,285,0],[286,0,311,0],[171,0,172,0],[173,0,174,0],[175,0,178,0],[204,0,217,0],[245,0,279,0],[2,0,5,0],[6,0,35,0],[233,0,244,0],[89,0,110,0],[111,0,115,0],[145,0,147,0],[36,0,88,0],[116,0,123,0],[181,0,187,0],[190,0,203,0],[124,0,144,0],[154,0,164,0],[165,0,170,0],[148,0,152,0],[218,0,232,0],[179,0,180,0],[188,0,189,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","H3C S5500-28C-EI","H3C S5500-28C-EI-DC","H3C S5500-52C-EI","H3C S5500-28F-EI","H3C S5500-28C-PWR-EI","H3C S5500-28C-PWR-EI(POE+)","H3C S5500-52C-PWR-EI","H3C S5500-52C-PWR-EI(POE+)","S5500-24C-HI\n","S5500-58C-HI\n"]
[null,"CPL","CPL","A5500-24G EI Switch with 2 Interface Slots\nJD377A","-","HP A5500-48G EI Switch with 2 Interface SlotsJD375A","A5500-24G-SFP EI Switch with 2 Interface Slots\nJD374A","-","A5500-24G-PoE+ EI Switch with 2 Interface Slots\nJG241A","-","A5500-48G-PoE+ EI Switch with 2 Interface Slots\nJG240A","A5500-24G-4SFP HI Switch with 2 interface Slots\nJG311A","A5500-48G-4SFP HI Switch with 2 interface Slots\nJG312A"]
["端口\nport","固定配置","Fixed configration","24 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *1000M SFP ( 8 comb)","24 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24*10/100/1000TX+4*SFP+ 2* 1G/10G SFP PLUS","48*10/100/1000TX+4*SFP+ 2*  1G/10G SFP PLUS"]
[null,"配置口","config interface","console ","console ","console","console ","console ","console ","console ","console ","console , outband mangement interface","console , outband mangement interface"]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4;  \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4;\ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4;\ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2SFP\n2*2CX4\n1*8 SFP (ONLY SLOT1 SUPPORT)\n1*8 10/100/10000Base-T(ONLY SLOT1 SUPPORT\n","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2SFP\n2*2CX4;  \n1*8 SFP \n1*8 10/100/10000Base-T"]
[null,"100FX SFP支持","100FX  suppport","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","128G","128G","176G","128G","128G","128G","176G","176G","176Gbps","224Gbps"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","95.23M","95.23M","130.94M","95.23M","95.23M","95.23M","130.94M","130.94M","130.9Mpps","166.6Mpps"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1K","1K","1K","1K","1K","1K","1K","1K","1k","1k"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","32k","32k"]
[null,"路由接口数","Max VLAN interface","1K","1K","1K","1K","1K","1K","1K","1K","1k","1k"]
[null,"IP V4路由条数","IP V4 routing num","up to 12K","up to 12K","up to 12K","up to 12K","up to 12K","up to 12K","up to 12K","up to 12K","12k","12k"]
[null,"整机支持L2组播数","Multicast L2  entries","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n"]
[null,"整机支持L3组播数","Multicast L3  entries","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n"]
[null,"跨VLAN组播复制能力","Multicast entries","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K","4K","4K","4K","4K","4k"]
[null,"QOS转发队列数","QOS forward queue Num",8,8,8,8,8,8,8,8,8,8]
[null,"ACL流分类数","ACL Num","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:6k\nEgress:\n832","Ingress:3072  Egress:512","Ingress:6144  Egress:1024"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM"]
[null,"ACL 方向","ACL direction","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:6k\nEgress:\n832","Ingress:3072  Egress:512","Ingress:6144 Egress:1024"]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","64kbps(outbound)","64kbps( outbound)","64kbps(outbound)","64kbps(outbound)","64kbps( outbound)","64kbps( outbound)","64kbps(outbound)","64kbps(outbound)","8kbps(outbound)","8kbps(outbound)"]
[null,"流量整形","traffic shaping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)"]
[null,"Flash大小","Flash","32M","32M","32M","32M","32M","32M","32M","32M","512M","512M"]
[null,"SDRAM大小","SDRAM","256M","256M","256M","256M","256M","256M","256M","256M","1G","1G"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","2M","2M","4M","2M","2M","2M","4M","4M","3M","6M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","9K","9K","9K","9K","9K","9K","9K","9K","12k","12k"]
[null,"堆叠方式","Stack mode","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF"]
[null,"堆叠带宽","Stack bandwidth","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 to 6\nStack bandwidth:120G(144G)\n","stackable port number:2 to 6\nStack bandwidth:120G(144G)\n"]
[null,"堆叠台数","MAX Stack num",9,9,9,9,9,9,9,9,9,9]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 16K","up tp 16K"]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)"]
[null,"PVST+","PVST+","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)"]
[null,"TC snooping","TC snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link","Smart Link","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(48 groups)","Y(48 groups)"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM snooping ","PIM snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN","MVR","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)"]
[null,"组播VLAN+","MVR+","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RRPP multi-instances","RRPP multi-instances","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(16 instances )","Y(16 instances )"]
[null,"EAD","support users by 5 rules","per port :307\nall:307","per port :307\nall:307","per port :614\nall:614","per port :307\nall:307","per port :307\nall:307","per port :307\nall:307","per port :614\nall:614","per port :614\nall:614","per port :307\nall:307(34C)","per port :307\nall:614(58C)"]
[null,null,"support users by 10 rules","per port :153\nall:153","per port :153\nall:153","per port :307\nall:307","per port :153\nall:153","per port :153\nall:153","per port :153\nall:153","per port :307\nall:307","per port :307\nall:307","per port :153\nall:153(34C)","per port :153\nall:306(58C)"]
[null,null,"support users by 20 rules","per port :76\nall:76","per port :76\nall:76","per port :153\nall:153","per port :76\nall:76","per port :76\nall:76","per port :76\nall:76","per port :153\nall:153","per port :153\nall:153","per port :76\nall:76(34C)","per port :76\nall:152(58C)"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n\n\n","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n\n","10s\n","11s\n"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","40s\n\n\n","40s\n\n\n","80s\n","40s\n\n\n","40s\n\n\n","40s\n\n\n","80s\n","80s\n","31s\n","62s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","65s\n\n\n","65s\n\n\n","130s\n","65s\n\n\n","65s\n\n\n","65s\n\n\n","130s\n","130s\n","31s\n","\n62s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-","-","-","-","-","-","-","-","-"]
[null,"IP+PORT绑定个数","IP+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000"]
[null,"可聚合端口数目","MAX num in one link group","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/6*10GE","8GE/6*10GE"]
[null,"端口聚合组数","Link group num","single device:14\nirf:128","single device:14\nirf:128","single device:26\nirf:128","single device:14\nirf:128","single device:14\nirf:128","single device:14\nirf:128","single device:26\nirf:128","single device:26\nirf:128","single device:128\nirf:128","single device:128\nirf:128"]
[null,"restore port default config","restore port default config","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","storm constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps or bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps or bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps or bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(8K)","Y(8K)"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)"]
[null,"Voice Vlan","Voice Vlan","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)"]
[null,"SuperVLAN","SuperVLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","PVLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPV1/2","RIPV1/2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V2","OSPF V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IS-IS","IS-IS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","BGP4","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"静态路由","Static routing","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)"]
[null,"支持second ip数目","MAX num of second ip ",9,9,9,9,9,9,9,9,9,9]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP","VRRP","Y(64)","Y(64)","Y(64)","Y(64)","Y(64)","Y(64)","Y(64)","Y(64)","Y(255)","Y(255)"]
[null,"VRRPE","VRRPE","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD","BFD","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)"]
[null,"Routed ports","Routed ports","Y(limited version)","Y(limited version)","Y(limited version)","Y(limited version)","Y(limited version)","Y(limited version)","Y(limited version)","Y(limited version)","Y","Y"]
[null,"ECMP(等值路由)","ECMP","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)"]
[null,"策略路由","Policy based routing","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","-","-","-","-","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","-","-","-","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-"]
["MCE","VPN数量","MAX num of VPN","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(1024)","Y(1024)"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-","-",null,null,"-","-","-","-"]
["MPLS","MPLS label number","MPLS label number","-","-","-","-",null,null,"-","-",4000,4000]
[null,"MPLS label depth","MPLS label depth","-","-","-","-",null,null,"-","-","3 layer","3 layer"]
[null,"MPLS interface number","MPLS interface number","-","-","-","-",null,null,"-","-",512,512]
[null,"static LSP number","static LSP number","-","-","-","-",null,null,"-","-",256,256]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-","-","-",null,null,"-","-",512,512]
[null,"等价LSP","等价LSP","-","-","-","-",null,null,"-","-","NO","NO"]
[null,"LDP local peer number","LDP local peer number","-","-","-","-",null,null,"-","-",128,128]
[null,"LDP remote peer number","LDP remote peer number","-","-","-","-",null,null,"-","-",256,256]
[null,"mpls TE","mpls TE","-","-","-","-",null,null,"-","-","Y","Y"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-","-","-",null,null,"-","-","Y","Y"]
[null,"mpls lsp ping","mpls lsp ping","-","-","-","-",null,null,"-","-","Y","Y"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-","-","-",null,null,"-","-","connection number:4000","connection number:4000"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-","-","-",null,null,"-","-","connection number:1000","connection number:1000"]
[null,"VPN number","VPN number","-","-","-","-",null,null,"-","-",1000,1000]
[null,"CE number per VPN","CE number per VPN","-","-","-","-",null,null,"-","-",200,200]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-","-","-",null,null,"-","-","connection number:512","connection number:512"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-","-","-",null,null,"-","-","connection number:512","connection number:512"]
["MPLS L3VPN","VRF number","VRF number","-","-","-","-",null,null,"-","-",1023,1023]
[null,"interface number per VRF","interface number per VRF","-","-","-","-",null,null,"-","-",128,128]
["VPLS","VSI number","VSI number","-","-","-","-",null,null,"-","-",1024,1024]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-","-","-",null,null,"-","-",4096,4096]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-","-","-",null,null,"-","-","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-","-","-",null,null,"-","-","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-","-","-",null,null,"-","-","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-","-","-",null,null,"-","-","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)"]
[null,"NetStream/NetFlow/IPFIX","NetStream/NetFlow","-","-","-","-","-","-","-","-","Y","Y"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP V3","IGMP V3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-SM","PIM-SM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-SSM","PIM-SSM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-DM","PIM-DM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"双向PIM","BI-PIM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSDP","MSDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["OAM","802.1AG","802.1AG","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3AH","802.3AH","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","Y","Y"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","shutdown-interval","shutdown-interval"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ISSU","ISSU","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自动节能","port auto power down","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","Y","Y"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","web authentication","-","-","-","-","-","-","-","-","-","-"]
[null,"triple authentication","triple authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"portal双机热备","portal hotbackup","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ",256,256,256,256,256,256,256,256,"2k","2k"]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","1K","1K","1K","1K","1K","1K","1K","1K","2k","2K"]
[null,"PORTAL认证用户数","portal  USERS","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan: 3000\nmax: 3000\nMaxFreeRule:64","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan: 3000\nmax: 3000\nMaxFreeRule:64","per vlan: 3000\nmax: 3000\nMaxFreeRule:64","ALL:3000(58C)/1500(34C)\nPER PORT OR PER VLAN:1500","ALL:3000(58C)/1500(34C)\nPER PORT OR PER VLAN:1500"]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","WFQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+WRR","SP+WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-","-","-","-","-","-","-","-","-"]
[null,"SDWRR","SDWRR","-","-","-","-","-","-","-","-","-","-"]
[null,"WDRR","WDRR","-","-","-","-","-","-","-","-","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-","-","-","-","-","-","-","-","-"]
[null,"设备buffer可配置特性","BUFFER configurable","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL logging","ACL logging","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:6k\nEgress:\n832","Ingress:3k  Egress:512","Ingress:3k  Egress:512"]
[null,"IPV6 ND数目","IPV6 ND NUM","4k","4k","4k","4k","4k","4k","4k","4k","8k（bind 1000）","8k（（bind 1000））"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND proxy","ND proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SAVI","SAVI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PMTU","PMTU","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","RIPng","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V3","OSPF V3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IS-IS V6","IS-IS V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPV6 策略路由","IPV6 policied routing","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MLD SNOOPING","MLD SNOOPING","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)"]
[null,"IPv6 PIM DM","IPv6 PIM DM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 PIM SM","IPv6 PIM SM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP V3","VRRP V3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 relay","DHCP V6 relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 server","DHCP V6 server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv6 STATIC ROUTING)","BFD v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv7 STATIC ROUTING)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"6VPE","6VPE",{"$nulls":8},"Y","Y"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","-","-","Y","Y","Y","Y","-","-"]
[null,"是否支持中功率POE","POE+","-","-","-","-","-","Y","-","Y","-","-"]
[null,"总功率","Total Power","-","-","-","-","AC：\n575W(205W for system and 370W for poe)\nDC:\n485W(115W for system and 370W fow poe)\n","AC：\n591W(221W for system and 370W for poe)\nDC:\n492W(122W for system and 370W fow poe)\n","AC：\n640W(270W for system and 370W for POE)\nDC：\n910W (170W for system and 370W for poe)\n","AC：\n661W(291W for system and 370W for POE)\nDC：\n930W (190W for system and 740W for poe)\n740W（其中编号为1～24的以太网口的PoE供电总功率为370W；编号为25～48的以太网口的PoE供电总功率为370W）","-","-"]
[null,"单端口最大功率","Power Per Port","-","-","-","-","15.4W","30W","15.4W","30W","-","-"]
[null,"802.3af","802.3af","-","-","-","-","15.4W","30W","15.4W","30W","-","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","Data wire mode","-","-"]
["物理特性\nphysical feature","电源","Power Supply","AC&RPS(12V)","DC(48V)&RPS(12V)","AC&RPS(12V)","AC/DC(48V)+BACKUP MODEL","AC&RPS(48V)","AC&RPS(48V)","AC&RPS(48V)","AC&RPS(48V)","AC/DC(48V)BAK 1+1 Dual-hot-pluggable","AC/DC(48V)BAK 1+1 Dual-hot-pluggable"]
[null,"功耗(W)","Power Consummtion",110,105,155,115,"AC：\n575W(205W for system and 370W for poe)\nDC(RPS):\n485W(115W for system and 370W fow poe)\n","AC：\n591W(221W for system and 370W for poe)\nDC(RPS):\n492W(122W for system and 370W fow poe)\n","AC：\n640W(270W for system and 370W for POE)\nDC(RPS)：\n910W (170W for system and 740W for poe)\n","AC：\n661W(291W for system and 370W for POE)\nDC(RPS)：\n930W (190W for system and 740W for poe)\n",141,191]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",375.3356695,358.27495725,528.88207975,392.39638175000005,"AC：1961.98190875\nDC(RPS):1654.88908825","AC：2016.576188\nDC(RPS):1678.774085","AC：2183.771168\nDC(RPS):3105.0496295","AC：2255.426159\nDC(RPS):3173.292479",481.11208545,651.71920795]
[null,"电源模块","Power Supply module","-","-","-","-","-","-","-","-","150W AC, 150W DC\n","150W AC, 150W DC\n"]
[null,"电源功率","power rating\n","-","-","-","-","-","-","-","-","AC:\nmax:141W\nmin:62W\nDC:\nmin 52W\nmax 111W","AC:\nmax:191W\nmin:94W\nDC:min 79W\nmax 150W\n"]
[null,"电源负载均衡","power load-sharing\n","-","-","-","-","-","-","-","-","No, hot-standby\n","No, hot-standby\n"]
[null,"PDU电缆","PDU cable\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"湿度","Humidity","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"温度","Temperature","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0℃～50℃","0℃～50℃"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","<5kg","<5kg","<5kg","<6kg","<7.5kg","<7.5kg","<7.5kg","<7.5kg","<7.5kg ","<8.5kg "]
[null,"风扇","Fan NUM",4,4,4,4,6,6,6,6,"3 fixed fans for system\n","3 fixed fans for system\n"]
[null,"风向\n","Airflow direction\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to side","side to side"]
[null,"风向反转","Ariflow reverse\n","-","-","-","-","-","-","-","-","-","-"]
[null,"风向控制","Airflow detection\n","-","-","-","-","-","-","-","-","-","-"]
[null,"缺省风向","Default Airflow\n","-","-","-","-","-","-","-","-","-","-"]
[null,"风扇速率可调","Fan Speed adjustment\n","2 level","2 level","2 level","2 level","2 level","2 level","2 level","2 level","8 level adjustment\n","8 level adjustment\n"]
[null,"安装方式","Installation\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise","42.6/49.7","42.6/49.7","41.3/50.1","45.3/50.4","48.1/51.1","48.1/51.1","49.5/54.1","49.5/54.1","47.9，51.1","48.6，57.6"]
[null,"MTBF(年)","MTBF","25.91/22.27(CX4/XFP)","25.91/22.27(CX4/XFP)","23.45/20.43(CX4/XFP)","28.54/24.29(CX4/XFP)","26.03/22.36(CX4/XFP)",28.5,"22.16/19.44(CX4/XFP)",24.4,46.71,42.94]
[null,"MTTR(小时)","MTTR",2,2,2,2,2,2,2,2,1,1]
[null,"RPS电源","RPS","Y(RPS800-A)","Y(RPS800-A)(12V)/\n（RPS1000-A3）(DC 48V)","Y(RPS800-A)","Y（RPS1000-A3）\n","Y（RPS1000-A3）","Y（RPS1000-A3）","Y（RPS1000-A3）","Y（RPS1000-A3）","-","-"]
[null,"热插拔","Hot-Swap","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440×300×43.6","440×300×43.6","440×300×43.6","440×360×43.7","440×420×43.6","440×420×43.6","440×420×43.6","440×420×43.6","440×360×43.6","440×420 ×43.6"]

{"sheet":"S5800","index":10,"n_rows":312,"n_cols":16,"rows_kept":312,"cut":false,"hidden":false,"merged":[[245,0,279,0],[280,0,285,0],[233,0,244,0],[124,0,144,0],[165,0,170,0],[171,0,172,0],[286,0,311,0],[36,0,88,0],[218,0,232,0],[179,0,180,0],[204,0,217,0],[145,0,147,0],[154,0,164,0],[181,0,187,0],[190,0,203,0],[188,0,189,0],[2,0,5,0],[6,0,35,0],[111,0,115,0],[116,0,123,0],[173,0,174,0],[175,0,178,0],[89,0,110,0],[148,0,152,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S5800-32C","S5800-56C","S5800-32F","S5800-32C-PWR","S5800-56C-PWR ","S5800-60C-PWR"," S5800-54S","S5820X-28C","S5820X-28S","S5820X-26S","S5810-50S"," S5800-54S\n","S5820X-26S\n"]
[null,"CPL","CPL","A5800-24G \nJC100A","A5800-48G Switch w 1 Interface Slot\nJC105A","A5800-24G-SFP Switch w 1 Intf Slt\nJC103A","A5800-24G-PoE+ \nJC099A","A5800-48G-PoE+ Switch w 1 Intf Slt\nJC104A","A5800-48G-PoE+ Switch w 2 Intf Slts\nJC101A",null,"A5820X-14XG-SFP+ Switch w 2 Intf Slts\nJC106A","A5820X-24XG-SFP+ \nJC102A",null,"-","A5800AF-48G\nJG225A","A5820AF-24XG\nJG219A"]
["端口\nport","固定配置","Fixed configration","24*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\n\n\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*10/100/1000M SFP+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 4*  SFP\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 6*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","14*1/10GBASE-X SFP PLUS  + 4*10/100/1000TX\n\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*1/10GBASE-X SFP PLUS + 4*10/100/1000BASE-T\n\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*1/10GBASE-X SFP PLUS + 4*10/100/1000BASE-T\nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX + 2*100/1000 BASE-X SFP Combo + 2*10G BASE-X SFP PLUS\n\n\nAttention: \nSFP PLUS  can only support 10G sfp+. ","48*10/100/1000TX+ 6*1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*1/10GBASE-X SFP PLUS + 2*10/100/1000BASE-T\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T"]
[null,"配置口","config interface","console , usb","console , usb","console , usb, outband mangement iterface","console , usb","console , usb","console , usb","console , usb, outband mangement iterface","console , usb","console , usb, outband mangement iterface","console , usb, outband mangement iterface","console , usb, outband mangement iterface","1 console , 1 usb, 1 outband mangement interface","1 console , 1 usb, 1 outband mangement interface"]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","2* four 10GE uplink slots or 2* 16 GE uplink slots or 2* dual 10GE uplink slots+OAA slot (support IPS/FW/Anti-Virus/AC)+POE SLOT","-","2* four 10GE uplink slots or  2* dual 10GE uplink slots+OAA slot (support IPS/FW/Anti-Virus/AC)","-","-","-","-","-"]
[null,"100FX SFP支持","100FX SFP support","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","208G","256G","208G","208G","256G","284G","216G","488G","488G",null,"136G","216G","484G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","155Mpps","190Mpps","155Mpps","155Mpps","190Mpps","211Mpps","161Mpps","363Mpps","363Mpps","360Mpps","101Mpps","161Mpps","360Mpps"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","10GE:<3","10GE:<3","10GE:<3","GE:<5\n10GE:<3","\nGE:<5\n10GE:<3","10GE:<3"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K"]
[null,"路由接口数","Max VLAN interface","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K",16,"1K","1K"]
[null,"IP V4路由条数","IP V4 routing num","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 12K","up to 12K","up to 12K","up to 12k","up to 16K","up to 12K"]
[null,"整机支持L2组播数","Multicast L2  entries","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n","1K","IPV4：4K\nIPV6：4K\n","IPV4：2K\nIPV6：1K\n"]
[null,"整机支持L3组播数","Multicast L3  entries","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n","-","IPV4：4K\nIPV6：4K\n","IPV4：2K\nIPV6：1K\n"]
[null,"跨VLAN组播复制能力","Multicast entries","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN数","Vlan table","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,"ACL流分类数","ACL Num","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:6k\nEgress:\n1k","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:1.5K\nEgress:\n512","Ingress:1.5K\nEgress:\n512","Ingress:1.5K\nEgress:\n512","Ingress and Egress shared: 12K","Ingress:12k\nEgress:\n2K","Ingress:1280\nEgress:\n512"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM"]
[null,"ACL 方向","ACL direction","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:6k\nEgress:\n1k","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:1280\nEgress:\n512","Ingress:1280\nEgress:\n512","Ingress:1.5K\nEgress:\n512","Ingress and Egress shared: 12K","Ingress:12k\nEgress:\n2K","Ingress:1280\nEgress:\n512"]
[null,"VACL","ACL BASED VLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","70kbps(outbound)","8kbps(outbound)","8kbps(outbound)"]
[null,"流量整形","traffic shaping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)"]
[null,"Flash大小","Flash","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M"]
[null,"SDRAM大小","SDRAM","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M","1G","1G"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","4M","4M+4M","4M","4M","4M+4M","4M+4M","4M+4M","2M","2M","2M","24M","8M","2M"]
[null,"支持的最大帧长","MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support",10000,10000,10000,10000,10000,10000,10000,10000,10000,10000,10000,10000,10000]
[null,"堆叠方式","Stack mode","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF LITE","IRF","IRF"]
[null,"堆叠带宽","Stack bandwidth","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2\nstack bandwidth:40G","stackable port number:2 to 6\nstack bandwidth:\n:40G~120G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G"]
[null,"堆叠台数","MAX Stack num",9,9,9,9,9,9,9,9,9,9,9,9,9]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 16K","up tp 8K"]
[null,"RARP","RARP","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"802.3x","802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"LACP短超时","LACP short-time","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"802.1P","802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)"]
[null,"PVST+","PVST+","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)"]
[null,"TC snooping","TC snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BPDU DROP","BPDU DROP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"Smart Link","Smart Link","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(16 instances)","Y(32 instances)","Y(32 instances)"]
[null,"LLDP","LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","poe power allocation via lldp","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"QINQ","QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM snooping","PIM snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"组播VLAN","MVR","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)"]
[null,"组播VLAN+","MVR+","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","-","Y(mvr/mvr+)","Y(mvr/mvr+)"]
[null,"GVRP","GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","GMRP","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","MVRP","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","RRPP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"RRPP multi-instances","RRPP multi-instances","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","-","Y(24 instances，16ring)","Y(24 instances，16ring)"]
[null,"EAD","support users by 5 rules","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","per port :600\nall:860","per port :600\nall:860"]
[null,null,"support users by 10 rules","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","per port :310\nall:590","per port :310\nall:590"]
[null,null,"support users by 20 rules","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","per port :160\nall:167","per port :160\nall:167"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","10s","10s"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","30s","30s"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","40s","40s"]
[null,"SSH V1.5","SSH V1.5","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"NTP","NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IP+PORT绑定个数","IP+PORT Binding","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all: 512\nper port:512","all: 512\nper port:512","all: 512\nper port:512","all: 1k\nper port:256","all 2K，per port 2K","all: 512\nper port:512"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all: 512\nper port:512","all: 512\nper port:512","all: 512\nper port:512","all: 1k\nper port:256","all 2K，per port 2K","all: 512\nper port:512"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all: 512\nper port:512","all: 512\nper port:512","all: 512\nper port:512","all: 1k\nper port:256","all 2K，per port 2K","all: 512\nper port:512"]
[null,"可聚合端口数目","MAX num in one link group","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/2*10GE","6GE/6*10GE","8GE/8*10GE"]
[null,"端口聚合组数","Link group num","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128",25,"IRF: 128","IRF: 128"]
[null,"restore port default config","restore port default config","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"单链路检测","DLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"虚链路检测","VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"多端口自环检测","Multi-Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:1","N:4","N:4"]
[null,"流镜像","Traffic Mirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:1","N:4","N:4"]
[null,"RSPAN","RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","flow constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(4K)","Y(4K)","Y(4K)","-","Y(8K)","Y(4K)"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","-","Y(ALL:512)","Y(ALL:256)"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","-","Y(16 per port)","Y(16 per port)"]
[null,"Voice Vlan","Voice Vlan","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128)","-","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)"]
[null,"SuperVLAN","SuperVLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"Guest vlan","Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"PVLAN","PVLAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","Y","Y"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","IRDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"RIPV1/2","RIPV1/2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V2","OSPF V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IS-IS","IS-IS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"BGP4","BGP4","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"静态路由","Static routing","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(1k)","Y(4k)","Y(4k)"]
[null,"支持second ip数目","MAX num of second ip ",48,48,48,48,48,48,48,48,48,9,9,48,48]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"VRRP","VRRP","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(16)","Y(255)","Y(255)"]
[null,"VRRPE","VRRPE","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"BFD","BFD","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","-","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)"]
[null,"Routed ports","Routed ports","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"ECMP(等值路由)","ECMP","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*4)","Y(256*8)","Y(256*8)"]
[null,"策略路由","Policy based routing","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["OSM","Firewall Modul","Firewall Modul","-","-","-","-","-","Y","Y","Y","-","-","-","Y","-"]
[null," IPS Module"," IPS Module","-","-","-","-","-","Y","Y","Y","-","-","-","Y","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y","Y","Y","-","-","-","Y(ONLY SMALL CARD)","-"]
["MCE","VPN数量","MAX num of VPN","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","-","Y(1024)","Y(1024)"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-","-","-","-","-","-","Y","Y","Y","-","-","Y"]
["MPLS","MPLS label number","MPLS label number",4000,4000,4000,4000,4000,4000,4000,"-","-","-","-",4000,"-"]
[null,"MPLS label depth","MPLS label depth","3 layer","3 layer","3 layer","3 layer","3 layer","3 layer","3 layer","-","-","-","-","3 layer","-"]
[null,"MPLS interface number","MPLS interface number",512,512,512,512,512,512,512,"-","-","-","-",512,"-"]
[null,"static LSP number","static LSP number",1010,1010,1010,1010,1010,1010,1010,"-","-","-","-",1010,"-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported",4096,4096,4096,4096,4096,4096,4096,"-","-","-","-",4096,"-"]
[null,"等价LSP","等价LSP","NO","NO","NO","NO","NO","NO","NO","-","-","-","-","NO","-"]
[null,"LDP local peer number","LDP local peer number",128,128,128,128,128,128,128,"-","-","-","-",128,"-"]
[null,"LDP remote peer number","LDP remote peer number",256,256,256,256,256,256,256,"-","-","-","-",256,"-"]
[null,"mpls TE","mpls TE","Y","Y","Y","Y","Y","Y","Y","-","-",null,"-","Y"]
[null,"mpls lsp tracert","mpls lsp tracert","Y","Y","Y","Y","Y","Y","Y","-","-",null,"-","Y"]
[null,"mpls lsp ping","mpls lsp ping","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","-","-","-","-","connection number:4000","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","-","-","-","-","connection number:1000","-"]
[null,"VPN number","VPN number",1000,1000,1000,1000,1000,1000,1000,"-","-","-","-",1000,"-"]
[null,"CE number per VPN","CE number per VPN",200,200,200,200,200,200,200,"-","-","-","-",200,"-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","-","-","-","-","connection number:512","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","-","-","-","-","connection number:512","-"]
["MPLS L3VPN","VRF number","VRF number","1k","1k","1k","1k","1k","1k","1k","-","-","-","-","1k","-"]
[null,"interface number per VRF","interface number per VRF","1k","1k","1k","1k","1k","1k","1k","-","-","-","-","1k","-"]
["VPLS","VSI number","VSI number",1024,1024,1024,1024,1024,1024,1024,"-","-","-","-",1024,"-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires",4096,4096,4096,4096,4096,4096,4096,"-","-","-","-",4096,"-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn",4000,4000,4000,4000,4000,4000,4000,"-","-","-","-",4000,"-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance",4000,4000,4000,4000,4000,4000,4000,"-","-","-","-",4000,"-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn",0,0,0,0,0,0,0,"-","-","-","-",0,"-"]
[null,"全局最大的switchgroup数量","global max switchgroup number",0,0,0,0,0,0,0,"-","-","-","-",0,"-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IPFIX","IPFIX","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IGMP V3","IGMP V3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"PIM-SM","PIM-SM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"PIM-SSM","PIM-SSM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"PIM-DM","PIM-DM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"双向PIM","BI-PIM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"MSDP","MSDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
["OAM","802.1AG","802.1AG","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"802.3AH","802.3AH","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
["网管特性\nweb management","RMON1","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","RMON2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SMON","SMON","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","HGMP V2 ","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)"]
[null,"IMC","IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","BIMS","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","NCC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","shutdown-interval","shutdown-interval"]
[null,"TELNET配置","TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP配置","FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-"]
[null,"SCP","SCP","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"设备访问控制","Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","schedule job","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"ISSU","ISSU","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","-","Y","Y"]
[null,"端口自动节能","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","-","Y","Y"]
[null,"EEE","EEE","-","-","-","-","-","-","-","-","-","-","-","Y","Y"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"web authentication","web authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"triple authentication","triple authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"HWTACACS","HWTACACS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","multi-radius server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"portal双机热备","portal hotbackup","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ","2K","2K","2K","2K","2K","2K","2K","2K","2K","2K","-","2K","2K"]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","2K","2K","2K","2K","2K","2K","2K","2K","2K","2K","-","2K","2K"]
[null,"PORTAL认证用户数","portal  USERS","Y(ALL:3000\nPER PORT OR PER VLAN:3000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:3000\nPER PORT OR PER VLAN:3000)","Y(ALL:3000\nPER PORT OR PER VLAN:3000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:640\nPER PORT OR PER VLAN:640)","Y(ALL:640\nPER PORT OR PER VLAN:640)","Y(ALL:640\nPER PORT OR PER VLAN:640)","-","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:640\nPER PORT OR PER VLAN:640)"]
["QOS","SP","Strict priority","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"WFQ","WFQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SP+WRR","SP+WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-","-","-","-","-","-","-","-","-","Y","-","-"]
[null,"SDWRR","SDWRR","-","-","-","-","-","-","-","-","-","-","Y","-","-"]
[null,"WDRR","WDRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SP+WDRR","SP+WDRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"设备buffer可配置特性","BUFFER configurable","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"ACL logging","ACL logging","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"RED","RED","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","WRED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 8k","up to 8k","up to 8k","up to 8k","up to 8k","up to 8k","up to 8k","up to 6k","up to 6k","up to 6k","-","up to 8k","up to 6k"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:6k\nEgress:\n1k","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:1.5K\nEgress:\n512","Ingress:1.5K\nEgress:\n512","Ingress:1.5K\nEgress:\n512","Ingress and Egress shared: 12K","Ingress:12k\nEgress:\n2K","Ingress:1280\nEgress:\n512"]
[null,"IPV6 ND数目","IPV6 ND NUM","8k","8k","8k","8k","8k","8k","8k","4k","4k","4k","-","8k","4k"]
[null,"ICMPV6","ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SFTP V6","SFTP V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"ND","ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"ND snooping","ND snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"ND proxy","ND proxy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"ND detection","ND detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SAVI","SAVI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"PMTU","PMTU","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"RIPng","RIPng","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"OSPF V3","OSPF V3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IS-IS V6","IS-IS V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IPV6 策略路由","IPV6 policied routing","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"MLD SNOOPING","MLD SNOOPING","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","-","Y(V1/V2)","Y(V1/V2)"]
[null,"IPv6 PIM DM","IPv6 PIM DM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IPv6 PIM SM","IPv6 PIM SM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"VRRP V3","VRRP V3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DHCP V6 snooping","DHCP V6 snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DHCP V6 client","DHCP V6 client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DHCP V6 relay","DHCP V6 relay","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"DHCP V6 server","DHCP V6 server","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"BFD v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv6 STATIC ROUTING)","BFD v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv6 STATIC ROUTING)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","-","Y(128)","Y(128)"]
[null,"6VPE","6VPE","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-","-","Y(15.4W)","Y(15.4W)","Y(15.4W)","-","-","-","-","-","-","-"]
[null,"是否支持中功率POE","POE(30W PER PORT)","-","-","-","Y(30W)","Y(30W)","Y(30W)","-","-","-","-","-","-","-"]
[null,"总功率","Total Power","-","-","-","MIN:\nDC：64W\nAC：85W\nMAX:\nDC：870W(740W for poe)\nAC：598W(370W for poe)","MIN:\nDC：107W\nAC：131W\nMAX:\nDC：973W(740W for poe)\nAC：673W(370W for poe)\n","MIN:\nDC：94W\nAC：96W\nMAX:\nsingle DC:1840W(1500W for poe)\ndual DC:1840W(1500W for poe)\nsingle AC:714W(425W for poe)\ndual AC:1147W(740W for poe)","-","-","-","-","-","-","-"]
[null,"单端口最大功率","Power Per Port","-","-","-","30W","30W","30W","-","-","-","-","-","-","-"]
[null,"802.3af","802.3af","-","-","-","Y","Y","Y","-","-","-","-","-","-","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-","-","Data wire mode","Data wire mode","Data wire mode","-","-","-","-","-","-","-"]
["物理特性\nphysical feature","电源","Power Supply","AC&RPS(12V)","AC&RPS(12V)","AC/DC(48V)BAK 1+1 ","AC&RPS(52V)","AC&RPS(52V)","AC/DC(52V)BAK 1+1 ","AC/DC(52V)BAK 1+1 ","AC/DC(48V)BAK 1+1 ","AC/DC(48V)BAK 1+1 ","AC/DC(48V)BAK 1+1","AC/DC(48V)BAK 1+1 ","AC/DC(52V)BAK 1+1 Dual-hot-pluggable\n","AC/DC(48V)BAK 1+1\nDual-hot-pluggable\n"]
[null,"功耗(W)","Power Consummtion","MIN:67W\nMAX:105W","MIN:102W\nMAX:163W","MIN:\nDC:58W\nAC:67W\nMAX:\nDC:136W\nAC:146W","MIN:\nDC：64W\nAC：85W\nMAX:\nDC：870W(740W for poe)\nAC：598W(370W for poe)","MIN:\nDC：107W\nAC：131W\nMAX:\nDC：973W(740W for poe)\nAC：673W(370W for poe)\n","MIN:\nDC：94W\nAC：96W\nMAX:\nsingle DC:1840W(1500W for poe)\ndual DC:1840W(1500W for poe)\nsingle AC:714W(425W for poe)\ndual AC:1147W(740W for poe)","125W","MIN:\nAC:105\nDC:103\nMAX:\nAC:245\nDC:241","MIN:\nAC:128\nDC:124\nMAX:\nAC:185\nDC:176","178W","MIN:110\nMAX:180","125W","178W"]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr","MIN:228.61354415\nMAX:358.27495725","MIN:348.0385299\nMAX:556.17921935","MIN:\nDC:197.9042621\nAC:228.61354415\nMAX:\nDC:464.0513732\nAC:498.1727977","MIN:\nDC:218.3771168\nAC:218.3771168\nMAX:\nDC:2968.5639315\nAC:2040.4611851","MIN:\nDC:365.09924215\nAC:446.99066095\nMAX:\nDC:3320.01460385\nAC:2296.37186885","MIN:\nDC:320.7413903\nAC:327.5656752\nMAX:\nDC:6278.342108\nAC:3913.72739015",426.51780625,"MIN:\nDC:358.27495725\nAC:351.45067235\nMAX:\nDC:835.97490025\nAC:822.32633045","MIN:\nDC:436.7542336\nAC:423.1056638\nMAX:\nDC:631.24635325\nAC:600.5370712",607.3613561,"MIN:375.3356695\nMAX:614.185641",426.51780625,607.3613561]
[null,"电源模块","Power Supply module","-","-","-","-","-","-","-","-","-","-","-","650W AC, 650W DC\n","650W AC, 650W DC\n"]
[null,"电源功率","power rating\n","-","-","-","-","-","-","-","-","-","-","-","AC: 90v~264v, \nDC: -36v~ -72v\n","AC: 90v~264v, \nDC: -36v~ -72v\n"]
[null,"电源负载均衡","power load-sharing\n","-","-","-","-","-","-","-","-","-","-","-","No, hot-standby\n","No, hot-standby\n"]
[null,"PDU电缆","PDU cable\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n",null,"shipped with switch\n","shipped with switch\n",null,"shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"湿度","Humidity","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%"]
[null,"温度","Temperature","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","《6.0kg","《6.5kg","《8.5kg","《8kg","《8.5kg"," 《18kg"," 《10kg","《15kg","《9kg","《10kg","《8.1kg","<10Kg\n","<10Kg\n"]
[null,"风扇","Fan NUM","fixed fan:4 fans","fixed fan:4 fans","hot-swapping fan: 1 fan","fixed fan:6 fans","fixed fan:6 fans","hot-swapping fan box:6 fans","hot-swapping fan box:2 fans","hot-swapping fan box:6 fans","hot-swapping fan: 1 fan","hot-swapping fan: 2 fan","hot-swapping fan : 1 fan","Dual-hot-pluggable  Fan tray\n","Dual-hot-pluggable  Fan tray\n"]
[null,"风向\n","Airflow direction\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","Front-to-Back: power->port\nBack-to-Front port->power\n","Front-to-Back: power->port\nBack-to-Front port->power\n"]
[null,"风向反转","Ariflow reverse\n","-","-","-","-","-","-","-","-","-","-","-","Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. \n","Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. \n"]
[null,"风向控制","Airflow detection\n","-","-","-","-","-","-","-","-","-","-","-","detect airflow direction via software\n","detect airflow direction via software\n"]
[null,"缺省风向","Default Airflow\n","-","-","-","-","-","-","-","-","-","-","-","front-to-back power->port\n","front-to-back power->port\n"]
[null,"风扇速率可调","Fan Speed adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n"]
[null,"安装方式","Installation\n","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount\n","rack mount\n"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise","42.3dB/52.9dB","45.3dB/56.5dB","49.6dB/58.1dB","47.5dB/52.4dB","50.5dB/57.9dB","54dB/58.5dB","67.1dB","44.3dB/54.1dB","48.4dB/59.7dB","69.9db","48.1dB/58.1dB","60.4dB、67.1dB","60.1dB、69.9db"]
[null,"MTBF(年)","MTBF",39.8,35.2,"46.99(without psu)\n35.27(AC)\n35.29(DC)",35.1,27.7,"40.8(without psu)\n33.09(AC)\n33.11(DC)","59.6年","49.3(without psu)\n32.46(AC)\n32.47(DC)","36.7(without psu)\n29.20(AC)\n29.21(DC)","62.7年","AC(28.8)\nDC(29.3)\nWithout PSU(36.1)","59.6年","62.7年"]
[null,"MTTR(小时)","MTTR",2,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"RPS电源","RPS","Y(RPS800-A)","Y(RPS800-A)","Y(RPS800-A)","rps 1000","rps 1000","-","-","-","-","-","-","-","-"]
[null,"热插拔","Hot-Swap","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"是否支持POE受电","Power Supply by POE","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440×367×43.6","440×367×43.6","441×426×43.6","440×427×43.6","440×427×43.6","440×465×86.1","440×660×43.6","440×467×86","440×427×43.6","440×660×43.6","440×420×43.6","440×660×43.6","440×660×43.6"]

{"sheet":"5830","index":11,"n_rows":207,"n_cols":5,"rows_kept":207,"cut":false,"hidden":true,"merged":[[149,0,152,0],[92,0,99,0],[116,1,118,1],[126,0,127,0],[128,0,133,0],[134,0,135,0],[136,0,148,0],[153,0,163,0],[164,0,173,0],[174,0,197,0],[198,0,206,0],[100,0,122,0],[1,0,3,0],[4,0,30,0],[31,0,70,0],[71,0,86,0],[87,0,91,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S5830-52SC","S5830-106S"]
["端口\nport","固定配置","Fixed configration","48*10/100/1000Base-T + 2*1000Base-X SFP COMBO + 2*1/10GBase-R SFP Plus + 1 Slot","96*10/100/1000Base-T + 10*10GBase-R SFP Plus "]
[null,"配置口","config interface","console ","console "]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","\n2-Port SFP+ 10G Module\n","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","160G","392G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","120Mpps","294Mpps"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM"]
[null,"静态MAC个数","Static mac table",5120,5120]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 32K","up to 32K"]
[null,"路由接口数","Max VLAN interface","1k","1k"]
[null,"IPV4路由条数","IP V4 routing num","up to 12K","up to 12K"]
[null,"整机支持L2组播数","Multicast L2  entries","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n"]
[null,"整机支持L3组播数","Multicast L3  entries","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n"]
[null,"跨VLAN组播复制能力","Multicast entries","Y","Y"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","Y","Y"]
[null,"VLAN数","Vlan table","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8]
[null,"ACL流分类数","ACL Num","Ingress:upto 4k\nEgress:upto 512","FOR GE(upto):\nIngress:8k\nEgress:1k\nFOR 10GE(upto):\nIngress:2k\nEgress:512"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM"]
[null,"ACL 方向","ACL direction","Ingress and Egress\n","Ingress and Egress\n"]
[null,"VACL","ACL BASED VLAN","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","64Kbps","64Kbps"]
[null,"流量整形","traffic shaping","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","64kbps(inbound and outbound)","64kbps(inbound and outbound)"]
[null,"Flash大小","Flash","64M","64M"]
[null,"SDRAM大小","SDRAM","1G","1G"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","1G","3G"]
[null,"缺省支持的最大帧长","Default MAX frame length",1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","9K","9K"]
[null,"堆叠方式","Stack mode","IRF","IRF"]
[null,"堆叠台数","MAX Stack num",4,4]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up tp 8K","up tp 8K"]
[null,"ARP can learn multicast mac or not","ARP can learn multicast mac or not","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y"]
[null,"802.3x","802.3x","-","-"]
[null,"802.3ad","802.3ad","Y","Y"]
[null,"LACP","LACP","Y","Y"]
[null,"802.1P","802.1P","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y"]
[null,"802.1X","802.1X","Y","Y"]
[null,"PVST","PVST","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Instances:32","Instances:32"]
[null,"BPDU Tunnel","BPDU Tunnel","Y","Y"]
[null,"Smart Link","Smart Link","Y(26 groups)","Y(26 groups)"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(32 instances)","Y(32 instances)"]
[null,"LLDP","LLDP","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y"]
[null,"QINQ","QINQ","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","Y","Y"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y"]
[null,"组播VLAN","Muticast vlan","Y","Y"]
[null,"GVRP","GVRP","Y","Y"]
[null,"GMRP","GMRP","-","-"]
[null,"RRPP","RRPP","Y","Y"]
[null,"RRPP multi-instances","RRPP multi-instances","Y(32 instances )","Y(32 instances )"]
[null,"EAD","EAD","802.1x EAD only","802.1x EAD only"]
[null,"SSH V1.5","SSH V1.5","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y"]
[null,"NTP","NTP","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y"]
["端口特性\nport features","可聚合端口数目","MAX num in one link group",8,8]
[null,"端口聚合组数","Link group num",128,128]
[null,"单链路检测","DLDP","Y","Y"]
[null,"虚链路检测","VCT","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y"]
[null,"镜像组数","mirroring group num",4,4]
[null,"端口镜像","Port mirroring","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:1","N:1"]
[null,"流镜像(N:4)","Traffic Mirroring(N:4)","Y","Y"]
[null,"RSPAN","RSPAN","Y","Y"]
[null,"ERSPAN","ERSPAN","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(percent or pps or bps)","Y(percent or pps or bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y(percent or pps or bps)","Y(percent or pps or bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(percent or pps or bps)","Y(percent or pps or bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y(1K)","Y(1K)"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","Y(ALL:256)","Y(ALL:256)"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(16 per port)","Y(16 per port)"]
[null,"Voice Vlan","Voice Vlan","-","-"]
[null,"SuperVLAN","SuperVLAN","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y"]
[null,"PVLAN","PVLAN","Y","Y"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y"]
[null,"ICMP","ICMP","Y","Y"]
[null,"RIPV1/2","RIPV1/2","Y","Y"]
[null,"OSPF V2","OSPF V2","Y","Y"]
[null,"IS-IS","IS-IS","Y","Y"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y"]
[null,"BGP4","BGP4","Y","Y"]
[null,"静态路由","Static routing","Y(1k)","Y(1k)"]
[null,"支持second ip数目","MAX num of second ip ",7,7]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y"]
[null,"VRRP","VRRP","Y(128)","Y(128)"]
[null,"VRRPE","VRRPE","Y","Y"]
[null,"BFD","Maximum number of BFD sessions",128]
[null,null,"The minimum interval for transmitting BFD control packets","100ms"]
[null,null,"BFD  for IP","Y(ISIS/OSPF/OSPFV3/VRRP/VRRPV3/BGP/IPV6 BGP/ISIS/IPV6 IS-IS/STATIC ROUTING/PIM)","Y(ISIS/OSPF/OSPFV3/VRRP/VRRPV3/BGP/IPV6 BGP/ISIS/IPV6 IS-IS/STATIC ROUTING/PIM)"]
[null,"Non-stop Routing","Non-stop Routing","Y(BGP(NO IRF)/OSPF/ISIS)","Y(BGP(NO IRF)/OSPF/ISIS)"]
[null,"Routed ports","Routed ports","Y","Y"]
[null,"ECMP(等值路由)","ECMP","Y(256*8)","Y(256*8)"]
[null,"策略路由","Policy based routing","Y","Y"]
["MCE","VPN数量","MAX num of VPN","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-"]
["MPLS","MPLS","MPLS","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","Y","Y"]
[null,"IPFIX","IPFIX","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","Y","Y"]
[null,"IGMP V3","IGMP V3","Y","Y"]
[null,"PIM-SM","PIM-SM","Y","Y"]
[null,"PIM-SSM","PIM-SSM","Y","Y"]
[null,"PIM-DM","PIM-DM","Y","Y"]
[null,"MSDP","MSDP","Y","Y"]
["OAM","802.1AG","802.1AG","Y","Y"]
[null,"802.3AH","802.3AH","Y","Y"]
["网管特性\nweb management","RMON1","RMON1","Y","Y"]
[null,"RMON2","RMON2","-","-"]
[null,"SMON","SMON","-","-"]
[null,"WEB","WEB","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-"]
[null,"HGMP V2 ","HGMP V2 ","-","-"]
[null,"IMC","IMC","Y","Y"]
[null,"BIMS","BIMS","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y"]
[null,"FTP配置","FTP","Y","Y"]
[null,"设备访问控制","Device access control","Y","Y"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y"]
[null,"web authentication","web authentication","-","-"]
[null,"HWTACACS","HWTACACS","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ","1K","1K"]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","2K","2K"]
["QOS","SP","Strict priority","Y","Y"]
[null,"WRR","WRR","Y","Y"]
[null,"WFQ","WFQ","Y","Y"]
[null,"SP+WRR","SP+WRR/SP+WFQ","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-"]
[null,"SDWRR","SDWRR","-","-"]
[null,"WDRR","WDRR","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-"]
[null,"RED","RED","-","-"]
[null,"WRED","WRED","Y","Y"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 6k","up to 6k"]
[null,"IPv6 multicast table, (S,G)","IPv6 multicast table, (S,G)",1000,1000]
[null,"IPV6 ND数目","IPV6 ND NUM","4k","4k"]
[null,"ND Snooping","ND Snooping","Y","Y"]
[null,"ND detection","ND detection","Y","Y"]
[null,"ICMPV6","ICMPV6","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y"]
[null,"ND","ND","Y","Y"]
[null,"PMTU","PMTU","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y"]
[null,"RIPng","RIPng","Y","Y"]
[null,"OSPF V3","OSPF V3","Y","Y"]
[null,"IS-IS V6","IS-IS V6","Y","Y"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","Y","Y"]
[null,"IPV6 策略路由","IPV6 policied routing","Y","Y"]
[null,"MLD ","MLD ","Y","Y"]
[null,"MLD Proxy","MLD Proxy","Y","Y"]
[null,"MLD SNOOPING","MLD SNOOPING","Y(V1/V2)","Y(V1/V2)"]
[null,"VRRP V3","VRRP V3","Y","Y"]
[null,"IPV6 Multicast vlan","IPV6 Multicast vlan","5 multicast vlan,4000 subvlan","5 multicast vlan,4000 subvlan"]
[null,"DHCP V6 relay/snooping/client","DHCP V6 relay/snooping/client","Y","Y"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","Y(127)","Y(127)"]
["物理特性\nphysical feature","电源","Power Supply","650W AC OR DC","650W AC OR DC"]
[null,"功耗","Power Consummtion(w)","200W","200W"]
[null,"湿度","Humidity","5～95%","5～95%"]
[null,"温度","Temperature","0 ～45℃","0 ～45℃"]
[null,"风扇","Fan NUM","4 fans","4 fans"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise(low speed/high speed)","常温25℃下≤58dBA;  环境最高规格范围内≤65dBA","常温25℃下≤58dBA;  环境最高规格范围内≤65dBA"]
[null,"MTTR(小时)","MTTR","≤1","≤1"]
[null,"是否支持POE受电","Power Supply by POE","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440×460×43.6 mm","440*660*86 mm"]

{"sheet":"Sheet1","index":12,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[]
[null,"1.58 rrpp域规格"]
[null,"2.55si gts为y"]
[null,"3.55EI supervlan为y"]
[null,"4.5820的入方向ACL 改为1280"]
[null,"5.31EI支持triple"]

{"sheet":"5820V2&5830V2","index":13,"n_rows":312,"n_cols":5,"rows_kept":312,"cut":false,"hidden":false,"merged":[[2,0,5,0],[6,0,35,0],[36,0,88,0],[89,0,110,0],[111,0,115,0],[116,0,123,0],[124,0,144,0],[145,0,147,0],[148,0,152,0],[154,0,164,0],[165,0,170,0],[171,0,172,0],[173,0,174,0],[175,0,178,0],[179,0,180,0],[181,0,187,0],[188,0,189,0],[190,0,203,0],[204,0,217,0],[218,0,232,0],[233,0,244,0],[245,0,279,0],[280,0,285,0],[286,0,311,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S5820V2-52QF","S5830V2-24S"]
[null,"CPL","CPL","5900AF-48XG-4QSFP\nJC100A","A5800-48G Switch w 1 Interface Slot\nJC105A"]
["端口\nport","固定配置","Fixed configration","48*1/10GBase-X SFP plus+ 4*40GBase-X QSFP\n\nAttention: \n1)SFP plus  can support 10G SR, LR, LRM, 1G sfp and 1G SFP-GE-T;\n2)40G QSFP can support up to 64*10G SFP+ ports by 40G to 4*10G breakout DAC cable","24*1/10GBase-X SFP plus\n\nAttention: \n1)SFP plus  can also support 1G sfp and 1G SFP-GE-T;"]
[null,"配置口","config interface","1 console , 1 usb, 1 outband mangement interface","1 console, 1 out-of-band mangement interface"]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","-","-"]
[null,"100FX SFP支持","100FX SFP support","-","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","1.28Tbps","480Gbps"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","952Mpps","357.12Mpps"]
[null,"转发时延(64byte/us)","Latency(64byte/us)","\n10GE:<1.51us","\n10GE:<1.7us"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM"]
[null,"静态MAC个数","Static mac table","1K","1K"]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 128K","up to 128K"]
[null,"路由接口数","Max VLAN interface","1K","1K"]
[null,"IP V4路由条数","IP V4 routing num","up to 16K","up to 16K"]
[null,"整机支持L2组播数","Multicast L2  entries","-","-"]
[null,"整机支持L3组播数","Multicast L3  entries","-","-"]
[null,"跨VLAN组播复制能力","Multicast entries","-","-"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","-","-"]
[null,"VLAN数","Vlan table","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8]
[null,"ACL流分类数","ACL Num","Ingress:1k\nEgress:1K","Ingress:1k\nEgress:1K"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM"]
[null,"ACL 方向","ACL direction","Ingress and Egress","Ingress and Egress"]
[null,"IPV4 ACL NUM","IPV4 ACL NUM","Ingress:1k\nEgress:1K","Ingress:1k\nEgress:1K"]
[null,"VACL","ACL BASED VLAN","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","8kbps(outbound)","8kbps(outbound)"]
[null,"流量整形","traffic shaping","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","8kbps(inbound and outbound)","8kbps(inbound and outbound)"]
[null,"Flash大小","Flash","512M","256M"]
[null,"SDRAM大小","SDRAM","2G","2G"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","9M","9M intergated, 3.6G off-chip"]
[null,"支持的最大帧长","MAX frame length",1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support",10000,10000]
[null,"堆叠方式","Stack mode","IRF2","IRF2"]
[null,"堆叠带宽","Stack bandwidth","stackable port number:max 4*40G or 16*10G SFP+\nstack bandwidth: :320Gbps","stackable port number:max 16*10G SFP+\nstack bandwidth: :320Gbps"]
[null,"堆叠台数","MAX Stack num",4,4]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up tp 16K","up tp 16K"]
[null,"RARP","RARP","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y"]
[null,"802.3x","802.3x","Y","Y"]
[null,"802.3ad","802.3ad","Y","Y"]
[null,"LACP","LACP","Y","Y"]
[null,"LACP本地优先转发功能","LACP local forwarding first","Y","Y"]
[null,"LACP短超时","LACP short-time","Y","Y"]
[null,"802.1P","802.1P","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y"]
[null,"802.1X","802.1X","-","-"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Y(64 instances)","Y(64 instances)"]
[null,"PVST+","PVST+","-","-"]
[null,"TC snooping","TC snooping","-","-"]
[null,"BPDU DROP","BPDU DROP","-","-"]
[null,"Smart Link","Smart Link","-","-"]
[null,"Smart Link multi-instances","Smart Link multi-instances","-","-"]
[null,"LLDP","LLDP","-","-"]
[null,"LLDP-MED","LLDP-MED","-","-"]
[null,"poe power allocation via lldp","poe power allocation via lldp","-","-"]
[null,"QINQ","QINQ","-","-"]
[null,"灵活QINQ","Selective QINQ","-","-"]
[null,"VLAN MAPPING ","VLAN MAPPING ","-","-"]
[null,"IGMP Snooping","IGMP Snooping","-","-"]
[null,"IGMP Snooping Fast-leave","Fast-leave","-","-"]
[null,"IGMP Snooping Group-policy","Group-policy","-","-"]
[null,"IGMP PROXY","IGMP PROXY","-","-"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","-","-"]
[null,"PIM snooping","PIM snooping","-","-"]
[null,"组播VLAN","MVR","-","-"]
[null,"组播VLAN+","MVR+","-","-"]
[null,"GVRP","GVRP","-","-"]
[null,"GMRP","GMRP","-","-"]
[null,"MVRP","MVRP","-","-"]
[null,"RRPP","RRPP","-","-"]
[null,"RRPP multi-instances","RRPP multi-instances","-","-"]
[null,"EAD","support users by 5 rules","-","-"]
[null,null,"support users by 10 rules","-","-"]
[null,null,"support users by 20 rules","-","-"]
[null,null,"consumed time for parallel authentication of 20 users per 10 rules ","-","-"]
[null,null,"consumed time for parallel authentication of all users per 10 rules ","-","-"]
[null,null,"consumed time for parallel authentication of all users per 20 rules ","-","-"]
[null,"SSH V1.5","SSH V1.5","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","-","-"]
[null,"Dhcp relay option82","Dhcp relay option82","-","-"]
[null,"NTP","NTP","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","-","-"]
[null,"DHCP Snooping表项备份功能","DHCP Snooping item backup","-","-"]
[null,"DHCP SNOOPING","DHCP SNOOPING","-","-"]
["端口特性\nport features","IP+MAC绑定个数","IP+MAC Binding","-","-"]
[null,"IP+PORT绑定个数","IP+PORT Binding","Y","Y"]
[null,"MAC+PORT绑定个数","MAC+PORT Binding","Y","Y"]
[null,"IP+MAC+PORT绑定个数","IP+MAC+PORT Binding","Y","Y"]
[null,"可聚合端口数目","MAX num in one link group",16,16]
[null,"端口聚合组数","Link group num","IRF: 128","IRF: 128"]
[null,"restore port default config","restore port default config","-","-"]
[null,"单链路检测","DLDP","-","-"]
[null,"虚链路检测","VCT","-","-"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y"]
[null,"端口自环检测","Port loopback-detection","-","-"]
[null,"多端口自环检测","Multi-Port loopback-detection","-","-"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y"]
[null,"端口镜像","Port miirroring","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:4","N:4"]
[null,"流镜像","Traffic Mirroring","Y","Y"]
[null,"流镜像比例","Proportion of Traffic Mirroring","N:4","N:4"]
[null,"RSPAN","RSPAN","Y","Y"]
[null,"storm constrain","flow constrain","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(1% or pps bps)","Y(1% or pps bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y(1% or pps bps)","Y(1% or pps bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(1% or pps bps)","Y(1% or pps bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y"]
[null,"Sticky Mac","Sticky Mac","-","-"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","-","-"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","-","-"]
[null,"基于协议类型VLAN","Protocal based vlan","-","-"]
[null,"Voice Vlan","Voice Vlan","-","-"]
[null,"SuperVLAN","SuperVLAN","-","-"]
[null,"Guest vlan","Guest vlan","-","-"]
[null,"PVLAN","PVLAN","-","-"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y"]
[null,"ICMP","ICMP","Y","Y"]
[null,"IRDP","IRDP","-","-"]
[null,"RIPV1/2","RIPV1/2","Y","Y"]
[null,"OSPF V2","OSPF V2","Y","Y"]
[null,"IS-IS","IS-IS","-","-"]
[null,"HWPING(NQA)","HWPING(NQA)","-","-"]
[null,"BGP4","BGP4","Y","Y"]
[null,"静态路由","Static routing","Y(4k)","Y(4k)"]
[null,"支持second ip数目","MAX num of second ip ",48,48]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","-","-"]
[null,"DHCP Relay","DHCP Relay","-","-"]
[null,"DHCP Client","DHCP Client","-","-"]
[null,"DHCP Server","DHCP Server","-","-"]
[null,"VRRP","VRRP","Y(255)","Y(255)"]
[null,"VRRPE","VRRPE","Y","Y"]
[null,"BFD","BFD","-","-"]
[null,"Routed ports","Routed ports","-","-"]
[null,"ECMP(等值路由)","ECMP","Y(256*8)","Y(256*8)"]
[null,"策略路由","Policy based routing","-","-"]
["OSM","Firewall Modul","Firewall Modul","-","-"]
[null," IPS Module"," IPS Module","-","-"]
[null,"Wireless Access Controller Module","Wireless Access Controller Module","-","-"]
["MCE","VPN数量","MAX num of VPN","Y(1024)","Y(1024)"]
[null,"MCE IPV4 UNICAST","MCE IPV4 UNICAST","Y","Y"]
[null,"MCE IPV4 MULTICAST","MCE IPV4 MULTICAST","-","-"]
[null,"MCE IPV6 UNICAST","MCE IPV6 UNICAST","-","-"]
[null,"MCE IPV6 MULTICAST","MCE IPV6 MULTICAST","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","Y","-"]
["MPLS","MPLS label number","MPLS label number","-","-"]
[null,"MPLS label depth","MPLS label depth","-","-"]
[null,"MPLS interface number","MPLS interface number","-","-"]
[null,"static LSP number","static LSP number","-","-"]
[null,"Maximum number of LSPs supported","Maximum number of LSPs supported","-","-"]
[null,"等价LSP","等价LSP","-","-"]
[null,"LDP local peer number","LDP local peer number","-","-"]
[null,"LDP remote peer number","LDP remote peer number","-","-"]
[null,"mpls TE","mpls TE","-","-"]
[null,"mpls lsp tracert","mpls lsp tracert","-","-"]
[null,"mpls lsp ping","mpls lsp ping","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","mpls l2vpn(VLL):martini","-","-"]
[null,"mpls l2vpn(VLL):kompella","mpls l2vpn(VLL):kompella","-","-"]
[null,"VPN number","VPN number","-","-"]
[null,"CE number per VPN","CE number per VPN","-","-"]
[null,"mpls l2vpn(VLL):CCC","mpls l2vpn(VLL):CCC","-","-"]
[null,"mpls l2vpn(VLL):SVC","mpls l2vpn(VLL):SVC","-","-"]
["MPLS L3VPN","VRF number","VRF number","-","-"]
[null,"interface number per VRF","interface number per VRF","-","-"]
["VPLS","VSI number","VSI number","-","-"]
[null,"Number of Pseudo Wires","Number of Pseudo Wires","-","-"]
["组播VPN","每个VPN实例内支持的最大组播表项数","the max multicast number per vpn","-","-"]
[null,"公网实例内支持的最大组播表项数","the max multicast number in public network instance","-","-"]
[null,"每个VPN最大的switchgroup数量","the max switchgroup number per vpn","-","-"]
[null,"全局最大的switchgroup数量","global max switchgroup number","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","-","-"]
[null,"IPFIX","IPFIX","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","-","-"]
[null,"IGMP V3","IGMP V3","-","-"]
[null,"PIM-SM","PIM-SM","-","-"]
[null,"PIM-SSM","PIM-SSM","-","-"]
[null,"PIM-DM","PIM-DM","-","-"]
[null,"双向PIM","BI-PIM","-","-"]
[null,"MSDP","MSDP","-","-"]
["OAM","802.1AG","802.1AG","-","-"]
[null,"802.3AH","802.3AH","-","-"]
["网管特性\nweb management","RMON1","RMON1","-","-"]
[null,"RMON2","RMON2","-","-"]
[null,"SMON","SMON","-","-"]
[null,"WEB","WEB","-","-"]
[null,"HTTPS","HTTPS","-","-"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-"]
[null,"HGMP V2 ","HGMP V2 ","-","-"]
[null,"IMC","IMC","Y","Y"]
[null,"BIMS","BIMS","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","-","-"]
[null,"NCC","NCC","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y"]
[null,"FTP配置","FTP","Y","Y"]
[null,"SCP","SCP","-","-"]
[null,"零配置（DHCP auto-config）","ZERO CONFIG(DHCP AUTO CONFIG)","-","-"]
[null,"零配置（CWMP-TR069)","ZERO CONFIG(CWMP-TR069)","-","-"]
[null,"设备访问控制","Device access control","Y","Y"]
[null,"schedule job","schedule job","-","-"]
[null,"告警温度上下限可以配置","the warning upper and lower temperature","Y","Y"]
[null,"arp,bfd,lacp mad堆叠分裂检测","arp,bfd,lacp mad","Y arp lacp only","Y arp lacp only"]
[null,"ISSU","ISSU","-","-"]
[null,"端口自动恢复","port auto recovery/shutdown-interval","shutdown-interval","shutdown-interval"]
[null,"端口自动节能","port auto power down","-","-"]
[null,"EEE","EEE","-","-"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","-","-"]
[null,"web authentication","web authentication","-","-"]
[null,"triple authentication","triple authentication","-","-"]
[null,"HWTACACS","HWTACACS","-","-"]
[null,"multi-radius server","multi-radius server","-","-"]
[null,"动态VLAN下发","Dynamic VLAN ","-","-"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","-","-"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-"]
[null,"portal双机热备","portal hotbackup","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","-","-"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","-","-"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ","-","-"]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","-","-"]
[null,"PORTAL认证用户数","portal  USERS","-","-"]
["QOS","SP","Strict priority","Y","Y"]
[null,"WRR","WRR","-","-"]
[null,"WFQ","WFQ","-","-"]
[null,"SP+WRR","SP+WRR","-","-"]
[null,"SP+SDWRR","SP+SDWRR","-","-"]
[null,"SDWRR","SDWRR",null,"-"]
[null,"WDRR","WDRR","Y","Y"]
[null,"SP+WDRR","SP+WDRR","Y","Y"]
[null,"设备buffer可配置特性","BUFFER configurable","-","-"]
[null,"ACL logging","ACL logging","-","-"]
[null,"RED","RED","-","-"]
[null,"WRED","WRED","Y","Y"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 8k","up to 8k"]
[null,"IPV6 ACL NUM","IPV6 ACL NUM","Ingress:1k\nEgress:\n1k","Ingress:1k\nEgress:\n1K"]
[null,"IPV6 ND数目","IPV6 ND NUM","8k","8k"]
[null,"ICMPV6","ICMPV6","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y"]
[null,"SSH2 V6","SSH2 V6","Y","Y"]
[null,"SFTP V6","SFTP V6","-","-"]
[null,"ND","ND","Y","Y"]
[null,"ND snooping","ND snooping","-","-"]
[null,"ND proxy","ND proxy","-","-"]
[null,"ND detection","ND detection","-","-"]
[null,"SAVI","SAVI","-","-"]
[null,"PMTU","PMTU","Y","Y"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","-","-"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","-","-"]
[null,"RIPng","RIPng","-","-"]
[null,"OSPF V3","OSPF V3","Y","Y"]
[null,"IS-IS V6","IS-IS V6","-","-"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","-","-"]
[null,"IPV6 策略路由","IPV6 policied routing","-","-"]
[null,"MLD SNOOPING","MLD SNOOPING","-","-"]
[null,"IPv6 PIM DM","IPv6 PIM DM","-","Y"]
[null,"IPv6 PIM SM","IPv6 PIM SM","-","Y"]
[null,"IPv6 双向PIM","IPv6 BI-PIM","-","Y"]
[null,"IPv6 PIM SSM","IPv6 PIM SSM","-","Y"]
[null,"VRRP V3","VRRP V3","Y","Y"]
[null,"DHCP V6 snooping","DHCP V6 snooping","-","-"]
[null,"DHCP V6 client","DHCP V6 client","-","-"]
[null,"DHCP V6 relay","DHCP V6 relay","-","-"]
[null,"DHCP V6 server","DHCP V6 server","-","-"]
[null,"IPv6 端口绑定","IPv6 source guard","Y","Y"]
[null,"BFD v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv6 STATIC ROUTING)","BFD v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv6 STATIC ROUTING)","-","-"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","-","-"]
[null,"6VPE","6VPE","-","-"]
[" 远程供电特性（设备馈电）\nPower Over Ethernet  ","是否支持POE供电","POE","-","-"]
[null,"是否支持中功率POE","POE(30W PER PORT)","-","-"]
[null,"总功率","Total Power","-","-"]
[null,"单端口最大功率","Power Per Port","-","-"]
[null,"802.3af","802.3af","-","-"]
[null,"供电模式","Mode of  Voltage Supply","-","-"]
["物理特性\nphysical feature","电源","Power Supply","1+1 Dual-hot-pluggable\n","1+1 Dual-hot-pluggable\n"]
[null,"功耗(W)","Power Consummtion","Min 200w, Max 260w","Min 343w, Max 366w"]
[null,"BTU/hr (功耗*3.41214245 )","BTU/hr",887.1570370000001,1248.8441367]
[null,"电源模块","Power Supply module","650W AC, 650W DC\n","650W AC, 650W DC\n"]
[null,"电源功率","power rating\n","AC: 90v~264v, \nDC: -36v~ -72v\n","AC: 90v~264v, \nDC: -36v~ -72v\n"]
[null,"电源负载均衡","power load-sharing\n","No, hot-standby\n","No, hot-standby\n"]
[null,"PDU电缆","PDU cable\n","shipped with switch for DC cable. AC cable is localized \n","shipped with switch for DC cable. AC cable is localized \n"]
[null,"湿度","Humidity","10%－90%","10%－90%"]
[null,"温度","Temperature","0~45","0~45"]
[null,"存储温度","Storage temperature","-40～+70℃","-40～+70℃"]
[null,"存储湿度","Storage humidity ","5～95%RH，无冷凝","5～95%RH，无冷凝"]
[null,"满配重量","Full load weight","<13Kg\n","<13Kg\n"]
[null,"风扇","Fan NUM","Dual-hot-pluggable  Fan tray","Dual-hot-pluggable  Fan tray"]
[null,"风向\n","Airflow direction\n","Front-to-Back: power->port\nBack-to-Front port->power"]
[null,"风向反转","Ariflow reverse\n","Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. ","Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. "]
[null,"风向控制","Airflow detection\n","detect airflow direction via software and report warning message if the mismatch is detected","detect airflow direction via software and report warning message if the mismatch is detected"]
[null,"缺省风向","Default Airflow\n","front-to-back power->port","front-to-back power->port"]
[null,"风扇速率可调","Fan Speed adjustment\n","10 level adjustment","10 level adjustment"]
[null,"安装方式","Installation\n","rack mount","rack mount"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise","65.7dB/70.6dB","62.1dB/76.7dB"]
[null,"MTBF(年)","MTBF",27.7,23]
[null,"MTTR(小时)","MTTR",1,1]
[null,"RPS电源","RPS","-","-"]
[null,"热插拔","Hot-Swap","Y","Y"]
[null,"是否支持POE受电","Power Supply by POE","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440×660×43.6","440×660×43.6"]