{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["5830","Sheet1","Combined"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":57,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"5830","index":0,"n_rows":207,"n_cols":5,"rows_kept":207,"cut":false,"hidden":true,"merged":[[149,0,152,0],[92,0,99,0],[116,1,118,1],[126,0,127,0],[128,0,133,0],[134,0,135,0],[136,0,148,0],[153,0,163,0],[164,0,173,0],[174,0,197,0],[198,0,206,0],[100,0,122,0],[1,0,3,0],[4,0,30,0],[31,0,70,0],[71,0,86,0],[87,0,91,0]],"flags":["formulas_cached_only"]}
[null,"项目名称[中文]","Item name[english]","S5830-52SC","S5830-106S"]
["端口\nport","固定配置","Fixed configration","48*10/100/1000Base-T + 2*1000Base-X SFP COMBO + 2*1/10GBase-R SFP Plus + 1 Slot","96*10/100/1000Base-T + 10*10GBase-R SFP Plus "]
[null,"配置口","config interface","console ","console "]
[null,"可选配置（插槽数*板子类型）","optional configration(slot× interface board)","\n2-Port SFP+ 10G Module\n","-"]
["性能\nperformance","端口交换容量(bps)","Port switch capacity","160G","392G"]
[null,"转发能力(pps)(存储转发)","Forwarding performance","120Mpps","294Mpps"]
[null,"三层路由转发机制","L3 route forwarding mode","LPM","LPM"]
[null,"静态MAC个数","Static mac table",5120,5120]
[null,"MAC地址表深度(HASH 算法)","MAC address table","up to 32K","up to 32K"]
[null,"路由接口数","Max VLAN interface","1k","1k"]
[null,"IPV4路由条数","IP V4 routing num","up to 12K","up to 12K"]
[null,"整机支持L2组播数","Multicast L2  entries","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n"]
[null,"整机支持L3组播数","Multicast L3  entries","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n"]
[null,"跨VLAN组播复制能力","Multicast entries","Y","Y"]
[null,"组播是否和ARP共享资源","Does multicast share resource with ARP","Y","Y"]
[null,"VLAN数","Vlan table","4K","4K"]
[null,"QOS转发队列数","QOS forward queue Num",8,8]
[null,"ACL流分类数","ACL Num","Ingress:upto 4k\nEgress:upto 512","FOR GE(upto):\nIngress:8k\nEgress:1k\nFOR 10GE(upto):\nIngress:2k\nEgress:512"]
[null,"ACL机制说明","ACL policy description","TCAM","TCAM"]
[null,"ACL 方向","ACL direction","Ingress and Egress\n","Ingress and Egress\n"]
[null,"VACL","ACL BASED VLAN","Y","Y"]
[null,"端口限速粒度","port line-rate granularity","64Kbps","64Kbps"]
[null,"流量整形","traffic shaping","Y","Y"]
[null,"ACL 流限速粒度","ACL Traffic-limit rate granularity","64kbps(inbound and outbound)","64kbps(inbound and outbound)"]
[null,"Flash大小","Flash","64M","64M"]
[null,"SDRAM大小","SDRAM","1G","1G"]
[null,"包缓存大小(Bytes)","Memory Capacity of Packet Buffer(bytes)","1G","3G"]
[null,"缺省支持的最大帧长","Default MAX frame length",1536,1536]
[null,"Jumbo frame Support","Jumbo frame Support","9K","9K"]
[null,"堆叠方式","Stack mode","IRF","IRF"]
[null,"堆叠台数","MAX Stack num",4,4]
["二层协议\nL2 protocal","静态ARP数目","Static ARP num","1K","1K"]
[null,"动态ARP数目","Dynamic ARP num","up tp 8K","up tp 8K"]
[null,"ARP can learn multicast mac or not","ARP can learn multicast mac or not","-","-"]
[null,"ARP Proxy","ARP Proxy","Y","Y"]
[null,"802.3x","802.3x","-","-"]
[null,"802.3ad","802.3ad","Y","Y"]
[null,"LACP","LACP","Y","Y"]
[null,"802.1P","802.1P","Y","Y"]
[null,"802.1Q","802.1Q","Y","Y"]
[null,"802.1X","802.1X","Y","Y"]
[null,"PVST","PVST","Y","Y"]
[null,"STP(802.1D)","STP(802.1D)","Y","Y"]
[null,"RSTP(802.1w)","RSTP(802.1w)","Y","Y"]
[null,"MSTP(802.1s)","MSTP(802.1s)","Instances:32","Instances:32"]
[null,"BPDU Tunnel","BPDU Tunnel","Y","Y"]
[null,"Smart Link","Smart Link","Y(26 groups)","Y(26 groups)"]
[null,"Smart Link multi-instances","Smart Link multi-instances","Y(32 instances)","Y(32 instances)"]
[null,"LLDP","LLDP","Y","Y"]
[null,"LLDP-MED","LLDP-MED","Y","Y"]
[null,"QINQ","QINQ","Y","Y"]
[null,"灵活QINQ","Selective QINQ","Y","Y"]
[null,"VLAN MAPPING ","VLAN MAPPING ","Y","Y"]
[null,"IGMP Snooping","IGMP Snooping","Y","Y"]
[null,"IGMP Snooping Fast-leave","Fast-leave","Y","Y"]
[null,"IGMP Snooping Group-policy","Group-policy","Y","Y"]
[null,"IGMP PROXY","IGMP PROXY","Y","Y"]
[null,"IGMP V3 Snooping","IGMP V3 Snooping","Y","Y"]
[null,"组播VLAN","Muticast vlan","Y","Y"]
[null,"GVRP","GVRP","Y","Y"]
[null,"GMRP","GMRP","-","-"]
[null,"RRPP","RRPP","Y","Y"]
[null,"RRPP multi-instances","RRPP multi-instances","Y(32 instances )","Y(32 instances )"]
[null,"EAD","EAD","802.1x EAD only","802.1x EAD only"]
[null,"SSH V1.5","SSH V1.5","Y","Y"]
[null,"SSH V2","SSH V2","Y","Y"]
[null,"Dhcp snooping option82","Dhcp snooping option82","Y","Y"]
[null,"Dhcp relay option82","Dhcp relay option82","Y","Y"]
[null,"NTP","NTP","Y","Y"]
[null,"DHCP SNOOPING TRUST","DHCP SNOOPING TRUST","Y","Y"]
[null,"DHCP SNOOPING","DHCP SNOOPING","Y","Y"]
["端口特性\nport features","可聚合端口数目","MAX num in one link group",8,8]
[null,"端口聚合组数","Link group num",128,128]
[null,"单链路检测","DLDP","Y","Y"]
[null,"虚链路检测","VCT","Y","Y"]
[null,"端口隔离（AM)","Access manage(port isolate)","Y","Y"]
[null,"端口自环检测","Port loopback-detection","Y","Y"]
[null,"端口环回（内环外环测试）","Port loop test(inclding inner loop and outer loop)","Y","Y"]
[null,"镜像组数","mirroring group num",4,4]
[null,"端口镜像","Port mirroring","Y","Y"]
[null,"端口镜象比例","Proportion of Port Miirroring","N:1","N:1"]
[null,"流镜像(N:4)","Traffic Mirroring(N:4)","Y","Y"]
[null,"RSPAN","RSPAN","Y","Y"]
[null,"ERSPAN","ERSPAN","Y","Y"]
[null,"未知单播抑制","Unicast Suppression","Y(percent or pps or bps)","Y(percent or pps or bps)"]
[null,"多播风暴抑制","Multicast  Suppression","Y(percent or pps or bps)","Y(percent or pps or bps)"]
[null,"广播风暴抑制","Broadcast Suppression","Y(percent or pps or bps)","Y(percent or pps or bps)"]
["端口安全特性\nport security","黑洞MAC","mac black hole","Y","Y"]
[null,"Sticky Mac","Sticky Mac","Y","Y"]
[null,"Dynamic  ARP Inspection","Dynamic  ARP Inspection","Y","Y"]
[null,"IPSource Guard","IPSource Guard","Y","Y"]
[null,"端口 MAC地址个数限制","Port Max-Mac-Count","Y","Y"]
["vlan ","基于端口VLAN","Port based vlan","Y","Y"]
[null,"基于MAC VLAN","MAC based vlan","Y(1K)","Y(1K)"]
[null,"基于 IPv4 子网VLAN","IPv4 subnet based vlan","Y(ALL:256)","Y(ALL:256)"]
[null,"基于协议类型VLAN","Protocal based vlan","Y(16 per port)","Y(16 per port)"]
[null,"Voice Vlan","Voice Vlan","-","-"]
[null,"SuperVLAN","SuperVLAN","-","-"]
[null,"Guest vlan","Guest vlan","Y","Y"]
[null,"PVLAN","PVLAN","Y","Y"]
["IPV4路由协议\nip routeing protocal","IP","IP","Y","Y"]
[null,"TCP/UDP","TCP/UDP","Y","Y"]
[null,"ICMP","ICMP","Y","Y"]
[null,"RIPV1/2","RIPV1/2","Y","Y"]
[null,"OSPF V2","OSPF V2","Y","Y"]
[null,"IS-IS","IS-IS","Y","Y"]
[null,"HWPING(NQA)","HWPING(NQA)","Y","Y"]
[null,"BGP4","BGP4","Y","Y"]
[null,"静态路由","Static routing","Y(1k)","Y(1k)"]
[null,"支持second ip数目","MAX num of second ip ",7,7]
[null,"DHCP RELAY SECURITY","DHCP RELAY SECURITY","Y","Y"]
[null,"DHCP Relay","DHCP Relay","Y","Y"]
[null,"DHCP Client","DHCP Client","Y","Y"]
[null,"DHCP Server","DHCP Server","Y","Y"]
[null,"VRRP","VRRP","Y(128)","Y(128)"]
[null,"VRRPE","VRRPE","Y","Y"]
[null,"BFD","Maximum number of BFD sessions",128]
[null,null,"The minimum interval for transmitting BFD control packets","100ms"]
[null,null,"BFD  for IP","Y(ISIS/OSPF/OSPFV3/VRRP/VRRPV3/BGP/IPV6 BGP/ISIS/IPV6 IS-IS/STATIC ROUTING/PIM)","Y(ISIS/OSPF/OSPFV3/VRRP/VRRPV3/BGP/IPV6 BGP/ISIS/IPV6 IS-IS/STATIC ROUTING/PIM)"]
[null,"Non-stop Routing","Non-stop Routing","Y(BGP(NO IRF)/OSPF/ISIS)","Y(BGP(NO IRF)/OSPF/ISIS)"]
[null,"Routed ports","Routed ports","Y","Y"]
[null,"ECMP(等值路由)","ECMP","Y(256*8)","Y(256*8)"]
[null,"策略路由","Policy based routing","Y","Y"]
["MCE","VPN数量","MAX num of VPN","-","-"]
["Cut Through","Cut Through Mode","Cut Through Mode","-","-"]
["MPLS","MPLS","MPLS","-","-"]
["流量统计\ntraffic statistic","SFLOW","SFLOW","Y","Y"]
[null,"IPFIX","IPFIX","-","-"]
["三层组播协议\nL3 multicast\nprotocal","IGMP","IGMP","Y","Y"]
[null,"IGMP V3","IGMP V3","Y","Y"]
[null,"PIM-SM","PIM-SM","Y","Y"]
[null,"PIM-SSM","PIM-SSM","Y","Y"]
[null,"PIM-DM","PIM-DM","Y","Y"]
[null,"MSDP","MSDP","Y","Y"]
["OAM","802.1AG","802.1AG","Y","Y"]
[null,"802.3AH","802.3AH","Y","Y"]
["网管特性\nweb management","RMON1","RMON1","Y","Y"]
[null,"RMON2","RMON2","-","-"]
[null,"SMON","SMON","-","-"]
[null,"WEB","WEB","Y","Y"]
[null,"HTTPS","HTTPS","Y","Y"]
[null,"SNMPV1/2/3","SNMPV1/2/3","Y","Y"]
[null,"HGMP V1 SERVER","HGMP V1 SERVER","-","-"]
[null,"HGMP V1 CLINET","HGMP V1 CLINET","-","-"]
[null,"HGMP V2 ","HGMP V2 ","-","-"]
[null,"IMC","IMC","Y","Y"]
[null,"BIMS","BIMS","-","-"]
[null,"IPV6 HOST MANGEMENT","IPV6 HOST MANGEMENT","Y","Y"]
[null,"DNS CLINET ","DNS CLINET ","Y","Y"]
["设备管理\ndevice management","CLI配置","CLI","Y","Y"]
[null,"TELNET配置","TELNET","Y","Y"]
[null,"FTP配置","FTP","Y","Y"]
[null,"设备访问控制","Device access control","Y","Y"]
["接入认证\naccess authentication","集中MAC认证","Mac address  authentication","Y","Y"]
[null,"web authentication","web authentication","-","-"]
[null,"HWTACACS","HWTACACS","Y","Y"]
[null,"动态VLAN下发","Dynamic VLAN ","Y","Y"]
[null,"PEAP/EAP-TLS","PEAP/EAP-TLS","Y","Y"]
[null,"二层 PORTAL认证","L2  PORTAL authentication","-","-"]
[null,"三层 PORTAL认证","L3  PORTAL authentication","-","-"]
[null,"802.1x认证设备（远端认证）","Remote 802.1x authentication ","Y","Y"]
[null,"802.1x认证SERVER（本地认证）","Local 802.1x authentication","Y","Y"]
[null,"单端口802.1x server时支持的最大用户数","MAX 802.1x USERS Per Port ","1K","1K"]
[null,"整机802.1x server时支持的最大用户数","MAX 802.1x USERS Total","2K","2K"]
["QOS","SP","Strict priority","Y","Y"]
[null,"WRR","WRR","Y","Y"]
[null,"WFQ","WFQ","Y","Y"]
[null,"SP+WRR","SP+WRR/SP+WFQ","Y","Y"]
[null,"SP+SDWRR","SP+SDWRR","-","-"]
[null,"SDWRR","SDWRR","-","-"]
[null,"WDRR","WDRR","-","-"]
[null,"SP+WDRR","SP+WDRR","-","-"]
[null,"RED","RED","-","-"]
[null,"WRED","WRED","Y","Y"]
["IPV6 ","IPV6 单播路由数目","IPV6 unitcast routing num","up to 6k","up to 6k"]
[null,"IPv6 multicast table, (S,G)","IPv6 multicast table, (S,G)",1000,1000]
[null,"IPV6 ND数目","IPV6 ND NUM","4k","4k"]
[null,"ND Snooping","ND Snooping","Y","Y"]
[null,"ND detection","ND detection","Y","Y"]
[null,"ICMPV6","ICMPV6","Y","Y"]
[null,"TRACEROUTE V6","TRACEROUTE V6","Y","Y"]
[null,"TELNET V6","TELNET V6","Y","Y"]
[null,"ND","ND","Y","Y"]
[null,"PMTU","PMTU","-","-"]
[null,"DNS CLINET FOR IPV6","DNS CLINET FOR IPV6","Y","Y"]
[null,"SNMP FOR IPV6","SNMP FOR IPV6","Y","Y"]
[null,"RIPng","RIPng","Y","Y"]
[null,"OSPF V3","OSPF V3","Y","Y"]
[null,"IS-IS V6","IS-IS V6","Y","Y"]
[null,"BGP4+ FOR IPV6","BGP4+ FOR IPV6","Y","Y"]
[null,"IPV6 策略路由","IPV6 policied routing","Y","Y"]
[null,"MLD ","MLD ","Y","Y"]
[null,"MLD Proxy","MLD Proxy","Y","Y"]
[null,"MLD SNOOPING","MLD SNOOPING","Y(V1/V2)","Y(V1/V2)"]
[null,"VRRP V3","VRRP V3","Y","Y"]
[null,"IPV6 Multicast vlan","IPV6 Multicast vlan","5 multicast vlan,4000 subvlan","5 multicast vlan,4000 subvlan"]
[null,"DHCP V6 relay/snooping/client","DHCP V6 relay/snooping/client","Y","Y"]
[null,"IPV6 TUNNEL","\nGRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","Y(127)","Y(127)"]
["物理特性\nphysical feature","电源","Power Supply","650W AC OR DC","650W AC OR DC"]
[null,"功耗","Power Consummtion(w)","200W","200W"]
[null,"湿度","Humidity","5～95%","5～95%"]
[null,"温度","Temperature","0 ～45℃","0 ～45℃"]
[null,"风扇","Fan NUM","4 fans","4 fans"]
[null,"ISO7779标准bystander声压级噪声测试方法（Lpa，dB）(low speed/high speed)","Noise(low speed/high speed)","常温25℃下≤58dBA;  环境最高规格范围内≤65dBA","常温25℃下≤58dBA;  环境最高规格范围内≤65dBA"]
[null,"MTTR(小时)","MTTR","≤1","≤1"]
[null,"是否支持POE受电","Power Supply by POE","-","-"]
[null,"外形尺寸（宽x深x高）","Size (WxHxd)","440×460×43.6 mm","440*660*86 mm"]

{"sheet":"Sheet1","index":1,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":true,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[]
[null,"1.58 rrpp域规格"]
[null,"2.55si gts为y"]
[null,"3.55EI supervlan为y"]
[null,"4.5820的入方向ACL 改为1280"]
[null,"5.31EI支持triple"]

{"sheet":"Combined","index":2,"n_rows":312,"n_cols":79,"rows_kept":312,"cut":false,"hidden":false,"merged":[[0,2,0,3],[0,4,0,7],[0,8,0,14],[0,22,0,25],[0,26,0,30],[0,31,0,33],[0,15,0,21],[0,34,0,38],[0,39,0,42],[0,43,0,50],[0,51,0,56],[0,58,0,61],[0,62,0,66],[0,67,0,68],[0,69,0,75],[286,0,311,0],[0,76,0,78],[204,0,217,0],[218,0,232,0],[233,0,244,0],[245,0,279,0],[280,0,285,0],[173,0,174,0],[175,0,178,0],[179,0,180,0],[181,0,187,0],[188,0,189,0],[190,0,203,0],[124,0,144,0],[145,0,147,0],[148,0,152,0],[154,0,164,0],[165,0,170,0],[171,0,172,0],[2,0,5,0],[6,0,35,0],[36,0,88,0],[89,0,110,0],[111,0,115,0],[116,0,123,0]],"flags":["formulas_cached_only"]}
[null,null,"3100v2 SI -Comware",null,"3100 SI - Comware",null,null,null,"3100v2 EI - Comware",{"$nulls":6},"3100 EI - Comware",{"$nulls":6},"3600v2 SI - Comware",null,null,null,"3600 SI - Comware",{"$nulls":4},"3600v2 EI - Comware",null,null,"3600 EI - Comware",{"$nulls":4},"3610 - Comware",null,null,null,"5120 SI - Comware",{"$nulls":7},"5120 EI - Comware",{"$nulls":5},"5120 HI - Comware","5500 SI - Comware",null,null,null,"5500 EI - Comware",{"$nulls":4},"5500 HI - Comware",null,"5800 - Comware",{"$nulls":6},"5820 - Comware"]
[null,null,"3100-8 v2 SI \nJG221A","3100-16 v2 SI \nJG222A","3100-24 v2 SI \nJG223A","3100-8 SI \nJD305A","3100-16 SI \nJD306A","3100-24 SI \nJD307A","3100-8 v2 EI \nJD318B","3100-16 v2 EI \nJD319B","3100-24 v2 EI JD320B","3100-48 v2 EI \nJG315A","3100-8-PoE v2 EI \nJD311B","3100-16-PoE v2 EI \nJD312B","3100-24-PoE v2 EI \n JD313B","3100-8 EI \nJD318A","3100-16EI \nJD319A","3100-24 EI \nJD320A","3100-48 EI\nJD317A","3100-8-PoE EI\nJD311A","3100-16-PoE EI\nJD312A","3100-24-PoE EI\nJD313A","3600-24 v2 SI\nJG304A","3600-48 v2 SI\nJG305A","3600-24-PoE+ v2 SI\nJG306A","3600-48-PoE+ v2 SI\nJG307A","3600-24 SI\nJD330A","3600-24TP SI\nJD329A"," 3600-48 SI \nJD332A","3600-24-PoE SI\nJD325A"," 3600-48-PoE SI \nJD327A","3600-24 v2 EI\nJG299A","3600-48 v2 EI\nJG300A","3600-24-PoE+ v2 EI\nJG301A","3600-24 EI \nJD331A","3600-48 EI \nJD333A","3600-24-PoE EI \nJD326A","3600-48-PoE EI \nJD328A","3600-24-SFP EI\nJD334A\n","3610-24 with 4 SPF Ports\nJD336A","3610-48\nJD335A","3610-24 with 2 GigT and 2 SPF Ports\nJD337A","3610-24-SFP\nJD338A","5120-8G SI \nJG308A","5120-16G SI \nJE073A","5120-24G SI \nJE074A ","5120-48G SI \nJE072A ","5120-8G-PPoE+ SI \nJG310A ","5120-24G-PPoE+ SI \nJG092A","5120-8G-PoE+ SI \nJG309A","5120-24G-PoE+ SI \nJG091A","5120-24G EI \nJE066A","5120-48G EI\nJE067A","5120-24G EI Switch with 2 Interface Slots\nJE068A","5120-48G EI Switch with 2 Interface Slots\nJE069A","5120-24G-PoE+ EI Switch with 2 Interface Slots\nJG236A","5120-48G-PoE+ EI Switch with 2 Interface Slots\nJG237A","5120AF-48G HI Switch w 1 intf Slot\nJG319A","5500-24G SI Switch with 2 Interface Slots\nJD369A","5500-48G SI Switch with 2 Interface Slots\nJD370A","5500-24G-PoE+ SI Switch with 2 Interface Slots\nJG238A","5500-48G-PoE+ SI Switch with 2 Interface Slots\nJG239A","5500-24G EI Switch with 2 Interface Slots\nJD377A","5500-48G EI Switch with 2 Interface SlotsJD375A","5500-24G-SFP EI Switch with 2 Interface Slots\nJD374A","5500-24G-PoE+ EI Switch with 2 Interface Slots\nJG241A","5500-48G-PoE+ EI Switch with 2 Interface Slots\nJG240A","5500-24G-4SFP HI Switch with 2 interface Slots\nJG311A","5500-48G-4SFP HI Switch with 2 interface Slots\nJG312A","5800-24G \nJC100A","5800AF-48G\nJG225A","5800-48G Switch w 1 Interface Slot\nJC105A","5800-24G-SFP Switch w 1 Intf Slt\nJC103A","5800-24G-PoE+ \nJC099A","5800-48G-PoE Switch w 1 Intf Slt\nJC104A","5800-48G-PoE+ Switch w 2 Intf Slts\nJC101A","5820X-14XG-SFP+ Switch w 2 Intf Slts\nJC106A","5820X-24XG-SFP+ \nJC102A","5820AF-24XG\nJG219A"]
["port","Fixed configration","8*10/100TX+1* 1000M(COMB","16*10/100TX+2* 1000M(COMB","24*10/100TX+2* 1000M(COMB","8*10/100TX+1* 1000M(COMB)","16*10/100TX+2 *1000M(COMB)","24*10/100TX+2* 1000M(COMB)","8*10/100TX+1* 1000M(COMB","16*10/100TX+2* 1000M(COMB","24*10/100TX+2* 1000M(COMB","48 *10/100TX+2 1000TX（combo）+4*1000SFP","8*10/100TX+1* 1000M(COMB","16*10/100TX+2* 1000M(COMB","24*10/100TX+2* 1000M(COMB","8 *10/100TX+1*10/100/1000TX(COMB)","16 *10/100TX+2*10/100/1000TX(COMB)","24 *10/100TX+2*10/100/1000TX(COMB)","48 * 10/100TX","8*10/100TX+1*10/100/1000TX(COMB)","16 *10/100TX+2*10/100/1000TX(COMB)","24 *10/100TX+2*10/100/1000TX(COMB)","24 *10/100TX+2 1000TX（combo）+4*1000SFP","48 *10/100TX+2 1000TX（combo）+4*1000SFP","24 *10/100TX（PoE+）+2 1000TX（combo）+4*1000SFP","48 *10/100TX（PoE+）+2 1000TX（combo）+4*1000SFP","24 * 10/100TX","24 * 10/100TX+2*10/100/1000TX","48 * 10/100TX","24 * 10/100TX","48 * 10/100TX","24 *10/100TX+2 1000TX（combo）+4*1000SFP","48 *10/100TX+2 1000TX（combo）+4*1000SFP","24 *10/100TX（PoE+）+2 1000TX（combo）+4*1000SFP","24 * 10/100TX","48 * 10/100TX","24 * 10/100TX","48 * 10/100TX","2*10/100/1000TX","24 *10/100TX+4*1000SFP","48 *10/100TX+4*1000SFP","24 *10/100TX+2*1000SFP+2*10/100/1000T","24 100M SFP+2*1000SFP+2*10/100/1000T","8*10/100/1000TX+1*SFP","16*10/100/1000TX+4*SFP","24*10/100/1000TX+4*SFP","48*10/100/1000TX+4*SFP","8*10/100/1000TX+1*SFP","24*10/100/1000TX+4*SFP","8*10/100/1000TX+1*SFP","24*10/100/1000TX+4*SFP","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","48*10/100/1000TX（2combo）+ 2*  1G/10G BASE-X SFP PLUS","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24 *1000M SFP ( 8 comb)","24 *10/100/1000TX( 4 comb)","48 *10/100/1000TX( 4 comb)","24*10/100/1000TX+4*SFP+ 2* 1G/10G SFP PLUS","48*10/100/1000TX+4*SFP+ 2*  1G/10G SFP PLUS","24*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\n\n\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 6*1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*10/100/1000M SFP+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 4*  1/10G BASE-X SFP PLUS\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","48*10/100/1000TX+ 4*  SFP\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","14*1/10GBASE-X SFP PLUS  + 4*10/100/1000TX\n\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*1/10GBASE-X SFP PLUS + 4*10/100/1000BASE-T\n\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T","24*1/10GBASE-X SFP PLUS + 2*10/100/1000BASE-T\n\nAttention: \nSFP PLUS  can also support 1 G sfp and 1G SFP-GE-T"]
[null,"config interface","console","console","console","console ","console ","console","console","console","console","console","console","console","console","console ","console ","console","console","console ","console ","console","console","console","console","console","console ","console ","console","console ","console ","console","console","console","console","console ","console ","console","console ","console ","console ","console","console ","console ","console ","console ","console","console ","console ","console ","console ","console ","console ","console","console ","console ","console ","console , outband mangement interface","console ","console ","console","console ","console ","console","console ","console ","console ","console , outband mangement interface","console , outband mangement interface","console , usb","1 console , 1 usb, 1 outband mangement interface","console , usb","console , usb, outband mangement iterface","console , usb","console , usb","console , usb","console , usb","console , usb, outband mangement iterface","1 console , 1 usb, 1 outband mangement interface"]
[null,"optional configration(slot× interface board)","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","-","1* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/1*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI,RJ45)/2*100MSFP(2km,15km,15km 100MBIDI)","1* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","1* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","2* 1000MSFP(550m,10km, 10km 1000M BIDI)/1*100MSFP(2km,15km,15km 100M BIDI)","-","-","-","-","4* 1000MSFP(550m,10km,40km,70km,RJ45)","2* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","-","-","-","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,40km,70km,RJ45)","24*100MSFP(2KM,15KM,40KM,80KM)/2* 1000MSFP(550m,10km,40km,70km,RJ45)","4* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/4*100MSFP","4* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/4*100MSFP","2* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/2*100MSFP","2* 1000MSFP(550m,10km,30km,40km,70km,RJ45)/2*100MSFP/24*100MSFP(2km,15km,40km,80km)","-","-","-","-","-","-","-","-","-","-","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","1*1XFP(SR/LR/ER)\n1*2XFP(SR/LR/ER)\n1*2SFP+\n1*2SFP\n1*2CX4;  \n","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2CX4\n2*2SFP+","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4;  \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4;\ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2CX4; \ncomb support 1000M SFP/100M SFP","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2SFP\n2*2CX4\n1*8 SFP (ONLY SLOT1 SUPPORT)\n1*8 10/100/10000Base-T(ONLY SLOT1 SUPPORT\n","2*1XFP(SR/LR/ER)\n2*2XFP(SR/LR/ER)\n2*2SFP+\n2*2SFP\n2*2CX4;  \n1*8 SFP \n1*8 10/100/10000Base-T","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","-","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","1* four 10GE uplink slot or 1* 16 GE uplink slot or 1* dual 10GE uplink slot","2* four 10GE uplink slots or 2* 16 GE uplink slots or 2* dual 10GE uplink slots+OAA slot (support IPS/FW/Anti-Virus/AC)+POE SLOT","2* four 10GE uplink slots or  2* dual 10GE uplink slots+OAA slot (support IPS/FW/Anti-Virus/AC)","-","-"]
[null,"100FX SFP Support","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-"]
["performance","Port switch capacity","3.6G","7.2G","8.8G","3.6G","7.2G","8.8G","3.6G","7.2G","8.8G","17.6Gbps","3.6G","7.2G","8.8G","3.6G","7.2G","8.8G","17.6G","3.6G","7.2G","8.8G","12.8Gbps","17.6Gbps","12.8Gbps","17.6Gbps","12.8G","12.8G","17.6G","12.8G","17.6G","12.8Gbps","17.6Gbps","12.8Gbps","12.8G","17.6G","12.8G","17.6G","12.8G","12.8G","17.6G","12.8G","12.8G","18G","40G","56G","104G","18G","56G","18G","56G","48G","96G","128G","176G","128G","176G","176Gbps","128G","176G","128G","176G","128G","176G","128G","128G","176G","176Gbps","224Gbps","208G","216G","256G","208G","208G","256G","284G","488G","488G","484G"]
[null,"Forwarding performance","2.68M","5.36M","6.55M","2.68M","5.36M","6.55M","2.68M","5.36M","6.55M","13.1M","2.68M","5.36M","6.55M","2.68M","5.36M","6.55M","11.78M","2.68M","5.36M","6.55M","9.53M","13.1M","9.53M","13.1M","9.53M","9.53M","11.78M","9.53M","11.78M","9.53M","13.1M","9.53M","9.53M","11.78M","9.53M","11.78M","9.53M","9.53M","13.1M","9.53M","9.53M","13.4Mpps","29.8Mpps","41.7Mpps","77.4Mpps","13.4Mpps","41.7Mpps","13.4Mpps","41.7Mpps","35.7Mpps","71.4Mpps","95.23M","130.94M","95.23M","130.94M","130.95Mpps","95.23M","130.94M","95.23M","130.94M","95.23M","130.94M","95.23M","95.23M","130.94M","130.9Mpps","166.6Mpps","155Mpps","161Mpps","190Mpps","155Mpps","155Mpps","190Mpps","211Mpps","363Mpps","363Mpps","360Mpps"]
[null,"Latency(64byte/us)","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","FE:<6\nGE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","GE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","\nGE:<5\n10GE:<3","10GE:<3","10GE:<3","10GE:<3"]
[null,"L3 route forwarding mode","-","-","-","-","-","-","-","-","-","LPM","-","-","-","-","-","-","-","-","-","-","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","ACL","ACL","ACL","ACL","ACL","ACL","ACL","ACL","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM","LPM"]
[null,"Static mac table","1k","1k","1k","1K","1K","1K","1k","1k","1k","1K","1k","1k","1k","1K","1K","1K",256,"1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1k","1k","1k","1k","1k","1K","1K","1K","1K","1K","1k","1k","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"MAC address table","8k","8k","8k","up to 8K","up to 8K","up to 8K","8k","8k","8k","up to 32K","8k","8k","8k","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 32K","up to 32K","up to 32K","up to 32K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 32K","up to 32K","up to 32K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 8K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","32k","up to 16K","up to 16K","up to 16K","up to 16K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","32k","32k","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K","up to 32K"]
[null,"Max VLAN interface",1,1,1,"-","-","-",1,1,1,8,1,1,1,"-","-","-","-","-","-","-","1K","1K","1K","1K",64,64,64,64,64,"1K","1K","1K",64,64,64,64,64,256,256,256,256,8,8,8,8,8,8,8,8,8,8,8,8,8,8,32,64,64,64,64,"1K","1K","1K","1K","1K","1k","1k","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"IP V4 routing num",16,16,16,"-","-","-",16,16,16,32,16,16,16,"-","-","-","-","-","-","-","up to 2K","up to 2K","up to 2K","up to 2K","up to 1088","up to 1088","up to 1088","up to 1088","up to 1088","up to 12K","up to 12K","up to 12K","up to 8448","up to 8448","up to 8448","up to 8448","up to 8448","up to 11K","up to 11K","up to 11K","up to 11K",32,32,32,32,32,32,32,32,32,32,32,32,32,32,128,"up to 512","up to 512","up to 512","up to 512","up to 12K","up to 12K","up to 12K","up to 12K","up to 12K","12k","12k","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 16K","up to 12K","up to 12K","up to 12K"]
[null,"Multicast L2  entries",512,512,512,256,256,256,512,512,512,"IPv4：up to 1K\nIPv6：up to 512",512,512,512,512,512,512,255,512,512,512,"IPv4：up to 1K\nIPv6：up to 512","IPv4：up to 1K\nIPv6：up to 512","IPv4：up to 1K\nIPv6：up to 512","IPv4：up to 1K\nIPv6：up to 512",255,255,255,255,255,"IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000",255,255,255,255,255,"ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4：1K\nipv6：1k\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","ipv4:256\nipv6:256\n200/per port\n","1000\n","1000\n","1000\n","1000\n","1000\n","1000\n","IPV4：1000\nIPV6：1000\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：128\nIPV6：128\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n"]
[null,"Multicast L3  entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-","-","-","-","-","-","-","-","-","-","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000","IPv4：up to 2000\nIPv6：up to 1000",{"$nulls":5},"ipv4：512\nipv6：200","ipv4：512\nipv6：200","ipv4：512\nipv6：200","ipv4：512\nipv6：200","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：2000\nIPV6：1000\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：4K\nIPV6：4K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n","IPV4：2K\nIPV6：1K\n"]
[null,"Multicast entries","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y",{"$nulls":5},"Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Does multicast share resource with ARP","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","NO","NO","NO","NO","NO","Y","Y","Y","NO","NO","NO","NO","NO","NO","NO","NO","NO","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Vlan table","4k","4k","4k","4K","4K","4K","4k","4k","4k","4K","4k","4k","4k","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K","4k","4K","4K","4K","4K","4K","4K","4K","4K","4K","4K"]
[null,"QOS forward queue Num",4,4,4,4,4,4,4,4,4,8,4,4,4,4,4,4,8,4,4,4,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,4,4,4,4,4,4,4,4,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8,8]
[null,"ACL Num","-","-","-","-","-","-",256,512,1000,"Ingress:1k*2\nEgress:512*2",256,512,1000,256,512,1000,"Per 8 FE: 160\nPer GE: 100",256,512,1000,"Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Ingress:1k\nEgress:512","Ingress:2k\nEgress:1k","Ingress:1k\nEgress:512","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100",1824,1824,1824,1824,960,960,960,960,960,960,960,960,"1k","2k","1k","2k","1k","2k",3072,"1k","2k","1k","2k","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3072  Egress:512","Ingress:6144  Egress:1024","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:6k\nEgress:\n1k","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:1.5K\nEgress:\n512","Ingress:1.5K\nEgress:\n512","Ingress:1280\nEgress:\n512"]
[null,"ACL policy description","-","-","-","-","-","-","global acl","global acl","global acl","TCAM","global acl","global acl","global acl","global acl","global acl","global acl","Each block for 8FE or one GE.\nIncluding rule and mask.","global acl","global acl","global acl","TCAM","TCAM","TCAM","TCAM","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","TCAM","TCAM","TCAM","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","Each block for 8FE or one GE.\nIncluding rule and mask.","only IPv4 ACL apply on phisical port can support 2K. IPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K;\n IPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K;\n IPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","only IPv4 ACL apply on phisical port can support 2K;\nIPv6 ACL, MAC ACL,user-defined ACL,VLAN ACL can support 1K","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM","TCAM"]
[null,"ACL direction","-","-","-","-","-","-","ingress","ingress","ingress","Ingress\nand\nEgress","ingress","ingress","ingress","ingress","ingress","ingress"," only Ingress","ingress","ingress","ingress","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress","Ingress\nand\nEgress","Ingress\nand\nEgress","Ingress\nand\nEgress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress"," only Ingress","Ingress:3072  Egress:1024"," only Ingress"," only Ingress"," only Ingress"," only Ingress","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n","Ingress\nand\nEgress\n"]
[null,"IPV4 ACL NUM","-","-","-","-","-","-",256,512,1000,"Ingress:1k*2\nEgress:512*2",256,512,1000,256,512,1000,"Per 8 FE: 160\nPer GE: 100",256,512,1000,"Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Ingress:1k\nEgress:512","Ingress:1k*2\nEgress:512*2","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Ingress:1k\nEgress:512","Ingress:1k\nEgress:512","Ingress:1k\nEgress:512","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100","Per 8 FE: 160\nPer GE: 100",1824,1824,1824,1824,960,960,960,960,960,960,960,960,"1k","2k","1k","2k","1k","2k","Ingress:3072  Egress:1024","1k","2k","1k","2k","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3072  Egress:512","Ingress:6144 Egress:1024","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:6k\nEgress:\n1k","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:1280\nEgress:\n512","Ingress:1280\nEgress:\n512","Ingress:1280\nEgress:\n512"]
[null,"ACL BASED VLAN","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"port line-rate granularity","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64Kbps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","8kbps(outbound)","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64Kbps(inbound and outbound)","64K bps（inbound and outbound）","64K bps（inbound and outbound）","64K bps（inbound and outbound）","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","64Kbps(inbound and outbound)","650Kbps(outbound)","650Kbps(outbound)","650Kbps(outbound)","650Kbps(outbound)","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","8kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps(outbound)","64kbps( outbound)","64kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)","8kbps(outbound)"]
[null,"traffic shaping","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL Traffic-limit rate granularity","-","-","-","-","-","-","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","8kbps(inbound and outbound)","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","64Kbps","64K bps（ingress）","64K bps（ingress）","64K bps（ingress）","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","64Kbps","64Kbps","64Kbps","64Kbps","64Kbps","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","1Kbps(granularity) \n4Kbps(minimum )\n(inbound)","-","-","-","-","-","-","-","-","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","8kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps（inbound）","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","64kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)","8kbps(inbound and outbound)"]
[null,"Flash","16M","16M","16M","8M","8M","8M","16M","16M","16M","128M （NAND）","16M","16M","16M","8M","8M","8M","8M","8M","8M","8M","128M （NAND）","128M （NAND）","128M （NAND）","128M （NAND）","8M","8M","8M","8M","8M","128M （NAND）","128M （NAND）","128M （NAND）","16M","16M","16M","16M","16M","32M","32M","32M","32M","128M","128M","128M","128M","128M","128M","128M","128M","16M","16M","16M","16M","32M","32M","128M","16M","16M","16M","16M","32M","32M","32M","32M","32M","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M","512M"]
[null,"SDRAM","128M","128M","128M","64M","64M","64M","128M","128M","128M","256M","128M","128M","128M","64M","64M","64M","64M","64M","64M","64M","256M","256M","256M","256M","64M","64M","64M","64M","64M","256M","256M","256M","64M","64M","64M","64M","64M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","128M","256M","256M","512M","128M","128M","128M","128M","256M","256M","256M","256M","256M","1G","1G","512M","1G","512M","512M","512M","512M","512M","512M","512M","1G"]
[null,"Memory Capacity of Packet Buffer(bytes)","384KBytes","384KBytes","384KBytes","256KBytes","256KBytes","256KBytes","384KBytes","384KBytes","384KBytes","4M","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","384KBytes","32M","384KBytes","384KBytes","384KBytes","2M","4M","2M","4M","32M","32M","32M","32M","32M","2M","4M","2M","32M","32M","32M","32M","32M","32M","32M","32M","32M","0.5M","0.5M","0.5M","1M","0.5M","0.5M","0.5M","0.5M","2M","4M","2M","4M","2M","4M","4M","2M","4M","2M","4M","2M","4M","2M","2M","4M","3M","6M","4M","8M","4M+4M","4M","4M","4M+4M","4M+4M","2M","2M","2M"]
[null,"MAX frame length",1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1522,1522,1522,1522,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536,1536]
[null,"Jumbo frame Support","2k","2k","2k","-","-","-","2k","2k","2k",10000,"2k","2k","2k","2k","2k","2k","9k","2k","2k","2k",10000,10000,10000,10000,"9k","9k","9k","9k","9k",10000,10000,10000,"9k","9k","9k","9k","9k","GE:10K\nFE:1552","GE:10K\nFE:1552","GE:10K\nFE:1552","GE:10K\nFE:1552","10k","10k","10k","10k","10k","10k","10k","10k","9K","9K","9K","9K","9K","9K","9k","9K","9K","9K","9K","9K","9K","9K","9K","9K","12k","12k",10000,10000,10000,10000,10000,10000,10000,10000,10000,10000]
[null,"Stack mode","IRF-Lite","IRF-Lite","IRF-Lite","-","HGMP V2 STACK","HGMP V2 STACK","IRF-Lite","IRF-Lite","IRF-Lite","IRF2 and IRF lite","IRF-Lite","IRF-Lite","IRF-Lite","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP STACK","HGMP V2 STACK","HGMP V2 STACK","HGMP V2 STACK","IRF2","IRF2","IRF2","IRF2","IRF(only DDM DLA)","IRF(only DDM DLA)","IRF(only DDM DLA)","IRF(only DDM DLA)","IRF(only DDM DLA)","IRF2","IRF2","IRF2","IRF","IRF","IRF","IRF","IRF","IRF LITE","IRF LITE","IRF LITE","IRF LITE","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","-","-","IRF ","IRF ","IRF ","IRF ","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF","IRF"]
[null,"Stack bandwidth","2G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","-","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","stackable port number:1/2\nstack bandwidth: first 2 ports 1Gbps, last 2 ports with SFP 1Gbps ,last 2 ports with Stack Cable 2.5Gbps","2G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection )","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","2G(Bidirection)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","stackable port number:1/2\nstack bandwidth: first 2 ports 1Gbps, last 2 ports with SFP 1Gbps ,last 2 ports with Stack Cable 2.5Gbps","stackable port number:1/2\nstack bandwidth: first 2 ports 1Gbps, last 2 ports with SFP 1Gbps ,last 2 ports with Stack Cable 2.5Gbps","stackable port number:1/2\nstack bandwidth: first 2 ports 1Gbps, last 2 ports with SFP 1Gbps ,last 2 ports with Stack Cable 2.5Gbps","stackable port number:1/2\nstack bandwidth: first 2 ports 1Gbps, last 2 ports with SFP 1Gbps ,last 2 ports with Stack Cable 2.5Gbps","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","stackable port number:1/2\nstack bandwidth: first 2 ports/1Gbps, last 2 ports with SFP/1Gbps, last 2 ports with Stack Cable/2.5Gbps\nStack ports support aggregation","stackable port number:1/2\nstack bandwidth: first 2 ports/1Gbps, last 2 ports with SFP/1Gbps, last 2 ports with Stack Cable/2.5Gbps\nStack ports support aggregation","stackable port number:1/2\nstack bandwidth: first 2 ports/1Gbps, last 2 ports with SFP/1Gbps, last 2 ports with Stack Cable/2.5Gbps\nStack ports support aggregation","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G(Bidirection and loop network)","4G","4G","4G","4G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","stackable port number:2 to 8\nstack bandwidth:\n:4G~16G","-","-","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 to 4\nStack bandwidth:\n80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 /4\nStack bandwidth:\n40G(48G)\nlink agg:80G(96G)","stackable port number:2 to 6\nStack bandwidth:120G(144G)\n","stackable port number:2 to 6\nStack bandwidth:120G(144G)\n","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 6\nstack bandwidth:\n:40G~120G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G","stackable port number:2 to 8\nstack bandwidth:\n:40G~160G"]
[null,"MAX Stack num",16,16,16,"-",16,16,16,16,16,"9（IRF）/16（IRF-Lite）",16,16,16,2,16,16,16,16,16,16,9,9,9,9,8,8,8,8,8,9,9,9,8,8,8,8,8,16,16,16,16,4,4,4,4,4,4,4,4,"-","-",4,4,4,4,9,4,4,4,4,9,9,9,9,9,9,9,9,9,9,9,9,9,9,9,9,9]
["L2 protocal","Static ARP num",16,16,16,16,16,16,16,16,16,256,16,16,16,16,16,16,16,16,16,16,"1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K",64,64,64,64,64,64,64,64,512,512,512,512,512,512,512,"1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K"]
[null,"Dynamic ARP num",256,256,256,256,256,256,256,256,256,"up to 256",256,256,256,256,256,256,256,256,256,256,"up to 2K","up to 2K","up to 2K","up to 2K","2K","2K","2K","2K","2K","up to 8K","up to 8K","up to 8K","4K","4K","4K","4K","4K","2.5K","2.5K","2.5K","2.5K",256,256,256,256,256,256,256,256,"1k","1k","1k","1k","1k","1k","1k","up to 2k","up to 2k","up to 2k","up to 2k","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 8K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 16K","up tp 8K","up tp 8K","up tp 8K"]
[null,"RARP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ARP Proxy","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3x","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3ad","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP local forwarding first","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LACP short-time","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1P","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1Q","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.1X","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"STP(802.1D)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RSTP(802.1w)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSTP(802.1s)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(32 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(15  instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)"]
[null,"PVST+","Y(16)","Y(16)","Y(16)","-","-","-","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(128)","Y(16 instances)","Y(16 instances)","Y(16 instances)","-","-","-","-","-","-","-","Y(128)","Y(128)","Y(128)","Y(128)","-","-","-","-","-","Y(128)","Y(128)","Y(128)","-","-","-","-","-","-","-","-","-","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(15)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(32)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)"]
[null,"TC snooping","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BPDU DROP","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Smart Link","-","-","-","-","-","-","Y","Y","Y","Y(26 groups)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y","Y","Y","Y","Y","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(4 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(48 groups)","Y(48 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)","Y(26 groups)"]
[null,"Smart Link multi-instances","-","-","-","-","-","-",24,24,24,"Y(16 instances)",24,24,24,"-","-","-","-","-","-","-","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","-","-","-","-","-","Y(16 instances)","Y(16 instances)","Y(16 instances)","-","-","-","-","-","Y","Y","Y","Y","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16  instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)","Y(32 instances)"]
[null,"LLDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"LLDP-MED","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"poe power allocation via lldp","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"QINQ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Selective QINQ","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VLAN MAPPING ","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Fast-leave","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Group-policy","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP PROXY","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP V3 Snooping","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM Snooping","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MVR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(mvr/mvr+)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y","Y(MVR+)","Y(MVR+)","Y(MVR+)","Y(MVR+)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)"]
[null,"MVR+","-","-","-","-","-","-","-","-","-","Y(mvr/mvr+)","-","-","-",null,null,"Y","Y","Y","Y","Y","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)","Y(mvr/mvr+)"]
[null,"GVRP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GMRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"MVRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"RRPP","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RRPP multi-instances","-","-","-","-","-","-","-","-","-","Y(24 instances，16ring)","-","-","-","-","-","-","-","-","-","-","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","-","-","-","-","-","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","-","-","-","-","-","Y(32)","Y(32)","Y(32)","Y(32)","-","-","-","-","-","-","-","-","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(8 instances )","Y(16 instances )","Y(16 instances )","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)","Y(24 instances，16ring)"]
[null,"support users by 5 rules","-","-","-","-","-","-","Y","Y","Y","per port :102\nall:204","Y","Y","Y","all:48\nper port max:48","all:96\nper port max:96","all:192\nper port max:192","all:192\nper 8 fe max:32\nper fe max:32","all:48\nper port max:48","all:96\nper port max:96","all:192\nper port max:192","per port :102\nall:102","per port :102\nall:204","per port :102\nall:102","per port :102\nall:204","all:96\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","per port :102\nall:102/204(Two Chips)","per port :102\nall:102/204(Two Chips)","per port :102\nall:102/204(Two Chips)","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all:192\nper 8 fe max:32\nper fe max:32","all:96\nper 8 fe max:32\nper fe max:32","all: 360\nper fe:50\nper ge:100","all: 360\nper fe:50\nper ge:100","all: 360\nper fe:50\nper ge:100","all: 360\nper fe:50\nper ge:100","Y","Y","Y","Y","Y","Y","Y","Y",140,280,140,280,140,280,"Per port :128\n",140,280,140,280,"per port :307\nall:307","per port :614\nall:614","per port :307\nall:307","per port :307\nall:307","per port :614\nall:614","per port :307\nall:307(34C)","per port :307\nall:614(58C)","Y","per port :600\nall:860","Y","Y","Y","Y","Y","Y","Y","per port :600\nall:860"]
[null,"support users by 10 rules","-","-","-","-","-","-","Y","Y","Y","per port :51\nall:102","Y","Y","Y","all:24\nper port max:24","all:48\nper port max:48","all:96\nper port max:96","all:96\nper 8 fe max:16\nper fe max:16","all:24\nper port max:24","all:48\nper port max:48","all:96\nper port max:96","per port :51\nall:51","per port :51\nall:102","per port :51\nall:51","per port :51\nall:102","all:48\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","per port :51\nall:51/102(Two Chips)","per port :51\nall:51/102(Two Chips)","per port :51\nall:51/102(Two Chips)","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all:96\nper 8 fe max:16\nper fe max:16","all:48\nper 8 fe max:16\nper fe max:16","all: 180\nper fe:25\nper ge:50","all: 180\nper fe:25\nper ge:50","all: 180\nper fe:25\nper ge:50","all: 180\nper fe:25\nper ge:50","Y","Y","Y","Y","Y","Y","Y","Y",70,140,70,140,70,140,"Per port:64",70,140,70,140,"per port :153\nall:153","per port :307\nall:307","per port :153\nall:153","per port :153\nall:153","per port :307\nall:307","per port :153\nall:153(34C)","per port :153\nall:306(58C)","Y","per port :310\nall:590","Y","Y","Y","Y","Y","Y","Y","per port :310\nall:590"]
[null,"support users by 20 rules","-","-","-","-","-","-","Y","Y","Y","per port :25\nall:50","Y","Y","Y","all:12\nper port max:12","all:24\nper port max:24","all:48\nper port max:48","all:48\nper 8 fe max:8\nper fe max:8","all:12\nper port max:12","all:24\nper port max:24","all:48\nper port max:48","per port :25\nall:25","per port :25\nall:50","per port :25\nall:25","per port :25\nall:50","all:24\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","per port :25\nall:25/50(Two Chips)","per port :25\nall:25/50(Two Chips)","per port :25\nall:25/50(Two Chips)","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all:48\nper 8 fe max:8\nper fe max:8","all:24\nper 8 fe max:8\nper fe max:8","all: 90\nper fe:12\nper ge:24","all: 90\nper fe:12\nper ge:24","all: 90\nper fe:12\nper ge:24","all: 90\nper fe:12\nper ge:24","Y","Y","Y","Y","Y","Y","Y","Y",35,70,35,70,35,70,"Per port:32\n",35,70,35,70,"per port :76\nall:76","per port :153\nall:153","per port :76\nall:76","per port :76\nall:76","per port :153\nall:153","per port :76\nall:76(34C)","per port :76\nall:152(58C)","Y","per port :160\nall:167","Y","Y","Y","Y","Y","Y","Y","per port :160\nall:167"]
[null,"consumed time for parallel authentication of 20 users per 10 rules ","-","-","-","-","-","-","Y","Y","Y","双芯片：4S","Y","Y","Y","20s","20s","20s","17s","20s","20s","20s","Single-Chip：4S","Two-Chip：4S","Single-Chip：4S","Two-Chip：4S","17s","17s","17s","17s","17s","Single-Chip：4S\nTwo-Chip：4S","Single-Chip：4S\nTwo-Chip：4S","Single-Chip：4S\nTwo-Chip：4S","17s","17s","17s","17s","17s","15s","15s","15s","15s","Y","Y","Y","Y","Y","Y","Y","Y","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n\n\n","10s\n\n","10s\n\n\n","5s\n","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n\n\n","10s\n\n\n","10s\n\n","10s\n","11s\n","Y","10s","Y","Y","Y","Y","Y","Y","Y","10s"]
[null,"consumed time for parallel authentication of all users per 10 rules ","-","-","-","-","-","-","Y","Y","Y","双芯片：10S","Y","Y","Y","40s","60s","80s","100s","40s","60s","80s","Single-Chip：9S","Two-Chip：10S","Single-Chip：9S","Two-Chip：10S","58s","58s","100s","58s","100s","Single-Chip：9S\nTwo-Chip：10S","Single-Chip：9S\nTwo-Chip：10S","Single-Chip：9S\nTwo-Chip：10S","58s","100s","58s","100s","58s","35s","60s","35s","35s","Y","Y","Y","Y","Y","Y","Y","Y","30s\n\n\n","60s\n\n\n","30s\n\n","60s\n\n\n","30s\n\n","60s\n\n\n","18s","30s\n\n\n","60s\n\n\n","30s\n\n","60s\n\n\n","40s\n\n\n","80s\n","40s\n\n\n","40s\n\n\n","80s\n","31s\n","62s","Y","30s","Y","Y","Y","Y","Y","Y","Y","30s"]
[null,"consumed time for parallel authentication of all users per 20 rules ","-","-","-","-","-","-","Y","Y","Y","双芯片：10S","Y","Y","Y","30s","40s","40s","42s","30s","40s","40s","Single-Chip：9S","Two-Chip：10S","Single-Chip：9S","Two-Chip：10S","28s","28s","42s","28s","42s","Single-Chip：9S\nTwo-Chip：10S","Single-Chip：9S\nTwo-Chip：10S","Single-Chip：9S\nTwo-Chip：10S","28s","42s","28s","42s","28s","50s","100s","50s","50s","Y","Y","Y","Y","Y","Y","Y","Y","20s\n\n\n","33s\n\n\n","20s\n\n","33s\n\n\n","20s\n\n","33s\n\n\n","17s","20s\n\n\n","33s\n\n\n","20s\n\n","33s\n\n\n","65s\n\n\n","130s\n","65s\n\n\n","65s\n\n\n","130s\n","31s\n","\n62s","Y","40s","Y","Y","Y","Y","Y","Y","Y","40s"]
[null,"SSH V1.5","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH V2","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp snooping option82","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dhcp relay option82","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING TRUST","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Snooping item backup","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y",null,null,"-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP SNOOPING","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["port features","IP+MAC Binding","-","-","-","-","-","-",128,128,128,"-",128,128,128,128,128,128,"Y",128,128,128,"-","-","-","-","Y","Y","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","-","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"IP+PORT Binding","-","-","-","-","-","-",128,128,128,"all 256，per port 256",128,128,128,128,128,128,"Y",128,128,128,"all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","Y","Y","Y","Y","Y","all 512，per port 256","all 1024，per port 256","all 512，per port 256","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all: 512\nper port:512","all: 512\nper port:512","all: 512\nper port:512"]
[null,"MAC+PORT Binding","-","-","-","-","-","-",128,128,128,"all 256，per port 256",128,128,128,128,128,128,"Y",128,128,128,"all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","Y","Y","Y","Y","Y","all 512，per port 256","all 1024，per port 256","all 512，per port 256","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all: 512\nper port:512","all: 512\nper port:512","all: 512\nper port:512"]
[null,"IP+MAC+PORT Binding","-","-","-","-","-","-",128,128,128,"all 256，per port 256",128,128,128,128,128,128,"GE:50   8FE:100\nTotal:500",128,128,128,"all 512，per port 256","all 1024，per port 256","all 512，per port 256","all 1024，per port 256","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","all 512，per port 256","all 1024，per port 256","all 512，per port 256","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","GE:50   8FE:100\nTotal:500","GE:50   8FE:100\nTotal:800","GE:50   8FE:100\nTotal:500","100 per port\nTotal: 500","100 per port\nTotal: 500","100 per port\nTotal: 500","100 per port\nTotal: 500","Y - ACL Specification Limits","Y - ACL Specification Limits","Y - ACL Specification Limits","Y - ACL Specification Limits","Y - ACL Specification Limits","Y - ACL Specification Limits","Y - ACL Specification Limits","Y - ACL Specification Limits","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","Y(500)","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :500 \nall      :500","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","per port :1000 \nall      :1000","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all 2K，per port 2K","all: 512\nper port:512","all: 512\nper port:512","all: 512\nper port:512"]
[null,"MAX num in one link group",8,8,8,8,8,8,8,8,8,"8FE/8GE",8,8,8,8,8,8,8,8,8,8,"8FE/8GE","8FE/8GE","8FE/8GE","8FE/8GE",8,8,8,8,8,"8FE/8GE","8FE/8GE","8FE/8GE",8,8,8,8,8,"8FE/4GE","8FE/4GE","8FE/4GE","8FE/4GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/8*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/4*10GE","8GE/6*10GE","8GE/6*10GE","8GE/8*10GE","6GE/6*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE","8GE/8*10GE"]
[null,"Link group num",4,9,13,2,2,3,4,9,13,"IRF: 128",4,9,13,4,9,13,26,4,9,13,"IRF: 128","IRF: 128","IRF: 128","IRF: 128","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","IRF: 128","IRF: 128","IRF: 128","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )","8 (PORT NUM/2  IF WITHOUT IRF )",14,26,14,14,4,10,14,26,4,14,4,14,12,24,"single device:14\nirf:128","single device:26\nirf:128","single device:14\nirf:128","single device:26\nirf:128",128,"14\nirf:128","26\nirf:128","14\nirf:128","26\nirf:128","single device:14\nirf:128","single device:26\nirf:128","single device:14\nirf:128","single device:14\nirf:128","single device:26\nirf:128","single device:128\nirf:128","single device:128\nirf:128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128","IRF: 128"]
[null,"restore port default config","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DLDP","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VCT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Access manage(port isolate)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Port loopback-detection","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Multi-Port loopback-detection","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-",null,"-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y",{"$nulls":5},"Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Port loop test(inclding inner loop and outer loop)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Port miirroring","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Proportion of Port Miirroring","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:4","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:4","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1","8:1","8:1","8:1","8:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"Traffic Mirroring","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Proportion of Traffic Mirroring","-","-","-","-","-","-","N:1","N:1","N:1","N:4","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:4","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1","N:4","N:4","N:4","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","N:1","-","-","-","-","-","-","-","-","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4","N:4"]
[null,"RSPAN","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","N","N","N","N","N","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"storm constrain","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Unicast Suppression","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y","Y","Y","Y(1% or pps bps)","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y(1% or pps)","Y(bps)","Y(bps)","Y(bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y","Y","Y","Y","Y","Y","Y","Y","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps or bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)"]
[null,"Multicast  Suppression","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y","Y","Y","Y(1% or pps bps)","Y","Y","Y","Y(bps)","Y(bps)","Y(bps)","Y(1% or pps)","Y(bps)","Y(bps)","Y(bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y","Y","Y","Y","Y","Y","Y","Y","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps or bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)"]
[null,"Broadcast Suppression","Y","Y","Y","Y(1% bps)","Y(1% bps)","Y(1% bps)","Y","Y","Y","Y(1% or pps bps)","Y","Y","Y","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1% or pps)","Y(1%/ bps)","Y(1%/ bps)","Y(1%/ bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y（%1）","Y（%1）","Y（%1）","Y（%1）","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% ,pps,kbps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps)","Y(1% or pps or bps)","Y(1% or pps or bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)","Y(1% or pps bps)"]
["port security","mac black hole","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Sticky Mac","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic  ARP Inspection","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPSource Guard","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Port Max-Mac-Count","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["vlan ","Port based vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MAC based vlan","Y","Y","Y","-","-","-","Y","Y","Y","Y(up to 8K)","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","-","-","-","-","-","Y(up to 8K)","Y(up to 8K)","Y(up to 8K)","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(1K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(8K)","Y(4K)","Y(4K)","Y(4K)"]
[null,"IPv4 subnet based vlan","-","-","-","-","-","-","-","-","-","Y(ALL:256)","-","-","-","-","-","-","-","-","-","-","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","-","-","-","-","-","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)","-","-","-","-","-","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","-","-","-","-","-","-","-","-","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:256 PER vlan:12)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:512)","Y(ALL:256)","Y(ALL:256)","Y(ALL:256)"]
[null,"Protocal based vlan","-","-","-","-","-","-","Y","Y","Y","Y(16 per port)","Y","Y","Y","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y(per port: 7)","Y( all: 16)","Y( all: 16)","Y( all: 16)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 7)","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y(per port: 12 )","Y","Y","Y","Y","Y","Y","Y","Y","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)","Y(16 per port)"]
[null,"Voice Vlan","-","-","-","-","-","-","Y","Y","Y","Y(oui 16,vlan 128)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y","Y","Y","Y","Y","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y(oui 16,vlan 128)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)","Y(oui 128,vlan 8)"]
[null,"SuperVLAN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Guest vlan","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PVLAN","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["ip routing protocal","IP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TCP/UDP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ICMP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IRDP","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPV1/2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V2","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IS-IS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HWPING(NQA)","Y","N","N","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Static routing","Y","Y","Y","-","-","-","Y","Y","Y",32,"Y","Y","Y","-","-","-","-","-","-","-","Y(2k)","Y(2k)","Y(2k)","Y(2k)",64,64,64,64,64,"Y(2k)","Y(2k)","Y(2k)",256,256,256,256,256,"1K","1K","1K","1K","Y","Y","Y","Y","Y","Y","Y","Y",32,32,32,32,32,32,128,64,64,64,64,"Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)","Y(4k)"]
[null,"MAX num of second ip ","-","-","-","-","-","-","-","-","-",4,"-","-","-","-","-","-","-","-","-","-",48,48,48,48,4,4,4,4,4,48,48,48,4,4,4,4,4,9,9,9,9,"-","-","-","-","-","-","-","-",4,4,4,4,4,4,4,4,4,4,4,9,9,9,9,9,9,9,48,48,48,48,48,48,48,48,48,48]
[null,"DHCP RELAY SECURITY","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Relay","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Client","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP Server","-","-","-","-","-","-","-","-","-","Y","-","-","-","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(16)","-","-","-","Y(255)","Y(255)","Y(255)","Y(255)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(255)","Y(255)","Y(255)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16)","Y(16 instance)","Y(16 instance)","Y(16 instance)","Y(16 instance)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(64)","Y(64)","Y(64)","Y(64)","Y(64)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)"]
[null,"VRRPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD","-","-","-","-","-","-","-","-","-","Y(STATIC ROUTING)","-","-","-","-","-","-","-","-","-","-","Y(VRRP/STATIC ROUTING)","Y(VRRP/STATIC ROUTING)","Y(VRRP/STATIC ROUTING)","Y(VRRP/STATIC ROUTING)","-","-","-","-","-","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","-","-","-","-","-","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","Y(VRRP /STATIC ROUTING/OSPF)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)","Y(OSPF/VRRP/BGP/ISIS/STATIC ROUTING)"]
[null,"Routed ports","-","-","-","-","-","-","-","-","-","Y","-","-","-",null,null,null,"-",null,null,null,"Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","Y(limited version)","Y(limited version)","Y(limited version)","Y(limited version)","Y(limited version)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ECMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)",{"$nulls":5},"Y(256*8)","Y(256*8)","Y(256*8)","Y(256*3)","Y(256*3)","Y(256*3)","Y(256*3)","Y(256*3)","Y(600*4)","Y(600*4)","Y(600*4)","Y(600*4)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)","Y(256*8)"]
[null,"Policy based routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["OSM","Firewall Modul","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","Y","Y","-","-"]
[null," IPS Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","Y","Y","-","-"]
[null,"Wireless Access Controller Module","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y(ONLY SMALL CARD)","Y","Y","-","-"]
["MCE","MAX num of VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(63 instances)","Y(63 instances)","Y(63 instances)","Y(63 instances)","-","-","-","-","-","Y(63 instances)","Y(63 instances)","Y(63 instances)","-","-","-","-","-","Y(16 instances)","Y(16 instances)","Y(16 instances)","Y(16 instances)","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(64 instances)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)","Y(1024)"]
[null,"MCE IPV4 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MCE IPV4 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MCE IPV6 UNICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MCE IPV6 MULTICAST","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Cut Through","Cut Through Mode","-","-","-",null,null,null,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":5},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-","-","-","-","-","-","-","-","Y","Y","Y"]
["MPLS","MPLS label number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",4000,4000,4000,4000,4000,4000,4000,4000,4000,"-","-","-"]
[null,"MPLS label depth","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","3 layer","3 layer","3 layer","3 layer","3 layer","3 layer","3 layer","3 layer","3 layer","-","-","-"]
[null,"MPLS interface number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",512,512,512,512,512,512,512,512,512,"-","-","-"]
[null,"static LSP number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",256,256,1010,1010,1010,1010,1010,1010,1010,"-","-","-"]
[null,"Maximum number of LSPs supported","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",512,512,4096,4096,4096,4096,4096,4096,4096,"-","-","-"]
[null,"Equivalent LSP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","NO","NO","NO","NO","NO","NO","NO","NO","NO","-","-","-"]
[null,"LDP local peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",128,128,128,128,128,128,128,128,128,"-","-","-"]
[null,"LDP remote peer number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",256,256,256,256,256,256,256,256,256,"-","-","-"]
[null,"mpls TE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-"]
[null,"mpls lsp tracert","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-"]
[null,"mpls lsp ping","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-"]
["MPLS L2VPN","mpls l2vpn(VLL):martini","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","connection number:4000","-","-","-"]
[null,"mpls l2vpn(VLL):kompella","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","connection number:1000","-","-","-"]
[null,"VPN number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",1000,1000,1000,1000,1000,1000,1000,1000,1000,"-","-","-"]
[null,"CE number per VPN","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",200,200,200,200,200,200,200,200,200,"-","-","-"]
[null,"mpls l2vpn(VLL):CCC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","-","-","-"]
[null,"mpls l2vpn(VLL):SVC","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","connection number:512","-","-","-"]
["MPLS L3VPN","VRF number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",1023,1023,"1k","1k","1k","1k","1k","1k","1k","-","-","-"]
[null,"interface number per VRF","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",128,128,"1k","1k","1k","1k","1k","1k","1k","-","-","-"]
["VPLS","VSI number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",1024,1024,1024,1024,1024,1024,1024,1024,1024,"-","-","-"]
[null,"Number of Pseudo Wires","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-",4096,4096,4096,4096,4096,4096,4096,4096,4096,"-","-","-"]
["VPN","the max multicast number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-",4000,4000,4000,4000,4000,4000,4000,"-","-","-"]
[null,"the max multicast number in public network instance","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-",4000,4000,4000,4000,4000,4000,4000,"-","-","-"]
[null,"the max switchgroup number per vpn","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-",0,0,0,0,0,0,0,"-","-","-"]
[null,"global max switchgroup number","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-",0,0,0,0,0,0,0,"-","-","-"]
["traffic statistic","SFLOW","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y(1/1000 TO 1/500000)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NetStream/NetFlow/IPFIX","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-"]
["L3 multicast\nprotocal","IGMP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IGMP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PIM-DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BI-PIM","-","-","-","-","-","-","-","-","-","-","-","-","-",null,null,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-",null,null,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MSDP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["OAM","802.1AG","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"802.3AH","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["web management","RMON1","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RMON2","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SMON","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WEB","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HTTPS","Y","Y","Y","Y(only for web manager)","Y(only for web manager)","Y(only for web manager)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMPV1/2/3","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"HGMP V1 SERVER","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V1 CLINET","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"HGMP V2 ","Y","Y","Y","Y（256）","Y（256）","Y（256）","Y","Y","Y","Y(255)","Y","Y","Y","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y(255)","Y(255)","Y(255)","Y(255)","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y(255)","Y(255)","Y(255)","Y（256）","Y（256）","Y（256）","Y（256）","Y（256）","Y(255)","Y(255)","Y(255)","Y(255)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)","Y(255)"]
[null,"IMC","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BIMS","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","-","Y","-","-","-","-","-","-","-","Y"]
[null,"IPV6 HOST MANGEMENT","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"NCC","-","-","-","-","-","-","-","-","-","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["device management","CLI","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","shutdown-interval","Y","Y","Y","Y","Y","Y","Y","Y","Y","shutdown-interval","shutdown-interval","Y","shutdown-interval","Y","Y","Y","Y","Y","Y","Y","shutdown-interval"]
[null,"TELNET","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"FTP","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-"]
[null,"SCP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"ZERO CONFIG(DHCP AUTO CONFIG)","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ZERO CONFIG(CWMP-TR069)","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Device access control","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"schedule job","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"the warning upper and lower temperature","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"arp,bfd,lacp mad","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ISSU","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"port auto recovery/shutdown-interval","-","-","-","-","-","-","-","-","-","shutdown-interval","-","-","-","-","-","-","-","-","-","-","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","-","-","-","-","-","shutdown-interval","shutdown-interval","shutdown-interval","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","shutdown-interval","Y","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","shutdown-interval","Y"]
[null,"port auto power down","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","port auto power down","Y","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","port auto power down","Y"]
[null,"EEE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","Y","Y","-","Y","-","-","-","-","-","-","-","Y"]
["access authentication","Mac address  authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"web authentication","-","-","-","-","-","-","-","-","-","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"triple authentication","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TACACS+","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"multi-radius server","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y",null,null,"-","-","-","-","-","Y","Y","Y","Y",{"$nulls":5},"Y","Y","Y",null,null,"-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Dynamic VLAN ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PEAP/EAP-TLS","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"L2  PORTAL authentication","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"L3  PORTAL authentication","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"portal hotbackup","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y",{"$nulls":5},"Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Remote 802.1x authentication ","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Local 802.1x authentication","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MAX 802.1x USERS Per Port ",256,256,256,256,256,256,256,256,256,"2K",256,256,256,256,256,256,256,256,256,256,"2K","2K","2K","2K",256,256,256,256,256,"2K","2K","2K",256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,256,"2k","2k","2K","2K","2K","2K","2K","2K","2K","2K","2K","2K"]
[null,"MAX 802.1x USERS Total",1024,1024,1024,"1K","1K","1K",1024,1024,1024,"2K",1024,1024,1024,"1K","1K","1K","1K","1K","1K","1K","2K","2K","2K","2K","1K","1K","1K","1K","1K","2K","2K","2K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","1K","2k","2K","2K","2K","2K","2K","2K","2K","2K","2K","2K","2K"]
[null,"portal  USERS",512,512,512,512,512,512,512,512,512,"Y(ALL:1024\nPER PORT OR PER VLAN:512",512,512,512,512,512,512,"-",512,512,512,"Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","Y(ALL:1024\nPER PORT OR PER VLAN:512","Y(ALL:512\nPER PORT OR PER VLAN:512","-","-","-","-",512,512,512,512,512,512,512,512,"-","-","-","-","-","-",1000,"-","-","-","-","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan: 3000\nmax: 3000\nMaxFreeRule:64","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan:1500\nmax: 1500\nMaxFreeRule:64","per vlan: 3000\nmax: 3000\nMaxFreeRule:64","ALL:3000(58C)/1500(34C)\nPER PORT OR PER VLAN:1500","ALL:3000(58C)/1500(34C)\nPER PORT OR PER VLAN:1500","Y(ALL:3000\nPER PORT OR PER VLAN:3000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:3000\nPER PORT OR PER VLAN:3000)","Y(ALL:3000\nPER PORT OR PER VLAN:3000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:6000\nPER PORT OR PER VLAN:6000)","Y(ALL:640\nPER PORT OR PER VLAN:640)","Y(ALL:640\nPER PORT OR PER VLAN:640)","Y(ALL:640\nPER PORT OR PER VLAN:640)"]
["QOS","Strict priority","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"WFQ","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+WRR","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"SDWRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SP+WDRR","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BUFFER configurable","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ACL logging","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RED","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"WRED","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["IPV6 ","IPV6 unitcast routing num",16,16,16,"-","-","-",16,16,16,"up to 32",16,16,16,"-","-","-","-","-","-","-","up to 1K","up to 1K","up to 1K","up to 1K","-","-","-","-","-","up to 6K","up to 6K","up to 6K","-","-","-","-","-","1K","1K","1K","1K","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 32","up to 64","up to 256","up to 256","up to 256","up to 256","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 6k","up to 8k","up to 8k","up to 8k","up to 8k","up to 8k","up to 8k","up to 8k","up to 6k","up to 6k","up to 6k"]
[null,"IPV6 ACL NUM","-","-","-","-","-","-",256,512,1000,"Ingress:512*2\nEgress:256*2",256,512,1000,256,512,1000,"-",256,512,1000,"Ingress:512\nEgress:256","Ingress:512*2\nEgress:256*2","Ingress:512\nEgress:256","Ingress:512*2\nEgress:256*2","-","-","-","-","-","Ingress:512\nEgress:256","Ingress:512\nEgress:256","Ingress:512\nEgress:256","-","-","-","-","-","1K","1K","1K","1K",480,480,480,480,480,480,480,480,"1k","2k","1k","2k","1k","2k","Ingress:3072  Egress:1024","1k","2k","1k","2k","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3k\nEgress:\n448","Ingress:3k\nEgress:\n448","Ingress:6k\nEgress:\n832","Ingress:3k  Egress:512","Ingress:3k  Egress:512","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:6k\nEgress:\n1k","Ingress:6k\nEgress:\n1k","Ingress:12k\nEgress:\n2K","Ingress:12k\nEgress:\n2K","Ingress:1.5K\nEgress:\n512","Ingress:1.5K\nEgress:\n512","Ingress:1280\nEgress:\n512"]
[null,"IPV6 ND NUM",1024,1024,1024,"-","-","-",1024,1024,1024,"up to 256",1024,1024,1024,"-","-","-","-","-","-","-","up to 1K","up to 1K","up to 1K","up to 1K","-","-","-","-","-","up to 4K","up to 4K","up to 4K","-","-","-","-","-","2.5K","2.5K","2.5K","2.5K",256,256,256,256,256,256,256,256,256,256,256,256,256,256,500,"1K","1K","1K","1K","4k","4k","4k","4k","4k","8k（bind 1000）","8k（（bind 1000））","8k","8k","8k","8k","8k","8k","8k","4k","4k","4k"]
[null,"ICMPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TRACEROUTE V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"TELNET V6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SSH2 V6","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SFTP V6","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND snooping","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND proxy","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"ND detection","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SAVI","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"PMTU","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DNS CLINET FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"SNMP FOR IPV6","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"RIPng","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"OSPF V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IS-IS V6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BGP4+ FOR IPV6","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPV6 policied routing","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"MLD SNOOPING","-","-","-","-","-","-","Y","Y","Y","Y(V1/V2)","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","-","-","-","-","-","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y","Y","Y","Y","Y","Y","Y","Y","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)","Y(V1/V2)"]
[null,"IPv6 PIM DM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 PIM SM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 BI-PIM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 PIM SSM","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"VRRP V3","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 snooping","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 client","Y","Y","Y","-","-","-","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 relay","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"DHCP V6 server","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"IPv6 source guard","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"BFD v6(OSPFv3/IPv6 VRRP/BGP4+/ISISv6/IPv6 STATIC ROUTING)","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"GRE over ipv4\nGRE over ipv6\nip6 over ipv4  mannul\n6to4\nISATAP\nipv6 over ipv6\nipv4 over ipv4\nipv4 over ipv6","-","-","-","-","-","-","-","-","-","Y","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","-","Y","Y","Y","-","-","-","-","-","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","IPv6 over IPv4 Config\nIPv6 over IPv4 Auto\nIPv6 over IPv4 6to4\nIPv6 over IPv4 ISATAP","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)","Y(128)"]
[null,"6VPE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","N","N","N","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":8},"Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
["Power Over Ethernet  ","POE","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","Y","Y","Y","-","-","Y(15.4W)","Y(15.4W)","-","-","-","Y","Y","-","-","Y(15.4W)","-","-","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","Y","Y","-","-","-","Y","Y","-","-","-","Y","Y","-","-","-","-","-","-","Y(15.4W)","Y(15.4W)","Y(15.4W)","-","-","-"]
[null,"POE+","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",null,"-","-","-","-","-","Y(30W)","Y(30W)",{"$nulls":5},"-","-","Y(30W)",{"$nulls":5},"-","-","-","-","-","-","-","-","-","-","Y","Y","-","-","-","-","Y","Y","-","-","-","Y","Y","-","-","-","Y","Y","-","-","-","-","-","-","Y(30W)","Y(30W)","Y(30W)","-","-","-"]
[null,"Total Power","-","-","-","-","-","-","-","-","-","-","125W","250W","370W","-","-","-","-","AC:\nALL:95W POE:65W\n","AC:\nALL:160W POE:125W","AC:\nALL:465W POE:370W\nDC:\nALL:400W POE:370W","-","-","DC：795W(720W for poe)\nAC：465W(370W for poe)","DC：820W(720W for poe)\nAC：440W(320W for poe)","-","-","-","DC:370W\nAC:300","DC:740W\nAC:300","-","-","DC：795W(720W for poe)\nAC：465W(370W for poe)","-","-","DC:370W\nAC:300","DC:740W\nAC:300","-","-","-","-","-","-","-","-","-","MIN:\nAC：10W\nMAX:\nAC：95W(65W for poe)","MIN:\nAC：25W\nMAX:\nAC：255W(170W for poe)","MIN:\nAC：19W\nMAX:\nAC：230W(180W for poe)","MIN:\nDC：27.5W\nAC：45.6W\nMAX:\nDC：832W(740W for poe)\nAC：528W(370W for poe)","-","-","-","-","MIN:65W\nMAX:585W(215W for system，370W for poe)","MIN:90W\nMAX:\nAC:550W(281W for system，370W for poe)\nRPS:920W(181W for system，740W for poe)","-","-","-","AC:\n585W (370W for poe)\nDC(RPS):\n491W (370W for poe)","AC:\n651W (370W for poe)\nDC(RPS):\n921W (740W fow poe)","-","-","-","AC：\n591W(221W for system and 370W for poe)\nDC:\n492W(122W for system and 370W fow poe)\n","AC：\n661W(291W for system and 370W for POE)\nDC：\n930W (190W for system and 740W for poe)","-","-","-","-","-","-","MIN:\nDC：64W\nAC：85W\nMAX:\nDC：870W(740W for poe)\nAC：598W(370W for poe)","MIN:\nDC：107W\nAC：131W\nMAX:\nDC：973W(740W for poe)\nAC：673W(370W for poe)\n","MIN:\nDC：94W\nAC：96W\nMAX:\nsingle DC:1840W(1500W for poe)\ndual DC:1840W(1500W for poe)\nsingle AC:714W(425W for poe)\ndual AC:1147W(740W for poe)","-","-","-"]
[null,"Power Per Port","-","-","-","-","-","-","-","-","-","-","15.4W","15.4W","15.4W","-","-","-","-","15.4W","15.4W","15.4W","-","-","30W","30W","-","-","-",15.4,15.4,"-","-","30W","-","-",15.4,15.4,"-","-","-","-","-","-","-","-","-","15.4W","15.4W","30W","30W","-","-","-","-","30W","30W","-","-","-","30W","30W","-","-","-","30W","30W","-","-","-","-","-","-","30W","30W","30W","-","-","-"]
[null,"802.3af","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","-","-","-","-","Y","Y","Y","-","-","Y","Y","-","-","-","Y","Y","-","-","Y","-","-","Y","Y","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","-","-","-","-","Y","Y","-","-","-","Y","Y","-","-","-","30W","30W","-","-","-","-","-","-","Y","Y","Y","-","-","-"]
[null,"Mode of  Voltage Supply","-","-","-","-","-","-","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","-","-","Data wire mode","Data wire mode","-","-","-","Data wire mode","Data wire mode","-","-","Data wire mode","-","-","Data wire mode","Data wire mode","-","-","-","-","-","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","Data wire mode","-","-","-","-","Data wire mode","Data wire mode","-","-","-","Data wire mode","Data wire mode","-","-","-","Data wire mode","Data wire mode","-","-","-","-","-","-","Data wire mode","Data wire mode","Data wire mode","-","-","-"]
["physical feature","Power Supply","AC","AC","AC","AC","AC","AC","AC","AC","AC","AC","AC","AC/DC","AC/DC","AC/DC","AC/DC","AC/DC","AC","AC","AC","AC&DC(RPS)","AC","AC","AC&RPS(52V)","AC&RPS(52V)","AC","AC","AC","AC&DC","AC&DC","AC&RPS(48V)","AC&RPS(48V)","AC&RPS(52V)","AC&DC","AC&DC","AC&DC","AC&DC","AC&DC","AC&DC","AC&DC","AC&DC","AC&DC","AC","AC","AC","AC","AC","AC","AC","AC/RPS",{"$nulls":6},"AC/DC(48V)BAK 1+1 Dual-hot-pluggable","AC/DC","AC/DC","AC/DC","AC/DC","AC&RPS(12V)","AC&RPS(12V)","AC/DC(48V)+BACKUP MODEL","AC&RPS(48V)","AC&RPS(48V)","AC/DC(48V)BAK 1+1 Dual-hot-pluggable","AC/DC(48V)BAK 1+1 Dual-hot-pluggable","AC&RPS(12V)","AC/DC(52V)BAK 1+1 Dual-hot-pluggable\n","AC&RPS(12V)","AC/DC(48V)BAK 1+1 ","AC&RPS(52V)","AC&RPS(52V)","AC/DC(52V)BAK 1+1 ","AC/DC(48V)BAK 1+1 ","AC/DC(48V)BAK 1+1 ","AC/DC(48V)BAK 1+1\nDual-hot-pluggable\n"]
[null,"Power Consummtion(w)",9,12,13,10,14,16,9,12,13,"41W",155,"AC:300\nDC:273","AC:465\nDC:400",12,15,17,50,"AC:\nALL:95W POE:65W\n","AC:\nALL:160W POE:125W","AC:\nALL:465W POE:370W\nDC:\nALL:400W POE:370W","26W","41W","DC：795W(720W for poe)\nAC：465W(370W for poe)","DC：820W(720W for poe)\nAC：440W(320W for poe)",40,40,50,"DC:430W;AC:450W","DC:820w;AC:465W","31W","43W","无PoE负载：42W\n满PoE负载：\nDC：795W(720W for poe)\nAC：465W(370W for poe)",40,50,"DC:430W;AC:450W","DC:820w;AC:465W",65,35,45,40,60,14.4,22.4,31.5,59.8,"MIN:\nAC：10W\nMAX:\nAC：95W(65W for poe)","MIN:\nAC：25W\nMAX:\nAC：255W(170W for poe)","MIN:\nAC：19W\nMAX:\nAC：230W(180W for poe)","MIN:\nDC：27.5W\nAC：45.6W\nMAX:\nDC：832W(740W for poe)\nAC：528W(370W for poe)","MIN:35W\nMAX:62W","MIN:54W\nMAX:110W","MIN:36W\nMAX:103W","MIN:55W\nMAX:145W","MIN:65W\nMAX:\nAC:585W(215W for system，370W for poe)\nDC:491W(121W for system，370W for poe)","MIN:90W\nMAX:\nAC:651W(281W for system，370W for poe)\nRPS:921W(181W for system，740W for poe)",145,80,120,"AC:\n585W (370W for poe)\nDC(RPS):\n491W (370W for poe)","AC:\n651W (370W for poe)\nDC(RPS):\n921W (740W fow poe)",110,155,115,"AC：\n591W(221W for system and 370W for poe)\nDC(RPS):\n492W(122W for system and 370W fow poe)\n","AC：\n661W(291W for system and 370W for POE)\nDC(RPS)：\n930W (190W for system and 740W for poe)\n",141,191,"MIN:67W\nMAX:105W","125W","MIN:102W\nMAX:163W","MIN:\nDC:58W\nAC:67W\nMAX:\nDC:136W\nAC:146W","MIN:\nDC：64W\nAC：85W\nMAX:\nDC：870W(740W for poe)\nAC：598W(370W for poe)","MIN:\nDC：107W\nAC：131W\nMAX:\nDC：973W(740W for poe)\nAC：673W(370W for poe)\n","MIN:\nDC：94W\nAC：96W\nMAX:\nsingle DC:1840W(1500W for poe)\ndual DC:1840W(1500W for poe)\nsingle AC:714W(425W for poe)\ndual AC:1147W(740W for poe)","MIN:\nAC:105\nDC:103\nMAX:\nAC:245\nDC:241","MIN:\nAC:128\nDC:124\nMAX:\nAC:185\nDC:176","178W"]
[null,"BTU/hr",30.709282050000002,40.9457094,44.35785185,34.1214245,47.7699943,54.5942792,30.70928205,40.9457094,44.35785185,139.8978405,532.2942222,"AC:1023.642735\nDC:931.51488885","AC:1586.64623925\nDC:1364.85698",40.9457094,51.182136750000005,58.00642165,170.6071225,324.15353275,545.942792,"AC:\n1586.64623925\nDC:\n1364.85698",88.7157037,139.8978405,"DC：2712.653248(2456.742564 for poe)\nAC：1586.646239(1262.492707 for poe)","DC：2797.956809(2456.742564 for poe)\nAC：1501.342678(1091.885584 for poe)",136.485698,136.485698,170.6071225,"DC:1467.2212535\nAC:1535.4641025","DC:2797.956809\nAC:1586.64623925",105.776416,146.7221254,"无PoE负载：143.3099829\n满PoE负载：\nDC：2712.653248(2456.742564 for poe)\nAC：1586.646239(1262.492707 for poe)",136.485698,170.6071225,"DC:1467.2212535\nAC:1535.4641025","DC:2797.956809\nAC:1586.64623925",221.78925925000001,119.42498575,153.54641025,136.485698,204.72854700000002,49.13485128000001,76.43199088,107.482487175,204.04611851,"MIN:34.1214245\n\nMAX:324.15353275","MIN:85.30356125\n\nMAX:870.09632475","MIN:64.83070655\n\nMAX:784.7927635","MIN:\nDC：93.833917375\nAC：155.59369572\nMAX:\nDC：2838.9025184\nAC：1801.6112136","MIN:119.42498575\nMAX:211.5528319","MIN:184.2556923\nMAX:375.3356695","MIN:122.8371282\nMAX:351.45067235","MIN:187.66783475\nMAX:494.76065525","MIN:221.7892593\nMAX:\nAC:1996.103333\nRPS:1675.361943","MIN:307.0928205\nMAX:\nAC:2221.304735\nRPS:3142.583196",494.76065525,272.971396,409.45709400000004,"AC: \n1996.103333\nDC(RPS):\n1675.361943","AC: \n2221.304735\nDC(RPS)：\n3139.171054\n",375.3356695,528.88207975,392.39638175000005,"AC：2016.576188\nDC(RPS):1678.774085","AC：2255.426159\nDC(RPS):3173.292479",481.11208545,651.71920795,"MIN:228.61354415\nMAX:358.27495725",426.51780625,"MIN:348.0385299\nMAX:556.17921935","MIN:\nDC:197.9042621\nAC:228.61354415\nMAX:\nDC:464.0513732\nAC:498.1727977","MIN:\nDC:218.3771168\nAC:218.3771168\nMAX:\nDC:2968.5639315\nAC:2040.4611851","MIN:\nDC:365.09924215\nAC:446.99066095\nMAX:\nDC:3320.01460385\nAC:2296.37186885","MIN:\nDC:320.7413903\nAC:327.5656752\nMAX:\nDC:6278.342108\nAC:3913.72739015","MIN:\nDC:358.27495725\nAC:351.45067235\nMAX:\nDC:835.97490025\nAC:822.32633045","MIN:\nDC:436.7542336\nAC:423.1056638\nMAX:\nDC:631.24635325\nAC:600.5370712",607.3613561]
[null,"Power Supply module",{"$nulls":6},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","150W AC, 150W DC\n","-","-","-","-","-","-","-","-","-","150W AC, 150W DC\n","150W AC, 150W DC\n","-","650W AC, 650W DC\n","-","-","-","-","-","-","-","650W AC, 650W DC\n"]
[null,"power rating\n",{"$nulls":6},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","AC: min：68W；max：145W\nDC: min：57.6W；max：126W\n","-","-","-","-","-","-","-","-","-","AC:\nmax:141W\nmin:62W\nDC:\nmin 52W\nmax 111W","AC:\nmax:191W\nmin:94W\nDC:min 79W\nmax 150W\n","-","AC: 90v~264v, \nDC: -36v~ -72v\n","-","-","-","-","-","-","-","AC: 90v~264v, \nDC: -36v~ -72v\n"]
[null,"power load-sharing\n",{"$nulls":6},"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","No, hot-standby\n","-","-","-","-","-","-","-","-","-","No, hot-standby\n","No, hot-standby\n","-","No, hot-standby\n","-","-","-","-","-","-","-","No, hot-standby\n"]
[null,"PDU cable\n",{"$nulls":6},"shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n","shipped with switch\n"]
[null,"Humidity","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","5～95%RH","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%～90%","10%－90%","10%－90%","10%－90%","5～95%RH","5～95%RH","5～95%RH","5～95%RH","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","5～95%RH","5～95%RH","5～95%RH","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%－90%","10%－90%","10%－90%","10%－90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%～90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－95%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","5～95%RH","5～95%RH","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%","10%－90%"]
[null,"Temperature","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0℃～50℃","0~45","0~45","0~45","0~45","0~45","0~45","0～45℃","0~45","0~45","0~45","0℃～50℃","0℃～50℃","0℃～50℃","0℃～50℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃","0℃～50℃","0℃～50℃","0℃～50℃","0～45℃","0～45℃","0～45℃","0～45℃","0～45℃","0~45","0~45","0~45","0~45","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0℃～45℃","0~45","0~45","0~45","0~45","0~45","0~45"," -5~50℃","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0℃～50℃","0℃～50℃","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45","0~45"]
[null,"Storage temperature","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃","-40～+70℃"]
[null,"Storage humidity ","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH，无冷凝","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH","5～95%RH"]
[null,"Full load weight","< 3.0kg","< 3.0kg","< 3.0kg","<2kg","≤3kg","≤3kg","< 3.0kg","< 3.0kg","< 3.0kg","< 5kg","< 3.0kg","< 6.5kg","< 6.5kg","<2kg","≤3kg","≤3kg","《4kg","<2kg","≤3kg","≤3kg","< 5kg","< 5kg","< 10kg","< 10kg","<3.5kg","<3.5kg","<4kg","<5.8kg","<6.2kg","< 5kg","< 5kg","< 10kg","<3.5kg","<4kg","<3.5kg","<4kg","<3.5kg","<4KG","<4KG","<4KG","<4KG","≤3kg","≤3kg","≤3kg","≤5kg","≤3kg","≤7kg","≤3kg","≤7kg","<4.5kg","<5kg","<4.5kg","<5kg","<7kg","<7.5kg","<8.2kg ","<4.5kg","<5kg","<7kg","<7.5kg","<5kg","<5kg","<6kg","<7.5kg","<7.5kg","<7.5kg ","<8.5kg ","<6.0kg","<10Kg\n","<6.5kg","<8.5kg","<8kg","<8.5kg","<18kg","<15kg","<9kg","<10Kg\n"]
[null,"Fan NUM",0,0,0,0,0,0,0,0,0,1,2,3,4,0,0,0,1,2,2,4,1,1,6,6,1,1,1,2,2,1,1,6,1,1,2,2,5,1,1,1,2,0,1,1,1,0,1,0,1,4,4,4,4,4,4,"Dual-hot-pluggable one Fan tray with two fans\n",4,4,4,4,4,4,4,6,6,"3 fixed fans for system\n","3 fixed fans for system\n","fixed fan:4 fans","Dual-hot-pluggable  Fan tray\n","fixed fan:4 fans","hot-swapping fan: 1 fan","fixed fan:6 fans","fixed fan:6 fans","hot-swapping fan box:6 fans","hot-swapping fan box:6 fans","hot-swapping fan: 1 fan","Dual-hot-pluggable  Fan tray\n"]
[null,"Airflow direction\n",{"$nulls":9},"side to back",{"$nulls":6},"side to back",null,null,null,"side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back",{"$nulls":4},"side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back",{"$nulls":6},"Front-to-Back: power->port\nBack-to-Front port->power\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to back","side to side","side to side","side to back","Front-to-Back: power->port\nBack-to-Front port->power\n","side to back","side to back","side to back","side to back","side to back","side to back","side to back","Front-to-Back: power->port\nBack-to-Front port->power\n"]
[null,"Ariflow reverse\n",{"$nulls":9},"-",{"$nulls":6},"-",null,null,null,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-",{"$nulls":6},"Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. \n","-","-","-","-","-","-","-","-","-","-","-","-","Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. \n","-","-","-","-","-","-","-","Yes,o reverse fans, remove fan-tray, unscrew the existing fans, reverse fan, attach with existing scews, re-insert fan-tray. \n"]
[null,"Airflow detection\n",{"$nulls":9},"-",{"$nulls":6},"-",null,null,null,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-",{"$nulls":6},"detect airflow direction via software\n","-","-","-","-","-","-","-","-","-","-","-","-","detect airflow direction via software\n","-","-","-","-","-","-","-","detect airflow direction via software\n"]
[null,"Default Airflow\n",{"$nulls":9},"-",{"$nulls":6},"-",null,null,null,"-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-",{"$nulls":4},"-","-","-","-","-","-","-","-",{"$nulls":6},"front-to-back power->port\n","-","-","-","-","-","-","-","-","-","-","-","-","front-to-back power->port\n","-","-","-","-","-","-","-","front-to-back power->port\n"]
[null,"Fan Speed adjustment\n",{"$nulls":9},"2 level adjustment\n",{"$nulls":6},"-",null,null,null,"2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","-","-","-","-","-","2 level adjustment\n","2 level adjustment\n","2 level adjustment\n","-","-","-","-","-",{"$nulls":4},"-","-","-","2 level adjustment\n","-","2 level adjustment\n","-","2 level adjustment\n",{"$nulls":6},"8 level adjustment\n","2 level","2 level","2 level","2 level","2 level","2 level","2 level","2 level","2 level","8 level adjustment\n","8 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n","10 level adjustment\n"]
[null,"Installation\n",{"$nulls":9},"rack mount\n",{"$nulls":6},"-",null,null,null,"rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","-","-","-","-","-",{"$nulls":4},"rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n",{"$nulls":6},"rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount\n","rack mount","rack mount\n","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount","rack mount\n"]
[null,"Noise(low speed/high speed)","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","No fan,no noise","43.2/50.0","37.6(low speed)\n44.7(high speed)","40.2(low speed)49.4(high speed)","42.2(low speed)51.5(high speed)","No fan,no noise","No fan,no noise","No fan,no noise",46.5,"37.6(low speed)\n44.7(high speed)","40.2(low speed)49.4(high speed)","42.2(low speed)51.5(high speed)","39.5/48.4","43.2/50.0","44.7/53.8","43.5/55.0",40.1,41.4,46.5,47.3,46.3,"42.8/49.9","43.2/50.0","44.7/53.8",40.1,46.5,47.3,46.3,51.3,41.7,47.8,41.6,48.8,"-","43.8dB(high speed)","44.4dB(high speed)","42.2dB(low speed)/50.0dB(high speed)","-","44.4dB(high speed)","39.4B/48.6B","44.4dB(high speed)","42.6(low speed)\n49.7(high speed)","41.3(low speed)\n50.1(high speed)","42.6(low speed)\n49.7(high speed)","41.3(low speed)\n50.1(high speed)","48.1(low speed)\n51.1(high speed)","49.5(low speed)\n54.1(high speed)","51.6/66.2","42.6(low speed)\n49.7(high speed)","41.3(low speed)\n50.1(high speed)","48.1(low speed)\n51.1(high speed)","49.5(low speed)\n54.1(high speed)","42.6/49.7","41.3/50.1","45.3/50.4","48.1/51.1","49.5/54.1","47.9，51.1","48.6，57.6","42.3dB/52.9dB","60.4dB、67.1dB","45.3dB/56.5dB","49.6dB/58.1dB","47.5dB/52.4dB","50.5dB/57.9dB","54dB/58.5dB","44.3dB/54.1dB","48.4dB/59.7dB","60.1dB、69.9db"]
[null,"MTBF","54.2(AC)","50.1(AC)","49.1(AC)",65,59.2,45.37,"54.2(AC)","50.1(AC)","49.1(AC)",67.38,"52.8(AC)","45.7(AC)","40.7(AC)","54.2/60.5(AC/DC)","50.1/55.4(AC/DC)","49.1/54.3(AC/DC)",51.8,52.8,45.7,40.7,82.99,67.38,37.94,28.97,57.1,84.5,51.8,29.5,26.9,82.68,67.36,37.94,45.91,42.4,29.5,26.9,51.9,32.2,30.3,31.4,26.9,77,77,73.6,54.5,70.8,50.5,58.4,48.6,"54.42","44.82","46.62","39.43","42.50","33.56",53.65,"20.1/23.0(XFP/CX4)","13.6/14.9(XFP/CX4)","19.8/21.9(XFP/CX4)","13.4/14.1(XFP/CX4)","25.91/22.27(CX4/XFP)","23.45/20.43(CX4/XFP)","28.54/24.29(CX4/XFP)",28.5,24.4,46.71,42.94,39.8,59.6,35.2,"46.99(without psu)\n35.27(AC)\n35.29(DC)",35.1,27.7,"40.8(without psu)\n33.09(AC)\n33.11(DC)","49.3(without psu)\n32.46(AC)\n32.47(DC)","36.7(without psu)\n29.20(AC)\n29.21(DC)",62.7]
[null,"MTTR",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,1,1,1,1,1,1,1,2,2,2,2,2,2,2,2,2,1,1,2,1,1,1,1,1,1,1,1,1]
[null,"RPS","-","-","-","-","-","-","-","-","-","-","-","RPS1000-A3","RPS1000-A3","-","-","-","-","-","-","RPS1000-A3","-","-","Y","Y","-","-","-","Y(RPS1000-A3)","Y(RPS1000-A3)","Y","Y","Y","Y（RPS800-A3/RPS1000-A3）","Y（RPS800-A / RPS1000-A3）","Y(RPS1000-A3)","Y(RPS1000-A3)","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","Y（RPS800-A /RPS1000-A3）","-","-","-","-","-","-","-","RPS 1000","Y（RP8500-A）","Y（RP8500-A）","Y（RP8500-A）","Y（RP8500-A）","Y（RPS1000-A3）","Y（RPS1000-A3）","-","Y（RPS800-A）","Y（RPS800-A）","Y（RPS1000-A3）","Y（RPS1000-A3）","Y(RPS800-A)","Y(RPS800-A)","Y（RPS1000-A3）\n","Y（RPS1000-A3）","Y（RPS1000-A3）","-","-","Y(RPS800-A)","-","Y(RPS800-A)","Y(RPS800-A)","rps 1000","rps 1000","-","-","-","-"]
[null,"Hot-Swap","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y","Y"]
[null,"Power Supply by POE","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,"Size (WxHxd)","230（W）*160（D）*43.6(H)","360（W）*160（D）*43.6(H)","440（W）*160（D）*43.6(H)","230×160×43.6","360×160×43.6","440×160×43.6","230（W）*160（D）*43.6(H)","360（W）*160（D）*43.6(H)","440（W）*160（D）*43.6(H)","440（W）*43.6(H)*260（D）","300（W）*220（D）*43.6(H)","440（W）*420（D）*43.6(H)","440（W）*420（D）*43.6(H)","230×160×43.6","360×160×43.6","440×160×43.6","440×43.6×260","300×220×43.6","300×260×43.6","440×420×43.6","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*420（D）","440（W）*43.6(H)*420（D）","440mm×43.6mm×260mm","440mm×43.6mm×260mm","440mm×43.6mm×260mm","440×43.6×420 mm","440×43.6×420 mm","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*260（D）","440（W）*43.6(H)*420（D）","440mm×43.6mm×260mm","440mm×43.6mm×260mm","440×43.6×420 mm","440×43.6×420 mm","440mm×43.6mm×260mm","440×43.6×260","440×43.6×260","440×43.6×260","440×43.6×260","210×43.6×210 （mm3）","440×43.6×160 （mm3）","440×43.6×160 （mm3）","440×43.6×260 （mm3）","300×260×43.6（mm3）","440×43.6×420 （mm3）","300×260×43.6（mm3）","440×43.6×420 （mm3）","440×300×43.6 mm","440×300×43.6 mm","440×300×43.6 mm","440×300×43.6 mm","440×420×43.6 mm","440×420×43.6 mm","440×420 ×43.6","440×43.6×300","440×43.6×420","440×43.6×300","440×43.6×420","440×300×43.6","440×300×43.6","440×360×43.7","440×420×43.6","440×420×43.6","440×360×43.6","440×420 ×43.6","440×367×43.6","440×660×43.6","440×367×43.6","441×426×43.6","440×427×43.6","440×427×43.6","440×465×86.1","440×467×86","440×427×43.6","440×660×43.6"]